From 6388f93fa432c2e6acc04d75b574b61c02d13ece Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dsteve@broadcom.com>
Date: Wed, 12 Feb 2014 11:39:20 +0000
Subject: [PATCH 170/196] V4L2: Correct BGR24 to RGB24 in format table

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>
---
 drivers/media/platform/bcm2835/bcm2835-camera.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/drivers/media/platform/bcm2835/bcm2835-camera.c b/drivers/media/platform/bcm2835/bcm2835-camera.c
index 6d0d77a..8285e6a 100644
--- a/drivers/media/platform/bcm2835/bcm2835-camera.c
+++ b/drivers/media/platform/bcm2835/bcm2835-camera.c
@@ -84,8 +84,8 @@ static struct mmal_fmt formats[] = {
 	 .mmal_component = MMAL_COMPONENT_CAMERA,
 	 },
 	{
-	 .name = "RGB24 (BE)",
-	 .fourcc = V4L2_PIX_FMT_BGR24,
+	 .name = "RGB24 (LE)",
+	 .fourcc = V4L2_PIX_FMT_RGB24,
 	 .flags = 0,
 	 .mmal = MMAL_ENCODING_BGR24,
 	 .depth = 24,
-- 
1.9.1

