From b36f694256f41bc71571f467646d015dda128d14 Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Sat, 9 Nov 2013 17:03:59 +0100
Subject: [PATCH 210/210] b44: register adm switch

---
 drivers/net/ethernet/broadcom/b44.c |   57 +++++++++++++++++++++++++++++++++++
 drivers/net/ethernet/broadcom/b44.h |    3 ++
 2 files changed, 60 insertions(+)

--- a/drivers/net/ethernet/broadcom/b44.c
+++ b/drivers/net/ethernet/broadcom/b44.c
@@ -31,6 +31,8 @@
 #include <linux/ssb/ssb.h>
 #include <linux/slab.h>
 #include <linux/phy.h>
+#include <linux/platform_device.h>
+#include <linux/platform_data/adm6996-gpio.h>
 
 #include <asm/uaccess.h>
 #include <asm/io.h>
@@ -2227,6 +2229,70 @@ static void b44_adjust_link(struct net_d
 	}
 }
 
+#ifdef CONFIG_BCM47XX
+static int b44_register_adm_switch(struct b44 *bp)
+{
+	int gpio;
+	struct platform_device *pdev;
+	struct adm6996_gpio_platform_data adm_data = {0};
+	struct platform_device_info info = {0};
+
+	adm_data.model = ADM6996L;
+	gpio = bcm47xx_nvram_gpio_pin("adm_eecs");
+	if (gpio >= 0)
+		adm_data.eecs = gpio;
+	else
+		adm_data.eecs = 2;
+
+	gpio = bcm47xx_nvram_gpio_pin("adm_eesk");
+	if (gpio >= 0)
+		adm_data.eesk = gpio;
+	else
+		adm_data.eesk = 3;
+
+	gpio = bcm47xx_nvram_gpio_pin("adm_eedi");
+	if (gpio >= 0)
+		adm_data.eedi = gpio;
+	else
+		adm_data.eedi = 4;
+
+	gpio = bcm47xx_nvram_gpio_pin("adm_rc");
+	if (gpio >= 0)
+		adm_data.eerc = gpio;
+	else
+		adm_data.eerc = 5;
+
+	info.parent = bp->sdev->dev;
+	info.name = "adm6996_gpio";
+	info.id = -1;
+	info.data = &adm_data;
+	info.size_data = sizeof(adm_data);
+
+	if (!bp->adm_switch) {
+		pdev = platform_device_register_full(&info);
+		if (IS_ERR(pdev))
+			return PTR_ERR(pdev);
+
+		bp->adm_switch = pdev;
+	}
+	return 0;
+}
+static void b44_unregister_adm_switch(struct b44 *bp)
+{
+	if (bp->adm_switch)
+		platform_device_unregister(bp->adm_switch);
+}
+#else
+static int b44_register_adm_switch(struct b44 *bp)
+{
+	return 0;
+}
+static void b44_unregister_adm_switch(struct b44 *bp)
+{
+
+}
+#endif /* CONFIG_BCM47XX */
+
 static int b44_register_phy_one(struct b44 *bp)
 {
 	struct mii_bus *mii_bus;
@@ -2270,6 +2336,9 @@ static int b44_register_phy_one(struct b
 	if (!bp->mii_bus->phy_map[bp->phy_addr] &&
 	    (sprom->boardflags_lo & (B44_BOARDFLAG_ROBO | B44_BOARDFLAG_ADM))) {
 
+		if (sprom->boardflags_lo & B44_BOARDFLAG_ADM)
+			b44_register_adm_switch(bp);
+
 		dev_info(sdev->dev,
 			 "could not find PHY at %i, use fixed one\n",
 			 bp->phy_addr);
@@ -2465,6 +2534,7 @@ static void b44_remove_one(struct ssb_de
 	unregister_netdev(dev);
 	if (bp->flags & B44_FLAG_EXTERNAL_PHY)
 		b44_unregister_phy_one(bp);
+	b44_unregister_adm_switch(bp);
 	ssb_device_disable(sdev, 0);
 	ssb_bus_may_powerdown(sdev->bus);
 	free_netdev(dev);
--- a/drivers/net/ethernet/broadcom/b44.h
+++ b/drivers/net/ethernet/broadcom/b44.h
@@ -404,6 +404,9 @@ struct b44 {
 	struct mii_bus		*mii_bus;
 	int			old_link;
 	struct mii_if_info	mii_if;
+
+	/* platform device for associated switch */
+	struct platform_device *adm_switch;
 };
 
 #endif /* _B44_H */
