From: Richard Zhu <r65037@freescale.com>
Subject: [PATCH] ARM: imx6q: update the sata bits definitions of gpr13

Replace the SATA_PHY_# by the more readable definitons.

tj: Being routed through libata branch to enable implementation of
    ahci_imx.

Signed-off-by: Richard Zhu <r65037@freescale.com>
Acked-by: Shawn Guo <shawn.guo@linaro.org>
Signed-off-by: Tejun Heo <tj@kernel.org>
---
 include/linux/mfd/syscon/imx6q-iomuxc-gpr.h | 121 +++++++++++++++++++---------
 1 file changed, 84 insertions(+), 37 deletions(-)

--- a/include/linux/mfd/syscon/imx6q-iomuxc-gpr.h
+++ b/include/linux/mfd/syscon/imx6q-iomuxc-gpr.h
@@ -279,41 +279,88 @@
 #define IMX6Q_GPR13_CAN2_STOP_REQ		BIT(29)
 #define IMX6Q_GPR13_CAN1_STOP_REQ		BIT(28)
 #define IMX6Q_GPR13_ENET_STOP_REQ		BIT(27)
-#define IMX6Q_GPR13_SATA_PHY_8_MASK		(0x7 << 24)
-#define IMX6Q_GPR13_SATA_PHY_8_0_5_DB		(0x0 << 24)
-#define IMX6Q_GPR13_SATA_PHY_8_1_0_DB		(0x1 << 24)
-#define IMX6Q_GPR13_SATA_PHY_8_1_5_DB		(0x2 << 24)
-#define IMX6Q_GPR13_SATA_PHY_8_2_0_DB		(0x3 << 24)
-#define IMX6Q_GPR13_SATA_PHY_8_2_5_DB		(0x4 << 24)
-#define IMX6Q_GPR13_SATA_PHY_8_3_0_DB		(0x5 << 24)
-#define IMX6Q_GPR13_SATA_PHY_8_3_5_DB		(0x6 << 24)
-#define IMX6Q_GPR13_SATA_PHY_8_4_0_DB		(0x7 << 24)
-#define IMX6Q_GPR13_SATA_PHY_7_MASK		(0x1f << 19)
-#define IMX6Q_GPR13_SATA_PHY_7_SATA1I		(0x10 << 19)
-#define IMX6Q_GPR13_SATA_PHY_7_SATA1M		(0x10 << 19)
-#define IMX6Q_GPR13_SATA_PHY_7_SATA1X		(0x1a << 19)
-#define IMX6Q_GPR13_SATA_PHY_7_SATA2I		(0x12 << 19)
-#define IMX6Q_GPR13_SATA_PHY_7_SATA2M		(0x12 << 19)
-#define IMX6Q_GPR13_SATA_PHY_7_SATA2X		(0x1a << 19)
-#define IMX6Q_GPR13_SATA_PHY_6_MASK		(0x7 << 16)
-#define IMX6Q_GPR13_SATA_SPEED_MASK		BIT(15)
-#define IMX6Q_GPR13_SATA_SPEED_1P5G		0x0
-#define IMX6Q_GPR13_SATA_SPEED_3P0G		BIT(15)
-#define IMX6Q_GPR13_SATA_PHY_5			BIT(14)
-#define IMX6Q_GPR13_SATA_PHY_4_MASK		(0x7 << 11)
-#define IMX6Q_GPR13_SATA_PHY_4_16_16		(0x0 << 11)
-#define IMX6Q_GPR13_SATA_PHY_4_14_16		(0x1 << 11)
-#define IMX6Q_GPR13_SATA_PHY_4_12_16		(0x2 << 11)
-#define IMX6Q_GPR13_SATA_PHY_4_10_16		(0x3 << 11)
-#define IMX6Q_GPR13_SATA_PHY_4_9_16		(0x4 << 11)
-#define IMX6Q_GPR13_SATA_PHY_4_8_16		(0x5 << 11)
-#define IMX6Q_GPR13_SATA_PHY_3_MASK		(0xf << 7)
-#define IMX6Q_GPR13_SATA_PHY_3_OFF		0x7
-#define IMX6Q_GPR13_SATA_PHY_2_MASK		(0x1f << 2)
-#define IMX6Q_GPR13_SATA_PHY_2_OFF		0x2
-#define IMX6Q_GPR13_SATA_PHY_1_MASK		(0x3 << 0)
-#define IMX6Q_GPR13_SATA_PHY_1_FAST		(0x0 << 0)
-#define IMX6Q_GPR13_SATA_PHY_1_MED		(0x1 << 0)
-#define IMX6Q_GPR13_SATA_PHY_1_SLOW		(0x2 << 0)
-
+#define IMX6Q_GPR13_SATA_RX_EQ_VAL_MASK		(0x7 << 24)
+#define IMX6Q_GPR13_SATA_RX_EQ_VAL_0_5_DB	(0x0 << 24)
+#define IMX6Q_GPR13_SATA_RX_EQ_VAL_1_0_DB	(0x1 << 24)
+#define IMX6Q_GPR13_SATA_RX_EQ_VAL_1_5_DB	(0x2 << 24)
+#define IMX6Q_GPR13_SATA_RX_EQ_VAL_2_0_DB	(0x3 << 24)
+#define IMX6Q_GPR13_SATA_RX_EQ_VAL_2_5_DB	(0x4 << 24)
+#define IMX6Q_GPR13_SATA_RX_EQ_VAL_3_0_DB	(0x5 << 24)
+#define IMX6Q_GPR13_SATA_RX_EQ_VAL_3_5_DB	(0x6 << 24)
+#define IMX6Q_GPR13_SATA_RX_EQ_VAL_4_0_DB	(0x7 << 24)
+#define IMX6Q_GPR13_SATA_RX_LOS_LVL_MASK	(0x1f << 19)
+#define IMX6Q_GPR13_SATA_RX_LOS_LVL_SATA1I	(0x10 << 19)
+#define IMX6Q_GPR13_SATA_RX_LOS_LVL_SATA1M	(0x10 << 19)
+#define IMX6Q_GPR13_SATA_RX_LOS_LVL_SATA1X	(0x1a << 19)
+#define IMX6Q_GPR13_SATA_RX_LOS_LVL_SATA2I	(0x12 << 19)
+#define IMX6Q_GPR13_SATA_RX_LOS_LVL_SATA2M	(0x12 << 19)
+#define IMX6Q_GPR13_SATA_RX_LOS_LVL_SATA2X	(0x1a << 19)
+#define IMX6Q_GPR13_SATA_RX_DPLL_MODE_MASK	(0x7 << 16)
+#define IMX6Q_GPR13_SATA_RX_DPLL_MODE_1P_1F	(0x0 << 16)
+#define IMX6Q_GPR13_SATA_RX_DPLL_MODE_2P_2F	(0x1 << 16)
+#define IMX6Q_GPR13_SATA_RX_DPLL_MODE_1P_4F	(0x2 << 16)
+#define IMX6Q_GPR13_SATA_RX_DPLL_MODE_2P_4F	(0x3 << 16)
+#define IMX6Q_GPR13_SATA_SPD_MODE_MASK		BIT(15)
+#define IMX6Q_GPR13_SATA_SPD_MODE_1P5G		0x0
+#define IMX6Q_GPR13_SATA_SPD_MODE_3P0G		BIT(15)
+#define IMX6Q_GPR13_SATA_MPLL_SS_EN		BIT(14)
+#define IMX6Q_GPR13_SATA_TX_ATTEN_MASK		(0x7 << 11)
+#define IMX6Q_GPR13_SATA_TX_ATTEN_16_16		(0x0 << 11)
+#define IMX6Q_GPR13_SATA_TX_ATTEN_14_16		(0x1 << 11)
+#define IMX6Q_GPR13_SATA_TX_ATTEN_12_16		(0x2 << 11)
+#define IMX6Q_GPR13_SATA_TX_ATTEN_10_16		(0x3 << 11)
+#define IMX6Q_GPR13_SATA_TX_ATTEN_9_16		(0x4 << 11)
+#define IMX6Q_GPR13_SATA_TX_ATTEN_8_16		(0x5 << 11)
+#define IMX6Q_GPR13_SATA_TX_BOOST_MASK		(0xf << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_0_00_DB	(0x0 << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_0_37_DB	(0x1 << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_0_74_DB	(0x2 << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_1_11_DB	(0x3 << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_1_48_DB	(0x4 << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_1_85_DB	(0x5 << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_2_22_DB	(0x6 << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_2_59_DB	(0x7 << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_2_96_DB	(0x8 << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_3_33_DB	(0x9 << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_3_70_DB	(0xa << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_4_07_DB	(0xb << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_4_44_DB	(0xc << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_4_81_DB	(0xd << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_5_28_DB	(0xe << 7)
+#define IMX6Q_GPR13_SATA_TX_BOOST_5_75_DB	(0xf << 7)
+#define IMX6Q_GPR13_SATA_TX_LVL_MASK		(0x1f << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_0_937_V		(0x00 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_0_947_V		(0x01 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_0_957_V		(0x02 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_0_966_V		(0x03 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_0_976_V		(0x04 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_0_986_V		(0x05 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_0_996_V		(0x06 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_005_V		(0x07 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_015_V		(0x08 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_025_V		(0x09 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_035_V		(0x0a << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_045_V		(0x0b << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_054_V		(0x0c << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_064_V		(0x0d << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_074_V		(0x0e << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_084_V		(0x0f << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_094_V		(0x10 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_104_V		(0x11 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_113_V		(0x12 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_123_V		(0x13 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_133_V		(0x14 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_143_V		(0x15 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_152_V		(0x16 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_162_V		(0x17 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_172_V		(0x18 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_182_V		(0x19 << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_191_V		(0x1a << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_201_V		(0x1b << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_211_V		(0x1c << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_221_V		(0x1d << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_230_V		(0x1e << 2)
+#define IMX6Q_GPR13_SATA_TX_LVL_1_240_V		(0x1f << 2)
+#define IMX6Q_GPR13_SATA_MPLL_CLK_EN		BIT(1)
+#define IMX6Q_GPR13_SATA_TX_EDGE_RATE		BIT(0)
 #endif /* __LINUX_IMX6Q_IOMUXC_GPR_H */
