From 07cddcb5820db42cadcc4627aad7391816b63b34 Mon Sep 17 00:00:00 2001
From: Thomas Langer <thomas.langer@lantiq.com>
Date: Fri, 9 Aug 2013 20:54:30 +0200
Subject: [PATCH 29/34] serial: MIPS: lantiq: add clk_enable() call to driver

Enable the clock if one is present when setting up the console.

Signed-off-by: Thomas Langer <thomas.langer@lantiq.com>
Acked-by: John Crispin <blogic@openwrt.org>
---
 drivers/tty/serial/lantiq.c |    3 +++
 1 file changed, 3 insertions(+)

--- a/drivers/tty/serial/lantiq.c
+++ b/drivers/tty/serial/lantiq.c
@@ -636,6 +636,9 @@ lqasc_console_setup(struct console *co,
 
 	port = &ltq_port->port;
 
+	if (!IS_ERR(ltq_port->clk))
+		clk_enable(ltq_port->clk);
+
 	port->uartclk = clk_get_rate(ltq_port->fpiclk);
 
 	if (options)
