From 158a11f25e070a6ed99cf8faa985da1f2669230f Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Sun, 21 Apr 2013 14:44:00 +0200
Subject: [PATCH 3/3] MIPS: BCM63XX: select BMIPS4350 and default to 2 CPUs
 for supported SoCs

All BCM63XX SoCs starting with BCM6358 have a BMIPS4350 instead of a
BMIPS3300, so select it unless support for any of the older SoCs is
selected.
All BMIPS4350 have only two CPUs, so select the appropriate default.

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/Kconfig |    2 ++
 1 file changed, 2 insertions(+)

--- a/arch/mips/Kconfig
+++ b/arch/mips/Kconfig
@@ -129,6 +129,8 @@ config BCM63XX
 	select DMA_NONCOHERENT
 	select IRQ_CPU
 	select SYS_HAS_CPU_MIPS32_R1
+	select SYS_HAS_CPU_BMIPS4350 if !BCM63XX_CPU_6338 && !BCM63XX_CPU_6345 && !BCM63XX_CPU_6348
+	select NR_CPUS_DEFAULT_2
 	select SYS_SUPPORTS_32BIT_KERNEL
 	select SYS_SUPPORTS_BIG_ENDIAN
 	select SYS_HAS_EARLY_PRINTK
