From 1b5fced71edb0a4e71012d79be29f1003c7b099f Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Wed, 13 Mar 2013 09:39:02 +0100
Subject: [PATCH 01/34] MIPS: lantiq: add pcie driver

---
 arch/mips/lantiq/Kconfig           |   10 +
 arch/mips/lantiq/xway/sysctrl.c    |    2 +
 arch/mips/pci/Makefile             |    2 +
 arch/mips/pci/fixup-lantiq-pcie.c  |   82 +++
 arch/mips/pci/fixup-lantiq.c       |    5 +-
 arch/mips/pci/ifxmips_pci_common.h |   57 ++
 arch/mips/pci/ifxmips_pcie.c       | 1099 ++++++++++++++++++++++++++++++
 arch/mips/pci/ifxmips_pcie.h       |  135 ++++
 arch/mips/pci/ifxmips_pcie_ar10.h  |  290 ++++++++
 arch/mips/pci/ifxmips_pcie_msi.c   |  392 +++++++++++
 arch/mips/pci/ifxmips_pcie_phy.c   |  478 +++++++++++++
 arch/mips/pci/ifxmips_pcie_pm.c    |  176 +++++
 arch/mips/pci/ifxmips_pcie_pm.h    |   36 +
 arch/mips/pci/ifxmips_pcie_reg.h   | 1001 +++++++++++++++++++++++++++
 arch/mips/pci/ifxmips_pcie_vr9.h   |  271 ++++++++
 arch/mips/pci/pci.c                |   25 +
 arch/mips/pci/pcie-lantiq.h        | 1305 ++++++++++++++++++++++++++++++++++++
 drivers/pci/pcie/aer/Kconfig       |    2 +-
 include/linux/pci.h                |    2 +
 include/linux/pci_ids.h            |    6 +
 20 files changed, 5374 insertions(+), 2 deletions(-)
 create mode 100644 arch/mips/pci/fixup-lantiq-pcie.c
 create mode 100644 arch/mips/pci/ifxmips_pci_common.h
 create mode 100644 arch/mips/pci/ifxmips_pcie.c
 create mode 100644 arch/mips/pci/ifxmips_pcie.h
 create mode 100644 arch/mips/pci/ifxmips_pcie_ar10.h
 create mode 100644 arch/mips/pci/ifxmips_pcie_msi.c
 create mode 100644 arch/mips/pci/ifxmips_pcie_phy.c
 create mode 100644 arch/mips/pci/ifxmips_pcie_pm.c
 create mode 100644 arch/mips/pci/ifxmips_pcie_pm.h
 create mode 100644 arch/mips/pci/ifxmips_pcie_reg.h
 create mode 100644 arch/mips/pci/ifxmips_pcie_vr9.h
 create mode 100644 arch/mips/pci/pcie-lantiq.h

--- a/arch/mips/lantiq/Kconfig
+++ b/arch/mips/lantiq/Kconfig
@@ -17,6 +17,7 @@ config SOC_XWAY
 	bool "XWAY"
 	select SOC_TYPE_XWAY
 	select HW_HAS_PCI
+	select ARCH_SUPPORTS_MSI
 
 config SOC_FALCON
 	bool "FALCON"
@@ -36,6 +37,15 @@ config PCI_LANTIQ
 	bool "PCI Support"
 	depends on SOC_XWAY && PCI
 
+config PCIE_LANTIQ
+	bool "PCIE Support"
+	depends on SOC_XWAY && PCI
+
+config PCIE_LANTIQ_MSI
+	bool
+	depends on PCIE_LANTIQ && PCI_MSI
+	default y
+
 config XRX200_PHY_FW
 	bool "XRX200 PHY firmware loader"
 	depends on SOC_XWAY
--- a/arch/mips/lantiq/xway/sysctrl.c
+++ b/arch/mips/lantiq/xway/sysctrl.c
@@ -377,6 +377,8 @@ void __init ltq_soc_init(void)
 				PMU_PPE_EMA | PMU_PPE_TC | PMU_PPE_SLL01 |
 				PMU_PPE_QSB | PMU_PPE_TOP);
 		clkdev_add_pmu("1f203000.rcu", "gphy", 0, PMU_GPHY);
+		pmu_w32(~0, PMU_PWDSR1);
+		pmu_w32(pmu_r32(PMU_PWDSR) & ~PMU_PCIE_CLK, PMU_PWDSR);
 	} else if (of_machine_is_compatible("lantiq,ar9")) {
 		clkdev_add_static(ltq_ar9_cpu_hz(), ltq_ar9_fpi_hz(),
 				ltq_ar9_fpi_hz(), CLOCK_250M);
--- a/arch/mips/pci/Makefile
+++ b/arch/mips/pci/Makefile
@@ -41,6 +41,8 @@ obj-$(CONFIG_SIBYTE_BCM1x80)	+= pci-bcm1
 obj-$(CONFIG_SNI_RM)		+= fixup-sni.o ops-sni.o
 obj-$(CONFIG_LANTIQ)		+= fixup-lantiq.o
 obj-$(CONFIG_PCI_LANTIQ)	+= pci-lantiq.o ops-lantiq.o
+obj-$(CONFIG_PCIE_LANTIQ)	+= ifxmips_pcie_phy.o ifxmips_pcie.o fixup-lantiq-pcie.o
+obj-$(CONFIG_PCIE_LANTIQ_MSI)	+= pcie-lantiq-msi.o
 obj-$(CONFIG_TANBAC_TB0219)	+= fixup-tb0219.o
 obj-$(CONFIG_TANBAC_TB0226)	+= fixup-tb0226.o
 obj-$(CONFIG_TANBAC_TB0287)	+= fixup-tb0287.o
--- /dev/null
+++ b/arch/mips/pci/fixup-lantiq-pcie.c
@@ -0,0 +1,82 @@
+/******************************************************************************
+**
+** FILE NAME    : ifxmips_fixup_pcie.c
+** PROJECT      : IFX UEIP for VRX200
+** MODULES      : PCIe 
+**
+** DATE         : 02 Mar 2009
+** AUTHOR       : Lei Chuanhua
+** DESCRIPTION  : PCIe Root Complex Driver
+** COPYRIGHT    :       Copyright (c) 2009
+**                      Infineon Technologies AG
+**                      Am Campeon 1-12, 85579 Neubiberg, Germany
+**
+**    This program is free software; you can redistribute it and/or modify
+**    it under the terms of the GNU General Public License as published by
+**    the Free Software Foundation; either version 2 of the License, or
+**    (at your option) any later version.
+** HISTORY
+** $Version $Date        $Author         $Comment
+** 0.0.1    17 Mar,2009  Lei Chuanhua    Initial version
+*******************************************************************************/
+/*!
+ \file ifxmips_fixup_pcie.c
+ \ingroup IFX_PCIE  
+ \brief PCIe Fixup functions source file
+*/
+#include <linux/pci.h>
+#include <linux/pci_regs.h>
+#include <linux/pci_ids.h>
+
+#include <lantiq_soc.h>
+
+#include "pcie-lantiq.h"
+
+#define PCI_VENDOR_ID_INFINEON         0x15D1
+#define PCI_DEVICE_ID_INFINEON_DANUBE  0x000F
+#define PCI_DEVICE_ID_INFINEON_PCIE    0x0011
+#define PCI_VENDOR_ID_LANTIQ        0x1BEF
+#define PCI_DEVICE_ID_LANTIQ_PCIE       0x0011
+
+
+
+static void
+ifx_pcie_fixup_resource(struct pci_dev *dev)
+{
+    u32 reg;
+
+    IFX_PCIE_PRINT(PCIE_MSG_FIXUP, "%s dev %s: enter\n", __func__, pci_name(dev));
+
+    printk("%s: fixup host controller %s (%04x:%04x)\n", 
+        __func__, pci_name(dev), dev->vendor, dev->device); 
+
+   /* Setup COMMAND register */
+    reg = PCI_COMMAND_IO | PCI_COMMAND_MEMORY | PCI_COMMAND_MASTER /* | 
+          PCI_COMMAND_INTX_DISABLE */| PCI_COMMAND_SERR;
+    pci_write_config_word(dev, PCI_COMMAND, reg);
+    IFX_PCIE_PRINT(PCIE_MSG_FIXUP, "%s dev %s: exit\n", __func__, pci_name(dev));
+}
+DECLARE_PCI_FIXUP_EARLY(PCI_VENDOR_ID_INFINEON, PCI_DEVICE_ID_INFINEON_PCIE, ifx_pcie_fixup_resource);
+DECLARE_PCI_FIXUP_EARLY(PCI_VENDOR_ID_LANTIQ, PCI_VENDOR_ID_LANTIQ, ifx_pcie_fixup_resource);
+
+static void
+ifx_pcie_rc_class_early_fixup(struct pci_dev *dev)
+{
+    IFX_PCIE_PRINT(PCIE_MSG_FIXUP, "%s dev %s: enter\n", __func__, pci_name(dev));
+
+    if (dev->devfn == PCI_DEVFN(0, 0) &&
+        (dev->class >> 8) == PCI_CLASS_BRIDGE_HOST) {
+
+        dev->class = (PCI_CLASS_BRIDGE_PCI << 8) | (dev->class & 0xff);
+
+        printk(KERN_INFO "%s: fixed pcie host bridge to pci-pci bridge\n", __func__);
+    }
+    IFX_PCIE_PRINT(PCIE_MSG_FIXUP, "%s dev %s: exit\n", __func__, pci_name(dev));
+    mdelay(10);
+}
+
+DECLARE_PCI_FIXUP_EARLY(PCI_VENDOR_ID_INFINEON, PCI_DEVICE_ID_INFINEON_PCIE,
+     ifx_pcie_rc_class_early_fixup);
+
+DECLARE_PCI_FIXUP_EARLY(PCI_VENDOR_ID_LANTIQ, PCI_DEVICE_ID_LANTIQ_PCIE,
+     ifx_pcie_rc_class_early_fixup);
--- a/arch/mips/pci/fixup-lantiq.c
+++ b/arch/mips/pci/fixup-lantiq.c
@@ -11,11 +11,12 @@
 
 int (*ltq_pci_plat_arch_init)(struct pci_dev *dev) = NULL;
 int (*ltq_pci_plat_dev_init)(struct pci_dev *dev) = NULL;
+int (*ltq_pci_map_irq)(const struct pci_dev *dev, u8 slot, u8 pin);
 
 int pcibios_plat_dev_init(struct pci_dev *dev)
 {
 	if (ltq_pci_plat_arch_init)
-		return ltq_pci_plat_arch_init(dev);
+		ltq_pci_plat_arch_init(dev);
 
 	if (ltq_pci_plat_dev_init)
 		return ltq_pci_plat_dev_init(dev);
@@ -28,6 +29,8 @@ int __init pcibios_map_irq(const struct
 	struct of_irq dev_irq;
 	int irq;
 
+	if (ltq_pci_map_irq)
+		return ltq_pci_map_irq(dev, slot, pin);
 	if (of_irq_map_pci(dev, &dev_irq)) {
 		dev_err(&dev->dev, "trying to map irq for unknown slot:%d pin:%d\n",
 			slot, pin);
--- /dev/null
+++ b/arch/mips/pci/ifxmips_pci_common.h
@@ -0,0 +1,57 @@
+/******************************************************************************
+**
+** FILE NAME    : ifxmips_pci_common.h
+** PROJECT      : IFX UEIP
+** MODULES      : PCI subsystem
+**
+** DATE         : 30 June 2009
+** AUTHOR       : Lei Chuanhua
+** DESCRIPTION  : PCIe Root Complex Driver
+** COPYRIGHT    :       Copyright (c) 2009
+**                      Infineon Technologies AG
+**                      Am Campeon 1-12, 85579 Neubiberg, Germany
+**
+**    This program is free software; you can redistribute it and/or modify
+**    it under the terms of the GNU General Public License as published by
+**    the Free Software Foundation; either version 2 of the License, or
+**    (at your option) any later version.
+** HISTORY
+** $Version $Date        $Author         $Comment
+** 0.0.1    30 June,2009  Lei Chuanhua    Initial version
+*******************************************************************************/
+
+#ifndef IFXMIPS_PCI_COMMON_H
+#define IFXMIPS_PCI_COMMON_H
+#include <linux/version.h>
+/*!
+ \defgroup IFX_PCI_COM  IFX PCI/PCIe common parts for OS integration  
+ \brief  PCI/PCIe common parts
+*/
+
+/*!
+ \defgroup IFX_PCI_COM_OS OS APIs
+ \ingroup IFX_PCI_COM
+ \brief PCI/PCIe bus driver OS interface functions
+*/
+/*!
+  \file ifxmips_pci_common.h
+  \ingroup IFX_PCI_COM
+  \brief PCI/PCIe bus driver common OS header file
+*/
+#if LINUX_VERSION_CODE < KERNEL_VERSION(2,6,24)
+#define IFX_PCI_CONST
+#else
+#define IFX_PCI_CONST const
+#endif
+#ifdef CONFIG_IFX_PCI
+extern int ifx_pci_bios_map_irq(IFX_PCI_CONST struct pci_dev *dev, u8 slot, u8 pin);
+extern int ifx_pci_bios_plat_dev_init(struct pci_dev *dev);
+#endif /* COFNIG_IFX_PCI */
+
+#ifdef CONFIG_IFX_PCIE
+extern int ifx_pcie_bios_map_irq(IFX_PCI_CONST struct pci_dev *dev, u8 slot, u8 pin);
+extern int ifx_pcie_bios_plat_dev_init(struct pci_dev *dev);
+#endif
+
+#endif /* IFXMIPS_PCI_COMMON_H */
+
--- /dev/null
+++ b/arch/mips/pci/ifxmips_pcie.c
@@ -0,0 +1,1099 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2009 Lei Chuanhua <chuanhua.lei@infineon.com>
+ *  Copyright (C) 2013 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/types.h>
+#include <linux/pci.h>
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/delay.h>
+#include <linux/mm.h>
+#include <asm/paccess.h>
+#include <linux/pci.h>
+#include <linux/pci_regs.h>
+#include <linux/module.h>
+
+#include "ifxmips_pcie.h"
+#include "ifxmips_pcie_reg.h"
+
+/* Enable 32bit io due to its mem mapped io nature */
+#define IFX_PCIE_ERROR_INT
+#define IFX_PCIE_IO_32BIT
+
+#define IFX_PCIE_IR                     (INT_NUM_IM4_IRL0 + 25)
+#define IFX_PCIE_INTA                   (INT_NUM_IM4_IRL0 + 8)
+#define IFX_PCIE_INTB                   (INT_NUM_IM4_IRL0 + 9)
+#define IFX_PCIE_INTC                   (INT_NUM_IM4_IRL0 + 10)
+#define IFX_PCIE_INTD                   (INT_NUM_IM4_IRL0 + 11)
+#define MS(_v, _f)  (((_v) & (_f)) >> _f##_S)
+#define SM(_v, _f)  (((_v) << _f##_S) & (_f))
+#define IFX_REG_SET_BIT(_f, _r) \
+	IFX_REG_W32((IFX_REG_R32((_r)) &~ (_f)) | (_f), (_r))
+
+#define IFX_PCIE_LTSSM_ENABLE_TIMEOUT 10
+
+static DEFINE_SPINLOCK(ifx_pcie_lock);
+
+u32 g_pcie_debug_flag = PCIE_MSG_ANY & (~PCIE_MSG_CFG);
+
+static ifx_pcie_irq_t pcie_irqs[IFX_PCIE_CORE_NR] = {
+    {
+        .ir_irq = {
+            .irq  = IFX_PCIE_IR,
+            .name = "ifx_pcie_rc0",
+        },
+
+        .legacy_irq = {
+            {
+                .irq_bit = PCIE_IRN_INTA,
+                .irq     = IFX_PCIE_INTA,
+            },
+            {
+                .irq_bit = PCIE_IRN_INTB,
+                .irq     = IFX_PCIE_INTB,
+            },
+            {
+                .irq_bit = PCIE_IRN_INTC,
+                .irq     = IFX_PCIE_INTC,
+            },
+            {
+                .irq_bit = PCIE_IRN_INTD,
+                .irq     = IFX_PCIE_INTD,
+            },
+        },
+    },
+
+};
+
+void ifx_pcie_debug(const char *fmt, ...)
+{
+	static char buf[256] = {0};      /* XXX */
+	va_list ap;
+
+	va_start(ap, fmt);
+	vsnprintf(buf, sizeof(buf), fmt, ap);
+	va_end(ap);
+
+	printk("%s", buf);
+}
+
+
+static inline int pcie_ltssm_enable(int pcie_port)
+{
+	int i;
+
+	/* Enable LTSSM */
+	IFX_REG_W32(PCIE_RC_CCR_LTSSM_ENABLE, PCIE_RC_CCR(pcie_port));
+
+	/* Wait for the link to come up */
+	for (i = 0; i < IFX_PCIE_LTSSM_ENABLE_TIMEOUT; i++) {
+		if (!(IFX_REG_R32(PCIE_LCTLSTS(pcie_port)) & PCIE_LCTLSTS_RETRAIN_PENDING))
+			return 0;
+		udelay(10);
+	}
+
+	printk("%s link timeout!!!!!\n", __func__);
+	return -1;
+}
+
+static inline void pcie_status_register_clear(int pcie_port)
+{
+	IFX_REG_W32(0, PCIE_RC_DR(pcie_port));
+	IFX_REG_W32(0, PCIE_PCICMDSTS(pcie_port));
+	IFX_REG_W32(0, PCIE_DCTLSTS(pcie_port));
+	IFX_REG_W32(0, PCIE_LCTLSTS(pcie_port));
+	IFX_REG_W32(0, PCIE_SLCTLSTS(pcie_port));
+	IFX_REG_W32(0, PCIE_RSTS(pcie_port));
+	IFX_REG_W32(0, PCIE_UES_R(pcie_port));
+	IFX_REG_W32(0, PCIE_UEMR(pcie_port));
+	IFX_REG_W32(0, PCIE_UESR(pcie_port));
+	IFX_REG_W32(0, PCIE_CESR(pcie_port));
+	IFX_REG_W32(0, PCIE_CEMR(pcie_port));
+	IFX_REG_W32(0, PCIE_RESR(pcie_port));
+	IFX_REG_W32(0, PCIE_PVCCRSR(pcie_port));
+	IFX_REG_W32(0, PCIE_VC0_RSR0(pcie_port));
+	IFX_REG_W32(0, PCIE_TPFCS(pcie_port));
+	IFX_REG_W32(0, PCIE_TNPFCS(pcie_port));
+	IFX_REG_W32(0, PCIE_TCFCS(pcie_port));
+	IFX_REG_W32(0, PCIE_QSR(pcie_port));
+	IFX_REG_W32(0, PCIE_IOBLSECS(pcie_port));
+}
+
+static inline int ifx_pcie_link_up(int pcie_port)
+{
+    return (IFX_REG_R32(PCIE_PHY_SR(pcie_port)) & PCIE_PHY_SR_PHY_LINK_UP) ? 1 : 0;
+}
+
+
+static inline void pcie_mem_io_setup(int pcie_port)
+{
+    u32 reg;
+    /*
+     * BAR[0:1] readonly register 
+     * RC contains only minimal BARs for packets mapped to this device 
+     * Mem/IO filters defines a range of memory occupied by memory mapped IO devices that
+     * reside on the downstream side fo the bridge.
+     */
+    reg = SM((PCIE_MEM_PHY_PORT_TO_END(pcie_port) >> 20), PCIE_MBML_MEM_LIMIT_ADDR)
+        | SM((PCIE_MEM_PHY_PORT_TO_BASE(pcie_port) >> 20), PCIE_MBML_MEM_BASE_ADDR);
+
+    IFX_REG_W32(reg, PCIE_MBML(pcie_port));
+
+
+#ifdef IFX_PCIE_PREFETCH_MEM_64BIT
+    reg = SM((PCIE_MEM_PHY_PORT_TO_END(pcie_port) >> 20), PCIE_PMBL_END_ADDR)
+        | SM((PCIE_MEM_PHY_PORT_TO_BASE(pcie_port) >> 20), PCIE_PMBL_UPPER_12BIT)
+        | PCIE_PMBL_64BIT_ADDR;
+    IFX_REG_W32(reg, PCIE_PMBL(pcie_port));
+
+    /* Must configure upper 32bit */
+    IFX_REG_W32(0, PCIE_PMBU32(pcie_port));
+    IFX_REG_W32(0, PCIE_PMLU32(pcie_port));
+#else
+    /* PCIe_PBML, same as MBML */
+    IFX_REG_W32(IFX_REG_R32(PCIE_MBML(pcie_port)), PCIE_PMBL(pcie_port));
+#endif 
+
+    /* IO Address Range */
+    reg = SM((PCIE_IO_PHY_PORT_TO_END(pcie_port) >> 12), PCIE_IOBLSECS_IO_LIMIT_ADDR)
+        | SM((PCIE_IO_PHY_PORT_TO_BASE(pcie_port) >> 12), PCIE_IOBLSECS_IO_BASE_ADDR);
+#ifdef IFX_PCIE_IO_32BIT    
+    reg |= PCIE_IOBLSECS_32BIT_IO_ADDR;
+#endif /* IFX_PCIE_IO_32BIT */
+    IFX_REG_W32(reg, PCIE_IOBLSECS(pcie_port));
+
+#ifdef IFX_PCIE_IO_32BIT
+    reg = SM((PCIE_IO_PHY_PORT_TO_END(pcie_port) >> 16), PCIE_IO_BANDL_UPPER_16BIT_IO_LIMIT)
+        | SM((PCIE_IO_PHY_PORT_TO_BASE(pcie_port) >> 16), PCIE_IO_BANDL_UPPER_16BIT_IO_BASE);
+    IFX_REG_W32(reg, PCIE_IO_BANDL(pcie_port));
+
+#endif /* IFX_PCIE_IO_32BIT */
+}
+
+static inline void
+pcie_device_setup(int pcie_port)
+{
+    u32 reg;
+
+    /* Device capability register, set up Maximum payload size */
+    reg = IFX_REG_R32(PCIE_DCAP(pcie_port));
+    reg |= PCIE_DCAP_ROLE_BASE_ERR_REPORT;
+    reg |= SM(PCIE_MAX_PAYLOAD_128, PCIE_DCAP_MAX_PAYLOAD_SIZE);
+
+    /* Only available for EP */
+    reg &= ~(PCIE_DCAP_EP_L0S_LATENCY | PCIE_DCAP_EP_L1_LATENCY);
+    IFX_REG_W32(reg, PCIE_DCAP(pcie_port));
+
+    /* Device control and status register */
+    /* Set Maximum Read Request size for the device as a Requestor */
+    reg = IFX_REG_R32(PCIE_DCTLSTS(pcie_port));
+
+    /* 
+     * Request size can be larger than the MPS used, but the completions returned 
+     * for the read will be bounded by the MPS size.
+     * In our system, Max request size depends on AHB burst size. It is 64 bytes.
+     * but we set it as 128 as minimum one.
+     */
+    reg |= SM(PCIE_MAX_PAYLOAD_128, PCIE_DCTLSTS_MAX_READ_SIZE)
+            | SM(PCIE_MAX_PAYLOAD_128, PCIE_DCTLSTS_MAX_PAYLOAD_SIZE);
+
+    /* Enable relaxed ordering, no snoop, and all kinds of errors */
+    reg |= PCIE_DCTLSTS_RELAXED_ORDERING_EN | PCIE_DCTLSTS_ERR_EN | PCIE_DCTLSTS_NO_SNOOP_EN;
+
+    IFX_REG_W32(reg, PCIE_DCTLSTS(pcie_port));
+}
+
+static inline void
+pcie_link_setup(int pcie_port)
+{
+    u32 reg;
+
+    /*
+     * XXX, Link capability register, bit 18 for EP CLKREQ# dynamic clock management for L1, L2/3 CPM 
+     * L0s is reported during link training via TS1 order set by N_FTS
+     */
+    reg = IFX_REG_R32(PCIE_LCAP(pcie_port));
+    reg &= ~PCIE_LCAP_L0S_EIXT_LATENCY;
+    reg |= SM(3, PCIE_LCAP_L0S_EIXT_LATENCY);
+    IFX_REG_W32(reg, PCIE_LCAP(pcie_port));
+
+    /* Link control and status register */
+    reg = IFX_REG_R32(PCIE_LCTLSTS(pcie_port));
+
+    /* Link Enable, ASPM enabled  */
+    reg &= ~PCIE_LCTLSTS_LINK_DISABLE;
+
+#ifdef CONFIG_PCIEASPM
+    /*  
+     * We use the same physical reference clock that the platform provides on the connector 
+     * It paved the way for ASPM to calculate the new exit Latency
+     */
+    reg |= PCIE_LCTLSTS_SLOT_CLK_CFG;
+    reg |= PCIE_LCTLSTS_COM_CLK_CFG;
+    /*
+     * We should disable ASPM by default except that we have dedicated power management support
+     * Enable ASPM will cause the system hangup/instability, performance degration
+     */
+    reg |= PCIE_LCTLSTS_ASPM_ENABLE;
+#else
+    reg &= ~PCIE_LCTLSTS_ASPM_ENABLE;
+#endif /* CONFIG_PCIEASPM */
+
+    /* 
+     * The maximum size of any completion with data packet is bounded by the MPS setting 
+     * in  device control register 
+     */
+
+    /* RCB may cause multiple split transactions, two options available, we use 64 byte RCB */
+    reg &= ~ PCIE_LCTLSTS_RCB128;
+
+    IFX_REG_W32(reg, PCIE_LCTLSTS(pcie_port));
+}
+
+static inline void pcie_error_setup(int pcie_port)
+{
+	u32 reg;
+
+	/* 
+	* Forward ERR_COR, ERR_NONFATAL, ERR_FATAL to the backbone 
+	* Poisoned write TLPs and completions indicating poisoned TLPs will set the PCIe_PCICMDSTS.MDPE 
+	*/
+	reg = IFX_REG_R32(PCIE_INTRBCTRL(pcie_port));
+	reg |= PCIE_INTRBCTRL_SERR_ENABLE | PCIE_INTRBCTRL_PARITY_ERR_RESP_ENABLE;
+
+	IFX_REG_W32(reg, PCIE_INTRBCTRL(pcie_port));
+
+	/* Uncorrectable Error Mask Register, Unmask <enable> all bits in PCIE_UESR */
+	reg = IFX_REG_R32(PCIE_UEMR(pcie_port));
+	reg &= ~PCIE_ALL_UNCORRECTABLE_ERR;
+	IFX_REG_W32(reg, PCIE_UEMR(pcie_port));
+
+	/* Uncorrectable Error Severity Register, ALL errors are FATAL */
+	IFX_REG_W32(PCIE_ALL_UNCORRECTABLE_ERR, PCIE_UESR(pcie_port));
+
+	/* Correctable Error Mask Register, unmask <enable> all bits */
+	reg = IFX_REG_R32(PCIE_CEMR(pcie_port));
+	reg &= ~PCIE_CORRECTABLE_ERR;
+	IFX_REG_W32(reg, PCIE_CEMR(pcie_port));
+
+	/* Advanced Error Capabilities and Control Registr */
+	reg = IFX_REG_R32(PCIE_AECCR(pcie_port));
+	reg |= PCIE_AECCR_ECRC_CHECK_EN | PCIE_AECCR_ECRC_GEN_EN;
+	IFX_REG_W32(reg, PCIE_AECCR(pcie_port));
+
+	/* Root Error Command Register, Report all types of errors */
+	reg = IFX_REG_R32(PCIE_RECR(pcie_port));
+	reg |= PCIE_RECR_ERR_REPORT_EN;
+	IFX_REG_W32(reg, PCIE_RECR(pcie_port));
+
+	/* Clear the Root status register */
+	reg = IFX_REG_R32(PCIE_RESR(pcie_port));
+	IFX_REG_W32(reg, PCIE_RESR(pcie_port));
+}
+
+static inline void pcie_port_logic_setup(int pcie_port)
+{
+	u32 reg;
+
+	/* FTS number, default 12, increase to 63, may increase time from/to L0s to L0  */
+	reg = IFX_REG_R32(PCIE_AFR(pcie_port));
+	reg &= ~(PCIE_AFR_FTS_NUM | PCIE_AFR_COM_FTS_NUM);
+	reg |= SM(PCIE_AFR_FTS_NUM_DEFAULT, PCIE_AFR_FTS_NUM)
+		| SM(PCIE_AFR_FTS_NUM_DEFAULT, PCIE_AFR_COM_FTS_NUM);
+	/* L0s and L1 entry latency */
+	reg &= ~(PCIE_AFR_L0S_ENTRY_LATENCY | PCIE_AFR_L1_ENTRY_LATENCY);
+	reg |= SM(PCIE_AFR_L0S_ENTRY_LATENCY_DEFAULT, PCIE_AFR_L0S_ENTRY_LATENCY)
+		| SM(PCIE_AFR_L1_ENTRY_LATENCY_DEFAULT, PCIE_AFR_L1_ENTRY_LATENCY);
+	IFX_REG_W32(reg, PCIE_AFR(pcie_port));
+
+
+	/* Port Link Control Register */
+	reg = IFX_REG_R32(PCIE_PLCR(pcie_port));
+	reg |= PCIE_PLCR_DLL_LINK_EN;  /* Enable the DLL link */
+	IFX_REG_W32(reg, PCIE_PLCR(pcie_port));
+
+	/* Lane Skew Register */
+	reg = IFX_REG_R32(PCIE_LSR(pcie_port));
+	/* Enable ACK/NACK and FC */
+	reg &= ~(PCIE_LSR_ACKNAK_DISABLE | PCIE_LSR_FC_DISABLE);
+	IFX_REG_W32(reg, PCIE_LSR(pcie_port));
+
+	/* Symbol Timer Register and Filter Mask Register 1 */
+	reg = IFX_REG_R32(PCIE_STRFMR(pcie_port));
+
+	/* Default SKP interval is very accurate already, 5us */
+	/* Enable IO/CFG transaction */
+	reg |= PCIE_STRFMR_RX_CFG_TRANS_ENABLE | PCIE_STRFMR_RX_IO_TRANS_ENABLE;
+	/* Disable FC WDT */
+	reg &= ~PCIE_STRFMR_FC_WDT_DISABLE;
+	IFX_REG_W32(reg, PCIE_STRFMR(pcie_port));
+
+	/* Filter Masker Register 2 */
+	reg = IFX_REG_R32(PCIE_FMR2(pcie_port));
+	reg |= PCIE_FMR2_VENDOR_MSG1_PASSED_TO_TRGT1 | PCIE_FMR2_VENDOR_MSG0_PASSED_TO_TRGT1;
+	IFX_REG_W32(reg, PCIE_FMR2(pcie_port));
+
+	/* VC0 Completion Receive Queue Control Register */
+	reg = IFX_REG_R32(PCIE_VC0_CRQCR(pcie_port));
+	reg &= ~PCIE_VC0_CRQCR_CPL_TLP_QUEUE_MODE;
+	reg |= SM(PCIE_VC0_TLP_QUEUE_MODE_BYPASS, PCIE_VC0_CRQCR_CPL_TLP_QUEUE_MODE);
+	IFX_REG_W32(reg, PCIE_VC0_CRQCR(pcie_port));
+}
+
+static inline void pcie_rc_cfg_reg_setup(int pcie_port)
+{
+	u32 reg;
+
+	/* Disable LTSSM */
+	IFX_REG_W32(0, PCIE_RC_CCR(pcie_port)); /* Disable LTSSM */
+
+	pcie_mem_io_setup(pcie_port);
+
+	/* XXX, MSI stuff should only apply to EP */
+	/* MSI Capability: Only enable 32-bit addresses */
+	reg = IFX_REG_R32(PCIE_MCAPR(pcie_port));
+	reg &= ~PCIE_MCAPR_ADDR64_CAP;
+
+	reg |= PCIE_MCAPR_MSI_ENABLE;
+
+	/* Disable multiple message */
+	reg &= ~(PCIE_MCAPR_MULTI_MSG_CAP | PCIE_MCAPR_MULTI_MSG_ENABLE);
+	IFX_REG_W32(reg, PCIE_MCAPR(pcie_port));
+
+
+	/* Enable PME, Soft reset enabled */
+	reg = IFX_REG_R32(PCIE_PM_CSR(pcie_port));
+	reg |= PCIE_PM_CSR_PME_ENABLE | PCIE_PM_CSR_SW_RST;
+	IFX_REG_W32(reg, PCIE_PM_CSR(pcie_port));
+
+	/* setup the bus */
+	reg = SM(0, PCIE_BNR_PRIMARY_BUS_NUM) | SM(1, PCIE_PNR_SECONDARY_BUS_NUM) | SM(0xFF, PCIE_PNR_SUB_BUS_NUM);
+	IFX_REG_W32(reg, PCIE_BNR(pcie_port));
+
+
+	pcie_device_setup(pcie_port);
+	pcie_link_setup(pcie_port);
+	pcie_error_setup(pcie_port);
+
+	/* Root control and capabilities register */
+	reg = IFX_REG_R32(PCIE_RCTLCAP(pcie_port));
+	reg |= PCIE_RCTLCAP_SERR_ENABLE | PCIE_RCTLCAP_PME_INT_EN;
+	IFX_REG_W32(reg, PCIE_RCTLCAP(pcie_port));
+
+	/* Port VC Capability Register 2 */
+	reg = IFX_REG_R32(PCIE_PVC2(pcie_port));
+	reg &= ~PCIE_PVC2_VC_ARB_WRR;
+	reg |= PCIE_PVC2_VC_ARB_16P_FIXED_WRR;
+	IFX_REG_W32(reg, PCIE_PVC2(pcie_port));
+
+	/* VC0 Resource Capability Register */
+	reg = IFX_REG_R32(PCIE_VC0_RC(pcie_port));
+	reg &= ~PCIE_VC0_RC_REJECT_SNOOP;
+	IFX_REG_W32(reg, PCIE_VC0_RC(pcie_port));
+
+	pcie_port_logic_setup(pcie_port);
+}
+
+static int ifx_pcie_wait_phy_link_up(int pcie_port)
+{
+#define IFX_PCIE_PHY_LINK_UP_TIMEOUT  1000 /* XXX, tunable */
+    int i;
+
+    /* Wait for PHY link is up */
+    for (i = 0; i < IFX_PCIE_PHY_LINK_UP_TIMEOUT; i++) {
+        if (ifx_pcie_link_up(pcie_port)) {
+            break;
+        }
+        udelay(100);
+    }
+    if (i >= IFX_PCIE_PHY_LINK_UP_TIMEOUT) {
+        printk(KERN_ERR "%s timeout\n", __func__);
+        return -1;
+    }
+
+    /* Check data link up or not */
+    if (!(IFX_REG_R32(PCIE_RC_DR(pcie_port)) & PCIE_RC_DR_DLL_UP)) {
+        printk(KERN_ERR "%s DLL link is still down\n", __func__);
+        return -1;
+    }
+
+    /* Check Data link active or not */
+    if (!(IFX_REG_R32(PCIE_LCTLSTS(pcie_port)) & PCIE_LCTLSTS_DLL_ACTIVE)) {
+        printk(KERN_ERR "%s DLL is not active\n", __func__);
+        return -1;
+    }
+    return 0;
+}
+
+static inline int pcie_app_loigc_setup(int pcie_port)
+{
+	/* supress ahb bus errrors */
+	IFX_REG_W32(PCIE_AHB_CTRL_BUS_ERROR_SUPPRESS, PCIE_AHB_CTRL(pcie_port));
+
+	/* Pull PCIe EP out of reset */
+	pcie_device_rst_deassert(pcie_port);
+
+	/* Start LTSSM training between RC and EP */
+	pcie_ltssm_enable(pcie_port);
+
+	/* Check PHY status after enabling LTSSM */
+	if (ifx_pcie_wait_phy_link_up(pcie_port) != 0)
+		return -1;
+
+	return 0;
+}
+
+/*
+ * The numbers below are directly from the PCIe spec table 3-4/5. 
+ */
+static inline void pcie_replay_time_update(int pcie_port)
+{
+	u32 reg;
+	int nlw;
+	int rtl;
+
+	reg = IFX_REG_R32(PCIE_LCTLSTS(pcie_port));
+
+	nlw = MS(reg, PCIE_LCTLSTS_NEGOTIATED_LINK_WIDTH);
+	switch (nlw) {
+	case PCIE_MAX_LENGTH_WIDTH_X1:
+		rtl = 1677;
+		break;
+	case PCIE_MAX_LENGTH_WIDTH_X2:
+		rtl = 867;
+		break;
+	case PCIE_MAX_LENGTH_WIDTH_X4:
+		rtl = 462;
+		break;
+	case PCIE_MAX_LENGTH_WIDTH_X8:
+		rtl = 258;
+		break;
+	default:
+		rtl = 1677;
+		break;
+	}
+	reg = IFX_REG_R32(PCIE_ALTRT(pcie_port));
+	reg &= ~PCIE_ALTRT_REPLAY_TIME_LIMIT;
+	reg |= SM(rtl, PCIE_ALTRT_REPLAY_TIME_LIMIT);
+	IFX_REG_W32(reg, PCIE_ALTRT(pcie_port));
+}
+
+/*
+ * Table 359 Enhanced Configuration Address Mapping1)
+ * 1) This table is defined in Table 7-1, page 341, PCI Express Base Specification v1.1
+ * Memory Address PCI Express Configuration Space
+ * A[(20+n-1):20] Bus Number 1 < n < 8
+ * A[19:15] Device Number
+ * A[14:12] Function Number
+ * A[11:8] Extended Register Number
+ * A[7:2] Register Number
+ * A[1:0] Along with size of the access, used to generate Byte Enables
+ * For VR9, only the address bits [22:0] are mapped to the configuration space:
+ * . Address bits [22:20] select the target bus (1-of-8)1)
+ * . Address bits [19:15] select the target device (1-of-32) on the bus
+ * . Address bits [14:12] select the target function (1-of-8) within the device.
+ * . Address bits [11:2] selects the target dword (1-of-1024) within the selected function.s configuration space
+ * . Address bits [1:0] define the start byte location within the selected dword.
+ */
+static inline u32 pcie_bus_addr(u8 bus_num, u16 devfn, int where)
+{
+	u32 addr;
+	u8  bus;
+
+	if (!bus_num) {
+		/* type 0 */
+		addr = ((PCI_SLOT(devfn) & 0x1F) << 15) | ((PCI_FUNC(devfn) & 0x7) << 12) | ((where & 0xFFF)& ~3);
+	} else {
+		bus = bus_num;
+		/* type 1, only support 8 buses  */
+		addr = ((bus & 0x7) << 20) | ((PCI_SLOT(devfn) & 0x1F) << 15) |
+			((PCI_FUNC(devfn) & 0x7) << 12) | ((where & 0xFFF) & ~3);
+	}
+	return addr;
+}
+
+static int pcie_valid_config(int pcie_port, int bus, int dev)
+{
+	/* RC itself */
+	if ((bus == 0) && (dev == 0)) {
+		return 1;
+	}
+
+	/* No physical link */
+	if (!ifx_pcie_link_up(pcie_port)) {
+		return 0;
+	}
+
+	/* Bus zero only has RC itself
+	* XXX, check if EP will be integrated 
+	*/
+	if ((bus == 0) && (dev != 0)) {
+		return 0;
+	}
+
+	/* Maximum 8 buses supported for VRX */
+	if (bus > 9) {
+		return 0;
+	}
+
+	/* 
+	 * PCIe is PtP link, one bus only supports only one device 
+	 * except bus zero and PCIe switch which is virtual bus device
+	 * The following two conditions really depends on the system design
+	 * and attached the device.
+	 * XXX, how about more new switch
+	*/
+	if ((bus == 1) && (dev != 0)) {
+		return 0;
+	}
+
+	if ((bus >= 3) && (dev != 0)) {
+		return 0;
+	}
+	return 1;
+}
+
+static inline u32 ifx_pcie_cfg_rd(int pcie_port, u32 reg)
+{
+    return IFX_REG_R32((volatile u32 *)(PCIE_CFG_PORT_TO_BASE(pcie_port) + reg));
+}
+
+static inline void ifx_pcie_cfg_wr(int pcie_port, unsigned int reg, u32 val)
+{
+    IFX_REG_W32( val, (volatile u32 *)(PCIE_CFG_PORT_TO_BASE(pcie_port) + reg));
+}
+
+static inline u32 ifx_pcie_rc_cfg_rd(int pcie_port, u32 reg)
+{
+    return IFX_REG_R32((volatile u32 *)(PCIE_RC_PORT_TO_BASE(pcie_port) + reg));
+}
+
+static inline void ifx_pcie_rc_cfg_wr(int pcie_port, unsigned int reg, u32 val)
+{
+	IFX_REG_W32(val, (volatile u32 *)(PCIE_RC_PORT_TO_BASE(pcie_port) + reg));
+}
+
+u32 ifx_pcie_bus_enum_read_hack(int where, u32 value)
+{
+	u32 tvalue = value;
+
+	if (where == PCI_PRIMARY_BUS) {
+		u8 primary, secondary, subordinate;
+
+		primary = tvalue & 0xFF;
+		secondary = (tvalue >> 8) & 0xFF;
+		subordinate = (tvalue >> 16) & 0xFF;
+		primary += pcibios_1st_host_bus_nr();
+		secondary += pcibios_1st_host_bus_nr();
+		subordinate += pcibios_1st_host_bus_nr();
+		tvalue = (tvalue & 0xFF000000) | (u32)primary | (u32)(secondary << 8) | (u32)(subordinate << 16);
+	}
+	return tvalue;
+}
+
+u32 ifx_pcie_bus_enum_write_hack(int where, u32 value)
+{
+    u32 tvalue = value;
+
+    if (where == PCI_PRIMARY_BUS) {
+        u8 primary, secondary, subordinate;
+
+        primary = tvalue & 0xFF;
+        secondary = (tvalue >> 8) & 0xFF;
+        subordinate = (tvalue >> 16) & 0xFF;
+        if (primary > 0 && primary != 0xFF) {
+            primary -= pcibios_1st_host_bus_nr();
+        }
+
+        if (secondary > 0 && secondary != 0xFF) {
+            secondary -= pcibios_1st_host_bus_nr();
+        }
+        if (subordinate > 0 && subordinate != 0xFF) {
+            subordinate -= pcibios_1st_host_bus_nr();
+        }
+        tvalue = (tvalue & 0xFF000000) | (u32)primary | (u32)(secondary << 8) | (u32)(subordinate << 16);
+    }
+    else if (where == PCI_SUBORDINATE_BUS) {
+        u8 subordinate = tvalue & 0xFF;
+
+        subordinate = subordinate > 0 ? subordinate - pcibios_1st_host_bus_nr() : 0;
+        tvalue = subordinate;
+    }
+    return tvalue;
+}
+
+static int ifx_pcie_read_config(struct pci_bus *bus, u32 devfn,
+				int where, int size, u32 *value)
+{
+    u32 data = 0;
+    int bus_number = bus->number;
+    static const u32 mask[8] = {0, 0xff, 0xffff, 0, 0xffffffff, 0, 0, 0};
+    int ret = PCIBIOS_SUCCESSFUL;
+    struct ifx_pci_controller *ctrl = bus->sysdata;
+    int pcie_port = ctrl->port;
+
+    if (unlikely(size != 1 && size != 2 && size != 4)){
+        ret = PCIBIOS_BAD_REGISTER_NUMBER;
+        goto out;
+    }
+
+    /* Make sure the address is aligned to natural boundary */
+    if (unlikely(((size - 1) & where))) {
+        ret = PCIBIOS_BAD_REGISTER_NUMBER;
+        goto out;
+    }
+
+    /* 
+     * If we are second controller, we have to cheat OS so that it assume 
+     * its bus number starts from 0 in host controller
+     */
+    bus_number = ifx_pcie_bus_nr_deduct(bus_number, pcie_port);
+
+    /* 
+     * We need to force the bus number to be zero on the root 
+     * bus. Linux numbers the 2nd root bus to start after all 
+     * busses on root 0. 
+     */ 
+    if (bus->parent == NULL) {
+        bus_number = 0; 
+    }
+
+    /* 
+     * PCIe only has a single device connected to it. It is 
+     * always device ID 0. Don't bother doing reads for other 
+     * device IDs on the first segment. 
+     */ 
+    if ((bus_number == 0) && (PCI_SLOT(devfn) != 0)) {
+        ret = PCIBIOS_FUNC_NOT_SUPPORTED;
+        goto out; 
+    }
+
+    if (pcie_valid_config(pcie_port, bus_number, PCI_SLOT(devfn)) == 0) {
+        *value = 0xffffffff;
+        ret = PCIBIOS_DEVICE_NOT_FOUND;
+        goto out;
+    }
+
+    PCIE_IRQ_LOCK(ifx_pcie_lock);
+    if (bus_number == 0) { /* RC itself */
+        u32 t;
+
+        t = (where & ~3);
+        data = ifx_pcie_rc_cfg_rd(pcie_port, t);
+    } else {
+        u32 addr = pcie_bus_addr(bus_number, devfn, where);
+
+        data = ifx_pcie_cfg_rd(pcie_port, addr);
+    #ifdef CONFIG_IFX_PCIE_HW_SWAP
+            data = le32_to_cpu(data);
+    #endif /* CONFIG_IFX_PCIE_HW_SWAP */
+    }
+    /* To get a correct PCI topology, we have to restore the bus number to OS */
+    data = ifx_pcie_bus_enum_hack(bus, devfn, where, data, pcie_port, 1);
+
+    PCIE_IRQ_UNLOCK(ifx_pcie_lock);
+
+    *value = (data >> (8 * (where & 3))) & mask[size & 7];
+out:
+    return ret;
+}
+
+static u32 ifx_pcie_size_to_value(int where, int size, u32 data, u32 value)
+{
+	u32 shift;
+	u32 tdata = data;
+
+	switch (size) {
+	case 1:
+		shift = (where & 0x3) << 3;
+		tdata &= ~(0xffU << shift);
+		tdata |= ((value & 0xffU) << shift);
+		break;
+	case 2:
+		shift = (where & 3) << 3;
+		tdata &= ~(0xffffU << shift);
+		tdata |= ((value & 0xffffU) << shift);
+		break;
+	case 4:
+		tdata = value;
+		break;
+	}
+	return tdata;
+}
+
+static int ifx_pcie_write_config(struct pci_bus *bus, u32 devfn,
+				int where, int size, u32 value)
+{
+	int bus_number = bus->number;
+	int ret = PCIBIOS_SUCCESSFUL;
+	struct ifx_pci_controller *ctrl = bus->sysdata;
+	int pcie_port = ctrl->port;
+	u32 tvalue = value;
+	u32 data;
+
+	/* Make sure the address is aligned to natural boundary */
+	if (unlikely(((size - 1) & where))) {
+		ret = PCIBIOS_BAD_REGISTER_NUMBER;
+		goto out;
+	}
+	/* 
+	* If we are second controller, we have to cheat OS so that it assume 
+	* its bus number starts from 0 in host controller
+	*/
+	bus_number = ifx_pcie_bus_nr_deduct(bus_number, pcie_port);
+
+	/* 
+	* We need to force the bus number to be zero on the root 
+	* bus. Linux numbers the 2nd root bus to start after all 
+	* busses on root 0. 
+	*/ 
+	if (bus->parent == NULL) {
+		bus_number = 0; 
+	}
+
+	if (pcie_valid_config(pcie_port, bus_number, PCI_SLOT(devfn)) == 0) {
+		ret = PCIBIOS_DEVICE_NOT_FOUND;
+		goto out;
+	}
+
+	/* XXX, some PCIe device may need some delay */
+	PCIE_IRQ_LOCK(ifx_pcie_lock);
+
+	/* 
+	* To configure the correct bus topology using native way, we have to cheat Os so that
+	* it can configure the PCIe hardware correctly.
+	*/
+	tvalue = ifx_pcie_bus_enum_hack(bus, devfn, where, value, pcie_port, 0);
+
+	if (bus_number == 0) { /* RC itself */
+		u32 t;
+
+		t = (where & ~3);
+		data = ifx_pcie_rc_cfg_rd(pcie_port, t);
+
+		data = ifx_pcie_size_to_value(where, size, data, tvalue);
+
+		ifx_pcie_rc_cfg_wr(pcie_port, t, data);
+	} else {
+		u32 addr = pcie_bus_addr(bus_number, devfn, where);
+
+		data = ifx_pcie_cfg_rd(pcie_port, addr);
+#ifdef CONFIG_IFX_PCIE_HW_SWAP
+		data = le32_to_cpu(data);
+#endif
+
+		data = ifx_pcie_size_to_value(where, size, data, tvalue);
+#ifdef CONFIG_IFX_PCIE_HW_SWAP
+		data = cpu_to_le32(data);
+#endif
+		ifx_pcie_cfg_wr(pcie_port, addr, data);
+	}
+	PCIE_IRQ_UNLOCK(ifx_pcie_lock);
+out:
+	return ret;
+}
+
+static struct resource ifx_pcie_io_resource = {
+	.name	= "PCIe0 I/O space",
+	.start	= PCIE_IO_PHY_BASE,
+	.end	= PCIE_IO_PHY_END,
+	.flags	= IORESOURCE_IO,
+};
+
+static struct resource ifx_pcie_mem_resource = {
+	.name	= "PCIe0 Memory space",
+	.start	= PCIE_MEM_PHY_BASE,
+	.end	= PCIE_MEM_PHY_END,
+	.flags	= IORESOURCE_MEM,
+};
+
+static struct pci_ops ifx_pcie_ops = {
+	.read	= ifx_pcie_read_config,
+	.write	= ifx_pcie_write_config,
+};
+
+static struct ifx_pci_controller ifx_pcie_controller[IFX_PCIE_CORE_NR] = {
+    {
+        .pcic = {
+            .pci_ops      = &ifx_pcie_ops,
+            .mem_resource = &ifx_pcie_mem_resource,
+            .io_resource  = &ifx_pcie_io_resource,
+         },
+         .port = IFX_PCIE_PORT0,
+    },
+};
+
+#ifdef IFX_PCIE_ERROR_INT
+
+static irqreturn_t pcie_rc_core_isr(int irq, void *dev_id)
+{
+	struct ifx_pci_controller *ctrl = (struct ifx_pci_controller *)dev_id;
+	int pcie_port = ctrl->port;
+	u32 reg;
+
+	printk("PCIe RC error intr %d\n", irq);
+	reg = IFX_REG_R32(PCIE_IRNCR(pcie_port));
+	reg &= PCIE_RC_CORE_COMBINED_INT;
+	IFX_REG_W32(reg, PCIE_IRNCR(pcie_port));
+
+	return IRQ_HANDLED;
+}
+
+static int
+pcie_rc_core_int_init(int pcie_port)
+{
+	int ret;
+
+	/* Enable core interrupt */
+	IFX_REG_SET_BIT(PCIE_RC_CORE_COMBINED_INT, PCIE_IRNEN(pcie_port));
+
+	/* Clear it first */
+	IFX_REG_SET_BIT(PCIE_RC_CORE_COMBINED_INT, PCIE_IRNCR(pcie_port));
+	ret = request_irq(pcie_irqs[pcie_port].ir_irq.irq, pcie_rc_core_isr, 0,
+		pcie_irqs[pcie_port].ir_irq.name, &ifx_pcie_controller[pcie_port]);
+	if (ret)
+		printk(KERN_ERR "%s request irq %d failed\n", __func__, IFX_PCIE_IR);
+
+	return ret;
+}
+#endif
+
+int ifx_pcie_bios_map_irq(IFX_PCI_CONST struct pci_dev *dev, u8 slot, u8 pin)
+{
+	u32 irq_bit = 0;
+	int irq = 0;
+	struct ifx_pci_controller *ctrl = dev->bus->sysdata;
+	int pcie_port = ctrl->port;
+
+	printk("%s port %d dev %s slot %d pin %d \n", __func__, pcie_port, pci_name(dev), slot, pin);
+
+	if ((pin == PCIE_LEGACY_DISABLE) || (pin > PCIE_LEGACY_INT_MAX)) {
+		printk(KERN_WARNING "WARNING: dev %s: invalid interrupt pin %d\n", pci_name(dev), pin);
+		return -1;
+	}
+
+	/* Pin index so minus one */
+	irq_bit = pcie_irqs[pcie_port].legacy_irq[pin - 1].irq_bit;
+	irq = pcie_irqs[pcie_port].legacy_irq[pin - 1].irq;
+	IFX_REG_SET_BIT(irq_bit, PCIE_IRNEN(pcie_port));
+	IFX_REG_SET_BIT(irq_bit, PCIE_IRNCR(pcie_port));
+	printk("%s dev %s irq %d assigned\n", __func__, pci_name(dev), irq);
+	return irq;
+}
+
+int  ifx_pcie_bios_plat_dev_init(struct pci_dev *dev)
+{
+    u16 config;
+#ifdef IFX_PCIE_ERROR_INT
+    u32 dconfig; 
+    int pos;
+#endif
+
+    /* Enable reporting System errors and parity errors on all devices */ 
+    /* Enable parity checking and error reporting */ 
+    pci_read_config_word(dev, PCI_COMMAND, &config);
+    config |= PCI_COMMAND_PARITY | PCI_COMMAND_SERR /*| PCI_COMMAND_INVALIDATE |
+          PCI_COMMAND_FAST_BACK*/;
+    pci_write_config_word(dev, PCI_COMMAND, config);
+
+    if (dev->subordinate) {
+        /* Set latency timers on sub bridges */
+        pci_write_config_byte(dev, PCI_SEC_LATENCY_TIMER, 0x40); /* XXX, */
+        /* More bridge error detection */
+        pci_read_config_word(dev, PCI_BRIDGE_CONTROL, &config);
+        config |= PCI_BRIDGE_CTL_PARITY | PCI_BRIDGE_CTL_SERR;
+        pci_write_config_word(dev, PCI_BRIDGE_CONTROL, config);
+    }
+#ifdef IFX_PCIE_ERROR_INT
+    /* Enable the PCIe normal error reporting */
+    pos = pci_find_capability(dev, PCI_CAP_ID_EXP);
+    if (pos) {
+
+        /* Disable system error generation in response to error messages */
+        pci_read_config_word(dev, pos + PCI_EXP_RTCTL, &config);
+        config &= ~(PCI_EXP_RTCTL_SECEE | PCI_EXP_RTCTL_SENFEE | PCI_EXP_RTCTL_SEFEE);
+        pci_write_config_word(dev, pos + PCI_EXP_RTCTL, config);
+
+        /* Clear PCIE Capability's Device Status */
+        pci_read_config_word(dev, pos + PCI_EXP_DEVSTA, &config);
+        pci_write_config_word(dev, pos + PCI_EXP_DEVSTA, config);
+
+        /* Update Device Control */ 
+        pci_read_config_word(dev, pos + PCI_EXP_DEVCTL, &config);
+        /* Correctable Error Reporting */
+        config |= PCI_EXP_DEVCTL_CERE;
+        /* Non-Fatal Error Reporting */
+        config |= PCI_EXP_DEVCTL_NFERE;
+        /* Fatal Error Reporting */
+        config |= PCI_EXP_DEVCTL_FERE;
+        /* Unsupported Request */
+        config |= PCI_EXP_DEVCTL_URRE;
+        pci_write_config_word(dev, pos + PCI_EXP_DEVCTL, config);
+    }
+
+    /* Find the Advanced Error Reporting capability */
+    pos = pci_find_ext_capability(dev, PCI_EXT_CAP_ID_ERR);
+    if (pos) {
+        /* Clear Uncorrectable Error Status */ 
+        pci_read_config_dword(dev, pos + PCI_ERR_UNCOR_STATUS, &dconfig);
+        pci_write_config_dword(dev, pos + PCI_ERR_UNCOR_STATUS, dconfig);
+        /* Enable reporting of all uncorrectable errors */
+        /* Uncorrectable Error Mask - turned on bits disable errors */
+        pci_write_config_dword(dev, pos + PCI_ERR_UNCOR_MASK, 0);
+        /* 
+        * Leave severity at HW default. This only controls if 
+        * errors are reported as uncorrectable or 
+        * correctable, not if the error is reported. 
+        */ 
+        /* PCI_ERR_UNCOR_SEVER - Uncorrectable Error Severity */
+        /* Clear Correctable Error Status */
+        pci_read_config_dword(dev, pos + PCI_ERR_COR_STATUS, &dconfig);
+        pci_write_config_dword(dev, pos + PCI_ERR_COR_STATUS, dconfig);
+        /* Enable reporting of all correctable errors */
+        /* Correctable Error Mask - turned on bits disable errors */
+        pci_write_config_dword(dev, pos + PCI_ERR_COR_MASK, 0);
+        /* Advanced Error Capabilities */ 
+        pci_read_config_dword(dev, pos + PCI_ERR_CAP, &dconfig);
+        /* ECRC Generation Enable */
+        if (dconfig & PCI_ERR_CAP_ECRC_GENC) {
+            dconfig |= PCI_ERR_CAP_ECRC_GENE;
+        }
+        /* ECRC Check Enable */
+        if (dconfig & PCI_ERR_CAP_ECRC_CHKC) {
+            dconfig |= PCI_ERR_CAP_ECRC_CHKE;
+        }
+        pci_write_config_dword(dev, pos + PCI_ERR_CAP, dconfig);
+
+        /* PCI_ERR_HEADER_LOG - Header Log Register (16 bytes) */
+        /* Enable Root Port's interrupt in response to error messages */
+        pci_write_config_dword(dev, pos + PCI_ERR_ROOT_COMMAND,
+              PCI_ERR_ROOT_CMD_COR_EN |
+              PCI_ERR_ROOT_CMD_NONFATAL_EN |
+              PCI_ERR_ROOT_CMD_FATAL_EN); 
+        /* Clear the Root status register */
+        pci_read_config_dword(dev, pos + PCI_ERR_ROOT_STATUS, &dconfig);
+        pci_write_config_dword(dev, pos + PCI_ERR_ROOT_STATUS, dconfig);
+    }
+#endif /* IFX_PCIE_ERROR_INT */
+    /* WAR, only 128 MRRS is supported, force all EPs to support this value */
+    pcie_set_readrq(dev, 128);
+    return 0;
+}
+
+static int
+pcie_rc_initialize(int pcie_port)
+{
+	int i;
+#define IFX_PCIE_PHY_LOOP_CNT  5
+
+	pcie_rcu_endian_setup(pcie_port);
+
+	pcie_ep_gpio_rst_init(pcie_port);
+
+	/* 
+	* XXX, PCIe elastic buffer bug will cause not to be detected. One more 
+	* reset PCIe PHY will solve this issue 
+	*/
+	for (i = 0; i < IFX_PCIE_PHY_LOOP_CNT; i++) {
+		/* Disable PCIe PHY Analog part for sanity check */
+		pcie_phy_pmu_disable(pcie_port);
+
+		pcie_phy_rst_assert(pcie_port);
+		pcie_phy_rst_deassert(pcie_port);
+
+		/* Make sure PHY PLL is stable */
+		udelay(20);
+
+		/* PCIe Core reset enabled, low active, sw programmed */
+		pcie_core_rst_assert(pcie_port);
+
+		/* Put PCIe EP in reset status */
+		pcie_device_rst_assert(pcie_port);
+
+		/* PCI PHY & Core reset disabled, high active, sw programmed */
+		pcie_core_rst_deassert(pcie_port);
+
+		/* Already in a quiet state, program PLL, enable PHY, check ready bit */
+		pcie_phy_clock_mode_setup(pcie_port);
+
+		/* Enable PCIe PHY and Clock */
+		pcie_core_pmu_setup(pcie_port);
+
+		/* Clear status registers */
+		pcie_status_register_clear(pcie_port);
+
+#ifdef CONFIG_PCI_MSI
+		pcie_msi_init(pcie_port);
+#endif /* CONFIG_PCI_MSI */
+		pcie_rc_cfg_reg_setup(pcie_port);
+
+		/* Once link is up, break out */
+		if (pcie_app_loigc_setup(pcie_port) == 0)
+			break;
+	}
+	if (i >= IFX_PCIE_PHY_LOOP_CNT) {
+		printk(KERN_ERR "%s link up failed!!!!!\n", __func__);
+		return -EIO;
+	}
+	/* NB, don't increase ACK/NACK timer timeout value, which will cause a lot of COR errors */
+	pcie_replay_time_update(pcie_port);
+	return 0;
+}
+
+extern int (*ltq_pci_plat_arch_init)(struct pci_dev *dev);
+extern int (*ltq_pci_map_irq)(const struct pci_dev *dev, u8 slot, u8 pin);
+
+static int __init ifx_pcie_bios_init(void)
+{
+    void __iomem *io_map_base;
+    int pcie_port;
+    int startup_port;
+
+
+	ltq_pci_map_irq = ifx_pcie_bios_map_irq;
+	ltq_pci_plat_arch_init = ifx_pcie_bios_plat_dev_init;
+
+    /* Enable AHB Master/ Slave */
+    pcie_ahb_pmu_setup();
+
+    startup_port = IFX_PCIE_PORT0;
+    
+    for (pcie_port = startup_port; pcie_port < IFX_PCIE_CORE_NR; pcie_port++){
+	if (pcie_rc_initialize(pcie_port) == 0) {
+	    IFX_PCIE_PRINT(PCIE_MSG_INIT, "%s: ifx_pcie_cfg_base 0x%p\n", 
+                 __func__, PCIE_CFG_PORT_TO_BASE(pcie_port));
+            /* Otherwise, warning will pop up */
+            io_map_base = ioremap(PCIE_IO_PHY_PORT_TO_BASE(pcie_port), PCIE_IO_SIZE);
+            if (io_map_base == NULL) {
+                IFX_PCIE_PRINT(PCIE_MSG_ERR, "%s io space ioremap failed\n", __func__);
+                return -ENOMEM;
+            }
+            ifx_pcie_controller[pcie_port].pcic.io_map_base = (unsigned long)io_map_base;
+
+            register_pci_controller(&ifx_pcie_controller[pcie_port].pcic);
+            /* XXX, clear error status */
+
+            IFX_PCIE_PRINT(PCIE_MSG_INIT, "%s: mem_resource 0x%p, io_resource 0x%p\n", 
+                              __func__, &ifx_pcie_controller[pcie_port].pcic.mem_resource, 
+                              &ifx_pcie_controller[pcie_port].pcic.io_resource);
+
+        #ifdef IFX_PCIE_ERROR_INT
+            pcie_rc_core_int_init(pcie_port);
+        #endif /* IFX_PCIE_ERROR_INT */
+        }
+    }
+
+    return 0;
+}
+arch_initcall(ifx_pcie_bios_init);
+
+MODULE_LICENSE("GPL");
+MODULE_AUTHOR("Chuanhua.Lei@infineon.com");
+MODULE_SUPPORTED_DEVICE("Infineon builtin PCIe RC module");
+MODULE_DESCRIPTION("Infineon builtin PCIe RC driver");
+
--- /dev/null
+++ b/arch/mips/pci/ifxmips_pcie.h
@@ -0,0 +1,135 @@
+/******************************************************************************
+**
+** FILE NAME    : ifxmips_pcie.h
+** PROJECT      : IFX UEIP for VRX200
+** MODULES      : PCIe module
+**
+** DATE         : 02 Mar 2009
+** AUTHOR       : Lei Chuanhua
+** DESCRIPTION  : PCIe Root Complex Driver
+** COPYRIGHT    :       Copyright (c) 2009
+**                      Infineon Technologies AG
+**                      Am Campeon 1-12, 85579 Neubiberg, Germany
+**
+**    This program is free software; you can redistribute it and/or modify
+**    it under the terms of the GNU General Public License as published by
+**    the Free Software Foundation; either version 2 of the License, or
+**    (at your option) any later version.
+** HISTORY
+** $Version $Date        $Author         $Comment
+** 0.0.1    17 Mar,2009  Lei Chuanhua    Initial version
+*******************************************************************************/
+#ifndef IFXMIPS_PCIE_H
+#define IFXMIPS_PCIE_H
+#include <linux/version.h>
+#include <linux/types.h>
+#include <linux/pci.h>
+#include <linux/interrupt.h>
+#include "ifxmips_pci_common.h"
+#include "ifxmips_pcie_reg.h"
+
+/*!
+ \defgroup IFX_PCIE  PCI Express bus driver module   
+ \brief  PCI Express IP module support VRX200 
+*/
+
+/*!
+ \defgroup IFX_PCIE_OS OS APIs
+ \ingroup IFX_PCIE
+ \brief PCIe bus driver OS interface functions
+*/
+
+/*!
+ \file ifxmips_pcie.h
+ \ingroup IFX_PCIE  
+ \brief header file for PCIe module common header file
+*/
+#define PCIE_IRQ_LOCK(lock) do {             \
+    unsigned long flags;                     \
+    spin_lock_irqsave(&(lock), flags);
+#define PCIE_IRQ_UNLOCK(lock)                \
+    spin_unlock_irqrestore(&(lock), flags);  \
+} while (0)
+
+#if LINUX_VERSION_CODE < KERNEL_VERSION(2,6,18)
+#define IRQF_SHARED SA_SHIRQ
+#endif
+
+#define PCIE_MSG_MSI        0x00000001
+#define PCIE_MSG_ISR        0x00000002
+#define PCIE_MSG_FIXUP      0x00000004
+#define PCIE_MSG_READ_CFG   0x00000008
+#define PCIE_MSG_WRITE_CFG  0x00000010
+#define PCIE_MSG_CFG        (PCIE_MSG_READ_CFG | PCIE_MSG_WRITE_CFG)
+#define PCIE_MSG_REG        0x00000020
+#define PCIE_MSG_INIT       0x00000040
+#define PCIE_MSG_ERR        0x00000080
+#define PCIE_MSG_PHY        0x00000100
+#define PCIE_MSG_ANY        0x000001ff
+
+#define IFX_PCIE_PORT0      0
+#define IFX_PCIE_PORT1      1
+
+#ifdef CONFIG_IFX_PCIE_2ND_CORE
+#define IFX_PCIE_CORE_NR    2
+#else
+#define IFX_PCIE_CORE_NR    1
+#endif
+
+#define IFX_PCIE_ERROR_INT
+
+//#define IFX_PCIE_DBG
+
+#if defined(IFX_PCIE_DBG)
+#define IFX_PCIE_PRINT(_m, _fmt, args...) do {   \
+        ifx_pcie_debug((_fmt), ##args);          \
+} while (0)
+
+#define INLINE 
+#else
+#define IFX_PCIE_PRINT(_m, _fmt, args...)   \
+    do {} while(0)
+#define INLINE inline
+#endif
+
+struct ifx_pci_controller {
+	struct pci_controller   pcic;
+    
+	/* RC specific, per host bus information */
+	u32   port;  /* Port index, 0 -- 1st core, 1 -- 2nd core */
+};
+
+typedef struct ifx_pcie_ir_irq {
+    const unsigned int irq;
+    const char name[16];
+}ifx_pcie_ir_irq_t;
+
+typedef struct ifx_pcie_legacy_irq{
+    const u32 irq_bit;
+    const int irq;
+}ifx_pcie_legacy_irq_t;
+
+typedef struct ifx_pcie_irq {
+    ifx_pcie_ir_irq_t ir_irq;
+    ifx_pcie_legacy_irq_t legacy_irq[PCIE_LEGACY_INT_MAX];
+}ifx_pcie_irq_t;
+
+extern u32 g_pcie_debug_flag;
+extern void ifx_pcie_debug(const char *fmt, ...);
+extern void pcie_phy_clock_mode_setup(int pcie_port);
+extern void pcie_msi_pic_init(int pcie_port);
+extern u32 ifx_pcie_bus_enum_read_hack(int where, u32 value);
+extern u32 ifx_pcie_bus_enum_write_hack(int where, u32 value);
+
+#define CONFIG_VR9
+
+#ifdef CONFIG_VR9
+#include "ifxmips_pcie_vr9.h"
+#elif defined (CONFIG_AR10)
+#include "ifxmips_pcie_ar10.h"
+#else
+#error "PCIE: platform not defined"
+#endif /* CONFIG_VR9 */
+
+#endif  /* IFXMIPS_PCIE_H */
+
--- /dev/null
+++ b/arch/mips/pci/ifxmips_pcie_ar10.h
@@ -0,0 +1,290 @@
+/****************************************************************************
+                              Copyright (c) 2010
+                            Lantiq Deutschland GmbH
+                     Am Campeon 3; 85579 Neubiberg, Germany
+
+  For licensing information, see the file 'LICENSE' in the root folder of
+  this software module.
+
+ *****************************************************************************/
+/*!
+  \file ifxmips_pcie_ar10.h
+  \ingroup IFX_PCIE
+  \brief PCIe RC driver ar10 specific file
+*/
+
+#ifndef IFXMIPS_PCIE_AR10_H
+#define IFXMIPS_PCIE_AR10_H
+#ifndef AUTOCONF_INCLUDED
+#include <linux/config.h>
+#endif /* AUTOCONF_INCLUDED */
+#include <linux/types.h>
+#include <linux/delay.h>
+
+/* Project header file */
+#include <asm/ifx/ifx_types.h>
+#include <asm/ifx/ifx_pmu.h>
+#include <asm/ifx/ifx_gpio.h>
+#include <asm/ifx/ifx_ebu_led.h>
+
+static inline void pcie_ep_gpio_rst_init(int pcie_port)
+{
+    ifx_ebu_led_enable();
+    if (pcie_port == 0) {
+        ifx_ebu_led_set_data(11, 1);        
+    }
+    else {
+        ifx_ebu_led_set_data(12, 1);  
+    }
+}
+
+static inline void pcie_ahb_pmu_setup(void) 
+{
+    /* XXX, moved to CGU to control AHBM */
+}
+
+static inline void pcie_rcu_endian_setup(int pcie_port)
+{
+    u32 reg;
+
+    reg = IFX_REG_R32(IFX_RCU_AHB_ENDIAN);
+    /* Inbound, big endian */
+    reg |= IFX_RCU_BE_AHB4S;
+    if (pcie_port == 0) {
+        reg |= IFX_RCU_BE_PCIE0M;
+
+    #ifdef CONFIG_IFX_PCIE_HW_SWAP
+        /* Outbound, software swap needed */
+        reg |= IFX_RCU_BE_AHB3M;
+        reg &= ~IFX_RCU_BE_PCIE0S;
+    #else
+        /* Outbound little endian  */
+        reg &= ~IFX_RCU_BE_AHB3M;
+        reg &= ~IFX_RCU_BE_PCIE0S;
+    #endif
+    }
+    else {
+        reg |= IFX_RCU_BE_PCIE1M;
+    #ifdef CONFIG_IFX_PCIE1_HW_SWAP
+        /* Outbound, software swap needed */
+        reg |= IFX_RCU_BE_AHB3M;
+        reg &= ~IFX_RCU_BE_PCIE1S;
+    #else
+        /* Outbound little endian  */
+        reg &= ~IFX_RCU_BE_AHB3M;
+        reg &= ~IFX_RCU_BE_PCIE1S;
+    #endif
+    }
+
+    IFX_REG_W32(reg, IFX_RCU_AHB_ENDIAN);
+    IFX_PCIE_PRINT(PCIE_MSG_REG, "%s IFX_RCU_AHB_ENDIAN: 0x%08x\n", __func__, IFX_REG_R32(IFX_RCU_AHB_ENDIAN));
+}
+
+static inline void pcie_phy_pmu_enable(int pcie_port)
+{
+    if (pcie_port == 0) { /* XXX, should use macro*/
+        PCIE0_PHY_PMU_SETUP(IFX_PMU_ENABLE);
+    }
+    else {
+        PCIE1_PHY_PMU_SETUP(IFX_PMU_ENABLE);
+    }
+}
+
+static inline void pcie_phy_pmu_disable(int pcie_port)
+{
+    if (pcie_port == 0) { /* XXX, should use macro*/
+        PCIE0_PHY_PMU_SETUP(IFX_PMU_DISABLE);
+    }
+    else {
+        PCIE1_PHY_PMU_SETUP(IFX_PMU_DISABLE);
+    }
+}
+
+static inline void pcie_pdi_big_endian(int pcie_port)
+{
+    u32 reg;
+
+    reg = IFX_REG_R32(IFX_RCU_AHB_ENDIAN);
+    if (pcie_port == 0) {
+        /* Config AHB->PCIe and PDI endianness */
+        reg |= IFX_RCU_BE_PCIE0_PDI;
+    }
+    else {
+        /* Config AHB->PCIe and PDI endianness */
+        reg |= IFX_RCU_BE_PCIE1_PDI;
+    }
+    IFX_REG_W32(reg, IFX_RCU_AHB_ENDIAN);
+}
+
+static inline void pcie_pdi_pmu_enable(int pcie_port)
+{
+    if (pcie_port == 0) {
+        /* Enable PDI to access PCIe PHY register */
+        PDI0_PMU_SETUP(IFX_PMU_ENABLE);
+    }
+    else {
+        PDI1_PMU_SETUP(IFX_PMU_ENABLE);
+    }
+}
+
+static inline void pcie_core_rst_assert(int pcie_port)
+{
+    u32 reg;
+
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+
+    /* Reset Core, bit 22 */
+    if (pcie_port == 0) {
+        reg |= 0x00400000;
+    }
+    else {
+        reg |= 0x08000000; /* Bit 27 */
+    }
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_core_rst_deassert(int pcie_port)
+{
+    u32 reg;
+
+    /* Make sure one micro-second delay */
+    udelay(1);
+
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+    if (pcie_port == 0) {
+        reg &= ~0x00400000; /* bit 22 */
+    }
+    else {
+        reg &= ~0x08000000; /* Bit 27 */
+    }
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_phy_rst_assert(int pcie_port)
+{
+    u32 reg;
+
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+    if (pcie_port == 0) {
+        reg |= 0x00001000; /* Bit 12 */
+    }
+    else {
+        reg |= 0x00002000; /* Bit 13 */
+    }
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_phy_rst_deassert(int pcie_port)
+{
+    u32 reg;
+
+    /* Make sure one micro-second delay */
+    udelay(1);
+
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+    if (pcie_port == 0) {
+        reg &= ~0x00001000; /* Bit 12 */
+    }
+    else {
+        reg &= ~0x00002000; /* Bit 13 */
+    }
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_device_rst_assert(int pcie_port)
+{
+    if (pcie_port == 0) {
+        ifx_ebu_led_set_data(11, 0);
+    }
+    else {
+        ifx_ebu_led_set_data(12, 0);
+    }
+}
+
+static inline void pcie_device_rst_deassert(int pcie_port)
+{
+    mdelay(100);
+    if (pcie_port == 0) {
+        ifx_ebu_led_set_data(11, 1);
+    }
+    else {
+        ifx_ebu_led_set_data(12, 1);
+    }
+    ifx_ebu_led_disable();
+}
+
+static inline void pcie_core_pmu_setup(int pcie_port)
+{
+    if (pcie_port == 0) {
+        PCIE0_CTRL_PMU_SETUP(IFX_PMU_ENABLE);
+    }
+    else {
+        PCIE1_CTRL_PMU_SETUP(IFX_PMU_ENABLE); 
+    }
+}
+
+static inline void pcie_msi_init(int pcie_port)
+{
+    pcie_msi_pic_init(pcie_port);
+    if (pcie_port == 0) {
+        MSI0_PMU_SETUP(IFX_PMU_ENABLE);
+    }
+    else {
+        MSI1_PMU_SETUP(IFX_PMU_ENABLE);
+    }
+}
+
+static inline u32
+ifx_pcie_bus_nr_deduct(u32 bus_number, int pcie_port)
+{
+    u32 tbus_number = bus_number;
+
+#ifdef CONFIG_IFX_PCIE_2ND_CORE
+    if (pcie_port == IFX_PCIE_PORT1) { /* Port 1 must check if there are two cores enabled */
+        if (pcibios_host_nr() > 1) {
+            tbus_number -= pcibios_1st_host_bus_nr();
+        }        
+    }
+#endif /* CONFIG_IFX_PCI */
+    return tbus_number;
+}
+
+static inline u32
+ifx_pcie_bus_enum_hack(struct pci_bus *bus, u32 devfn, int where, u32 value, int pcie_port, int read)
+{
+    struct pci_dev *pdev;
+    u32 tvalue = value;
+
+    /* Sanity check */
+    pdev = pci_get_slot(bus, devfn);
+    if (pdev == NULL) {
+        return tvalue;
+    }
+
+    /* Only care about PCI bridge */
+    if (pdev->hdr_type != PCI_HEADER_TYPE_BRIDGE) {
+        return tvalue;
+    }
+
+    if (read) { /* Read hack */
+    #ifdef CONFIG_IFX_PCIE_2ND_CORE
+        if (pcie_port == IFX_PCIE_PORT1) { /* Port 1 must check if there are two cores enabled */
+            if (pcibios_host_nr() > 1) {
+                tvalue = ifx_pcie_bus_enum_read_hack(where, tvalue);
+            }
+        }
+    #endif /* CONFIG_IFX_PCIE_2ND_CORE */
+    }
+    else { /* Write hack */
+    #ifdef CONFIG_IFX_PCIE_2ND_CORE
+        if (pcie_port == IFX_PCIE_PORT1) { /* Port 1 must check if there are two cores enabled */
+            if (pcibios_host_nr() > 1) {
+                tvalue = ifx_pcie_bus_enum_write_hack(where, tvalue);
+            }
+        }
+    #endif
+    }
+    return tvalue;
+}
+
+#endif /* IFXMIPS_PCIE_AR10_H */
--- /dev/null
+++ b/arch/mips/pci/ifxmips_pcie_msi.c
@@ -0,0 +1,392 @@
+/******************************************************************************
+**
+** FILE NAME    : ifxmips_pcie_msi.c
+** PROJECT      : IFX UEIP for VRX200
+** MODULES      : PCI MSI sub module
+**
+** DATE         : 02 Mar 2009
+** AUTHOR       : Lei Chuanhua
+** DESCRIPTION  : PCIe MSI Driver
+** COPYRIGHT    :       Copyright (c) 2009
+**                      Infineon Technologies AG
+**                      Am Campeon 1-12, 85579 Neubiberg, Germany
+**
+**    This program is free software; you can redistribute it and/or modify
+**    it under the terms of the GNU General Public License as published by
+**    the Free Software Foundation; either version 2 of the License, or
+**    (at your option) any later version.
+** HISTORY
+** $Date        $Author         $Comment
+** 02 Mar,2009  Lei Chuanhua    Initial version
+*******************************************************************************/
+/*!
+ \defgroup IFX_PCIE_MSI MSI OS APIs
+ \ingroup IFX_PCIE
+ \brief PCIe bus driver OS interface functions
+*/
+
+/*!
+ \file ifxmips_pcie_msi.c
+ \ingroup IFX_PCIE 
+ \brief PCIe MSI OS interface file
+*/
+
+#ifndef AUTOCONF_INCLUDED
+#include <linux/config.h>
+#endif /* AUTOCONF_INCLUDED */
+#include <linux/init.h>
+#include <linux/sched.h>
+#include <linux/slab.h>
+#include <linux/interrupt.h>
+#include <linux/kernel_stat.h>
+#include <linux/pci.h>
+#include <linux/msi.h>
+#include <linux/module.h>
+#include <asm/bootinfo.h>
+#include <asm/irq.h>
+#include <asm/traps.h>
+
+#include <asm/ifx/ifx_types.h>
+#include <asm/ifx/ifx_regs.h>
+#include <asm/ifx/common_routines.h>
+#include <asm/ifx/irq.h>
+
+#include "ifxmips_pcie_reg.h"
+#include "ifxmips_pcie.h"
+
+#define IFX_MSI_IRQ_NUM    16
+
+enum {
+    IFX_PCIE_MSI_IDX0 = 0,
+    IFX_PCIE_MSI_IDX1,
+    IFX_PCIE_MSI_IDX2,
+    IFX_PCIE_MSI_IDX3,
+};
+
+typedef struct ifx_msi_irq_idx {
+    const int irq;
+    const int idx;
+}ifx_msi_irq_idx_t;
+
+struct ifx_msi_pic {
+    volatile u32  pic_table[IFX_MSI_IRQ_NUM];
+    volatile u32  pic_endian;    /* 0x40  */
+};
+typedef struct ifx_msi_pic *ifx_msi_pic_t;
+
+typedef struct ifx_msi_irq {
+    const volatile ifx_msi_pic_t msi_pic_p;
+    const u32 msi_phy_base;
+    const ifx_msi_irq_idx_t msi_irq_idx[IFX_MSI_IRQ_NUM];
+    /*
+     * Each bit in msi_free_irq_bitmask represents a MSI interrupt that is 
+     * in use.
+     */
+    u16 msi_free_irq_bitmask;
+
+    /*
+     * Each bit in msi_multiple_irq_bitmask tells that the device using 
+     * this bit in msi_free_irq_bitmask is also using the next bit. This 
+     * is used so we can disable all of the MSI interrupts when a device 
+     * uses multiple.
+     */
+    u16 msi_multiple_irq_bitmask;
+}ifx_msi_irq_t;
+
+static ifx_msi_irq_t msi_irqs[IFX_PCIE_CORE_NR] = {
+    {
+        .msi_pic_p = (const volatile ifx_msi_pic_t)IFX_MSI_PIC_REG_BASE,
+        .msi_phy_base = PCIE_MSI_PHY_BASE,
+        .msi_irq_idx = {
+            {IFX_PCIE_MSI_IR0, IFX_PCIE_MSI_IDX0}, {IFX_PCIE_MSI_IR1, IFX_PCIE_MSI_IDX1},
+            {IFX_PCIE_MSI_IR2, IFX_PCIE_MSI_IDX2}, {IFX_PCIE_MSI_IR3, IFX_PCIE_MSI_IDX3},
+            {IFX_PCIE_MSI_IR0, IFX_PCIE_MSI_IDX0}, {IFX_PCIE_MSI_IR1, IFX_PCIE_MSI_IDX1},
+            {IFX_PCIE_MSI_IR2, IFX_PCIE_MSI_IDX2}, {IFX_PCIE_MSI_IR3, IFX_PCIE_MSI_IDX3},
+            {IFX_PCIE_MSI_IR0, IFX_PCIE_MSI_IDX0}, {IFX_PCIE_MSI_IR1, IFX_PCIE_MSI_IDX1},
+            {IFX_PCIE_MSI_IR2, IFX_PCIE_MSI_IDX2}, {IFX_PCIE_MSI_IR3, IFX_PCIE_MSI_IDX3},
+            {IFX_PCIE_MSI_IR0, IFX_PCIE_MSI_IDX0}, {IFX_PCIE_MSI_IR1, IFX_PCIE_MSI_IDX1},
+            {IFX_PCIE_MSI_IR2, IFX_PCIE_MSI_IDX2}, {IFX_PCIE_MSI_IR3, IFX_PCIE_MSI_IDX3},
+        },
+        .msi_free_irq_bitmask = 0,
+        .msi_multiple_irq_bitmask= 0,
+    },
+#ifdef CONFIG_IFX_PCIE_2ND_CORE
+    {
+        .msi_pic_p = (const volatile ifx_msi_pic_t)IFX_MSI1_PIC_REG_BASE,
+        .msi_phy_base = PCIE1_MSI_PHY_BASE,
+        .msi_irq_idx = {
+            {IFX_PCIE1_MSI_IR0, IFX_PCIE_MSI_IDX0}, {IFX_PCIE1_MSI_IR1, IFX_PCIE_MSI_IDX1},
+            {IFX_PCIE1_MSI_IR2, IFX_PCIE_MSI_IDX2}, {IFX_PCIE1_MSI_IR3, IFX_PCIE_MSI_IDX3},
+            {IFX_PCIE1_MSI_IR0, IFX_PCIE_MSI_IDX0}, {IFX_PCIE1_MSI_IR1, IFX_PCIE_MSI_IDX1},
+            {IFX_PCIE1_MSI_IR2, IFX_PCIE_MSI_IDX2}, {IFX_PCIE1_MSI_IR3, IFX_PCIE_MSI_IDX3},
+            {IFX_PCIE1_MSI_IR0, IFX_PCIE_MSI_IDX0}, {IFX_PCIE1_MSI_IR1, IFX_PCIE_MSI_IDX1},
+            {IFX_PCIE1_MSI_IR2, IFX_PCIE_MSI_IDX2}, {IFX_PCIE1_MSI_IR3, IFX_PCIE_MSI_IDX3},
+            {IFX_PCIE1_MSI_IR0, IFX_PCIE_MSI_IDX0}, {IFX_PCIE1_MSI_IR1, IFX_PCIE_MSI_IDX1},
+            {IFX_PCIE1_MSI_IR2, IFX_PCIE_MSI_IDX2}, {IFX_PCIE1_MSI_IR3, IFX_PCIE_MSI_IDX3},
+        },
+        .msi_free_irq_bitmask = 0,
+        .msi_multiple_irq_bitmask= 0,
+
+    },
+#endif /* CONFIG_IFX_PCIE_2ND_CORE */
+};
+
+/* 
+ * This lock controls updates to msi_free_irq_bitmask, 
+ * msi_multiple_irq_bitmask and pic register settting
+ */ 
+static DEFINE_SPINLOCK(ifx_pcie_msi_lock);
+
+void pcie_msi_pic_init(int pcie_port)
+{
+    spin_lock(&ifx_pcie_msi_lock);
+    msi_irqs[pcie_port].msi_pic_p->pic_endian = IFX_MSI_PIC_BIG_ENDIAN;
+    spin_unlock(&ifx_pcie_msi_lock);
+}
+
+/** 
+ * \fn int arch_setup_msi_irq(struct pci_dev *pdev, struct msi_desc *desc)
+ * \brief Called when a driver request MSI interrupts instead of the 
+ * legacy INT A-D. This routine will allocate multiple interrupts 
+ * for MSI devices that support them. A device can override this by 
+ * programming the MSI control bits [6:4] before calling 
+ * pci_enable_msi(). 
+ * 
+ * \param[in] pdev   Device requesting MSI interrupts 
+ * \param[in] desc   MSI descriptor 
+ * 
+ * \return   -EINVAL Invalid pcie root port or invalid msi bit
+ * \return    0        OK
+ * \ingroup IFX_PCIE_MSI
+ */
+int 
+arch_setup_msi_irq(struct pci_dev *pdev, struct msi_desc *desc)
+{
+    int  irq, pos;
+    u16  control;
+    int  irq_idx;
+    int  irq_step;
+    int configured_private_bits;
+    int request_private_bits;
+    struct msi_msg msg;
+    u16 search_mask;
+    struct ifx_pci_controller *ctrl = pdev->bus->sysdata;
+    int pcie_port = ctrl->port;
+
+    IFX_PCIE_PRINT(PCIE_MSG_MSI, "%s %s enter\n", __func__, pci_name(pdev));
+
+    /* XXX, skip RC MSI itself */
+    if (pdev->pcie_type == PCI_EXP_TYPE_ROOT_PORT) {
+        IFX_PCIE_PRINT(PCIE_MSG_MSI, "%s RC itself doesn't use MSI interrupt\n", __func__);
+        return -EINVAL;
+    }
+
+    /*
+     * Read the MSI config to figure out how many IRQs this device 
+     * wants.  Most devices only want 1, which will give 
+     * configured_private_bits and request_private_bits equal 0. 
+     */
+    pci_read_config_word(pdev, desc->msi_attrib.pos + PCI_MSI_FLAGS, &control);
+
+    /*
+     * If the number of private bits has been configured then use 
+     * that value instead of the requested number. This gives the 
+     * driver the chance to override the number of interrupts 
+     * before calling pci_enable_msi(). 
+     */
+    configured_private_bits = (control & PCI_MSI_FLAGS_QSIZE) >> 4; 
+    if (configured_private_bits == 0) {
+        /* Nothing is configured, so use the hardware requested size */
+        request_private_bits = (control & PCI_MSI_FLAGS_QMASK) >> 1;
+    }
+    else {
+        /*
+         * Use the number of configured bits, assuming the 
+         * driver wanted to override the hardware request 
+         * value.
+         */
+        request_private_bits = configured_private_bits;
+    }
+
+    /*
+     * The PCI 2.3 spec mandates that there are at most 32
+     * interrupts. If this device asks for more, only give it one.
+     */
+    if (request_private_bits > 5) {
+        request_private_bits = 0;
+    }
+again:
+    /*
+     * The IRQs have to be aligned on a power of two based on the
+     * number being requested.
+     */
+    irq_step = (1 << request_private_bits);
+
+    /* Mask with one bit for each IRQ */
+    search_mask = (1 << irq_step) - 1;
+
+    /*
+     * We're going to search msi_free_irq_bitmask_lock for zero 
+     * bits. This represents an MSI interrupt number that isn't in 
+     * use.
+     */
+    spin_lock(&ifx_pcie_msi_lock);
+    for (pos = 0; pos < IFX_MSI_IRQ_NUM; pos += irq_step) {
+        if ((msi_irqs[pcie_port].msi_free_irq_bitmask & (search_mask << pos)) == 0) {
+            msi_irqs[pcie_port].msi_free_irq_bitmask |= search_mask << pos; 
+            msi_irqs[pcie_port].msi_multiple_irq_bitmask |= (search_mask >> 1) << pos;
+            break; 
+        }
+    }
+    spin_unlock(&ifx_pcie_msi_lock); 
+
+    /* Make sure the search for available interrupts didn't fail */ 
+    if (pos >= IFX_MSI_IRQ_NUM) {
+        if (request_private_bits) {
+            IFX_PCIE_PRINT(PCIE_MSG_MSI, "%s: Unable to find %d free "
+                  "interrupts, trying just one", __func__, 1 << request_private_bits);
+            request_private_bits = 0;
+            goto again;
+        }
+        else {
+            printk(KERN_ERR "%s: Unable to find a free MSI interrupt\n", __func__);
+            return -EINVAL;
+        }
+    } 
+    irq = msi_irqs[pcie_port].msi_irq_idx[pos].irq;
+    irq_idx = msi_irqs[pcie_port].msi_irq_idx[pos].idx;
+
+    IFX_PCIE_PRINT(PCIE_MSG_MSI, "pos %d, irq %d irq_idx %d\n", pos, irq, irq_idx);
+
+    /*
+     * Initialize MSI. This has to match the memory-write endianess from the device 
+     * Address bits [23:12]
+     */
+    spin_lock(&ifx_pcie_msi_lock); 
+    msi_irqs[pcie_port].msi_pic_p->pic_table[pos] = SM(irq_idx, IFX_MSI_PIC_INT_LINE) |
+                    SM((msi_irqs[pcie_port].msi_phy_base >> 12), IFX_MSI_PIC_MSG_ADDR) |
+                    SM((1 << pos), IFX_MSI_PIC_MSG_DATA);
+
+    /* Enable this entry */
+    msi_irqs[pcie_port].msi_pic_p->pic_table[pos] &= ~IFX_MSI_PCI_INT_DISABLE;
+    spin_unlock(&ifx_pcie_msi_lock);
+
+    IFX_PCIE_PRINT(PCIE_MSG_MSI, "pic_table[%d]: 0x%08x\n",
+        pos, msi_irqs[pcie_port].msi_pic_p->pic_table[pos]);
+
+    /* Update the number of IRQs the device has available to it */
+    control &= ~PCI_MSI_FLAGS_QSIZE;
+    control |= (request_private_bits << 4);
+    pci_write_config_word(pdev, desc->msi_attrib.pos + PCI_MSI_FLAGS, control);
+
+    set_irq_msi(irq, desc);
+    msg.address_hi = 0x0;
+    msg.address_lo = msi_irqs[pcie_port].msi_phy_base;
+    msg.data = SM((1 << pos), IFX_MSI_PIC_MSG_DATA);
+    IFX_PCIE_PRINT(PCIE_MSG_MSI, "msi_data: pos %d 0x%08x\n", pos, msg.data);
+
+    write_msi_msg(irq, &msg);
+    IFX_PCIE_PRINT(PCIE_MSG_MSI, "%s exit\n", __func__);
+    return 0;
+}
+
+static int
+pcie_msi_irq_to_port(unsigned int irq, int *port)
+{
+    int ret = 0;
+
+    if (irq == IFX_PCIE_MSI_IR0 || irq == IFX_PCIE_MSI_IR1 ||
+        irq == IFX_PCIE_MSI_IR2 || irq == IFX_PCIE_MSI_IR3) {
+        *port = IFX_PCIE_PORT0;
+    }
+#ifdef CONFIG_IFX_PCIE_2ND_CORE
+    else if (irq == IFX_PCIE1_MSI_IR0 || irq == IFX_PCIE1_MSI_IR1 ||
+        irq == IFX_PCIE1_MSI_IR2 || irq == IFX_PCIE1_MSI_IR3) {
+        *port = IFX_PCIE_PORT1;
+    }
+#endif /* CONFIG_IFX_PCIE_2ND_CORE */
+    else {
+        printk(KERN_ERR "%s: Attempted to teardown illegal " 
+            "MSI interrupt (%d)\n", __func__, irq);
+        ret = -EINVAL;
+    }
+    return ret;
+}
+
+/** 
+ * \fn void arch_teardown_msi_irq(unsigned int irq)
+ * \brief Called when a device no longer needs its MSI interrupts. All 
+ * MSI interrupts for the device are freed. 
+ * 
+ * \param irq   The devices first irq number. There may be multple in sequence.
+ * \return none
+ * \ingroup IFX_PCIE_MSI
+ */
+void 
+arch_teardown_msi_irq(unsigned int irq)
+{
+    int pos;
+    int number_irqs; 
+    u16 bitmask;
+    int pcie_port;
+
+    IFX_PCIE_PRINT(PCIE_MSG_MSI, "%s enter\n", __func__);
+
+    BUG_ON(irq > INT_NUM_IM4_IRL31);
+
+    if (pcie_msi_irq_to_port(irq, &pcie_port) != 0) {
+        return;
+    }
+
+    /* Shift the mask to the correct bit location, not always correct 
+     * Probally, the first match will be chosen.
+     */
+    for (pos = 0; pos < IFX_MSI_IRQ_NUM; pos++) {
+        if ((msi_irqs[pcie_port].msi_irq_idx[pos].irq == irq) 
+            && (msi_irqs[pcie_port].msi_free_irq_bitmask & ( 1 << pos))) {
+            break;
+        }
+    }
+    if (pos >= IFX_MSI_IRQ_NUM) {
+        printk(KERN_ERR "%s: Unable to find a matched MSI interrupt\n", __func__);
+        return;
+    }
+    spin_lock(&ifx_pcie_msi_lock);
+    /* Disable this entry */
+    msi_irqs[pcie_port].msi_pic_p->pic_table[pos] |= IFX_MSI_PCI_INT_DISABLE;
+    msi_irqs[pcie_port].msi_pic_p->pic_table[pos] &= ~(IFX_MSI_PIC_INT_LINE | IFX_MSI_PIC_MSG_ADDR | IFX_MSI_PIC_MSG_DATA);
+    spin_unlock(&ifx_pcie_msi_lock); 
+    /*
+     * Count the number of IRQs we need to free by looking at the
+     * msi_multiple_irq_bitmask. Each bit set means that the next
+     * IRQ is also owned by this device.
+     */ 
+    number_irqs = 0; 
+    while (((pos + number_irqs) < IFX_MSI_IRQ_NUM) && 
+        (msi_irqs[pcie_port].msi_multiple_irq_bitmask & (1 << (pos + number_irqs)))) {
+        number_irqs++;
+    }
+    number_irqs++;
+
+    /* Mask with one bit for each IRQ */
+    bitmask = (1 << number_irqs) - 1;
+
+    bitmask <<= pos;
+    if ((msi_irqs[pcie_port].msi_free_irq_bitmask & bitmask) != bitmask) {
+        printk(KERN_ERR "%s: Attempted to teardown MSI "
+             "interrupt (%d) not in use\n", __func__, irq);
+        return;
+    }
+    /* Checks are done, update the in use bitmask */
+    spin_lock(&ifx_pcie_msi_lock);
+    msi_irqs[pcie_port].msi_free_irq_bitmask &= ~bitmask;
+    msi_irqs[pcie_port].msi_multiple_irq_bitmask &= ~(bitmask >> 1);
+    spin_unlock(&ifx_pcie_msi_lock);
+    IFX_PCIE_PRINT(PCIE_MSG_MSI, "%s exit\n", __func__);
+}
+
+MODULE_LICENSE("GPL");
+MODULE_AUTHOR("Chuanhua.Lei@infineon.com");
+MODULE_SUPPORTED_DEVICE("Infineon PCIe IP builtin MSI PIC module");
+MODULE_DESCRIPTION("Infineon PCIe IP builtin MSI PIC driver");
+
--- /dev/null
+++ b/arch/mips/pci/ifxmips_pcie_phy.c
@@ -0,0 +1,478 @@
+/******************************************************************************
+**
+** FILE NAME    : ifxmips_pcie_phy.c
+** PROJECT      : IFX UEIP for VRX200
+** MODULES      : PCIe PHY sub module
+**
+** DATE         : 14 May 2009
+** AUTHOR       : Lei Chuanhua
+** DESCRIPTION  : PCIe Root Complex Driver
+** COPYRIGHT    :       Copyright (c) 2009
+**                      Infineon Technologies AG
+**                      Am Campeon 1-12, 85579 Neubiberg, Germany
+**
+**    This program is free software; you can redistribute it and/or modify
+**    it under the terms of the GNU General Public License as published by
+**    the Free Software Foundation; either version 2 of the License, or
+**    (at your option) any later version.
+** HISTORY
+** $Version $Date        $Author         $Comment
+** 0.0.1    14 May,2009  Lei Chuanhua    Initial version
+*******************************************************************************/
+/*!
+ \file ifxmips_pcie_phy.c
+ \ingroup IFX_PCIE  
+ \brief PCIe PHY PLL register programming source file
+*/
+#include <linux/types.h>
+#include <linux/kernel.h>
+#include <asm/paccess.h>
+#include <linux/delay.h>
+
+#include "ifxmips_pcie_reg.h"
+#include "ifxmips_pcie.h"
+
+/* PCIe PDI only supports 16 bit operation */
+
+#define IFX_PCIE_PHY_REG_WRITE16(__addr, __data) \
+    ((*(volatile u16 *) (__addr)) = (__data))
+    
+#define IFX_PCIE_PHY_REG_READ16(__addr)  \
+    (*(volatile u16 *) (__addr))
+
+#define IFX_PCIE_PHY_REG16(__addr)   \
+    (*(volatile u16 *) (__addr))
+
+#define IFX_PCIE_PHY_REG(__reg, __value, __mask) do { \
+    u16 read_data;                                    \
+    u16 write_data;                                   \
+    read_data = IFX_PCIE_PHY_REG_READ16((__reg));      \
+    write_data = (read_data & ((u16)~(__mask))) | (((u16)(__value)) & ((u16)(__mask)));\
+    IFX_PCIE_PHY_REG_WRITE16((__reg), write_data);               \
+} while (0)
+
+#define IFX_PCIE_PLL_TIMEOUT 1000 /* Tunnable */
+
+//#define IFX_PCI_PHY_REG_DUMP
+
+#ifdef IFX_PCI_PHY_REG_DUMP
+static void
+pcie_phy_reg_dump(int pcie_port) 
+{
+    printk("PLL REGFILE\n");
+    printk("PCIE_PHY_PLL_CTRL1    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_CTRL1(pcie_port)));
+    printk("PCIE_PHY_PLL_CTRL2    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_CTRL2(pcie_port)));
+    printk("PCIE_PHY_PLL_CTRL3    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_CTRL3(pcie_port)));
+    printk("PCIE_PHY_PLL_CTRL4    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_CTRL4(pcie_port)));
+    printk("PCIE_PHY_PLL_CTRL5    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_CTRL5(pcie_port)));
+    printk("PCIE_PHY_PLL_CTRL6    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_CTRL6(pcie_port)));
+    printk("PCIE_PHY_PLL_CTRL7    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_CTRL7(pcie_port)));
+    printk("PCIE_PHY_PLL_A_CTRL1  0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_A_CTRL1(pcie_port)));
+    printk("PCIE_PHY_PLL_A_CTRL2  0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_A_CTRL2(pcie_port)));
+    printk("PCIE_PHY_PLL_A_CTRL3  0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_A_CTRL3(pcie_port)));
+    printk("PCIE_PHY_PLL_STATUS   0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_STATUS(pcie_port)));
+
+    printk("TX1 REGFILE\n");
+    printk("PCIE_PHY_TX1_CTRL1    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX1_CTRL1(pcie_port)));
+    printk("PCIE_PHY_TX1_CTRL2    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX1_CTRL2(pcie_port)));
+    printk("PCIE_PHY_TX1_CTRL3    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX1_CTRL3(pcie_port)));
+    printk("PCIE_PHY_TX1_A_CTRL1  0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX1_A_CTRL1(pcie_port)));
+    printk("PCIE_PHY_TX1_A_CTRL2  0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX1_A_CTRL2(pcie_port)));
+    printk("PCIE_PHY_TX1_MOD1     0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX1_MOD1(pcie_port)));
+    printk("PCIE_PHY_TX1_MOD2     0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX1_MOD2(pcie_port)));
+    printk("PCIE_PHY_TX1_MOD3     0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX1_MOD3(pcie_port)));
+
+    printk("TX2 REGFILE\n");
+    printk("PCIE_PHY_TX2_CTRL1    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX2_CTRL1(pcie_port)));
+    printk("PCIE_PHY_TX2_CTRL2    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX2_CTRL2(pcie_port)));
+    printk("PCIE_PHY_TX2_A_CTRL1  0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX2_A_CTRL1(pcie_port)));
+    printk("PCIE_PHY_TX2_A_CTRL2  0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX2_A_CTRL2(pcie_port)));
+    printk("PCIE_PHY_TX2_MOD1     0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX2_MOD1(pcie_port)));
+    printk("PCIE_PHY_TX2_MOD2     0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX2_MOD2(pcie_port)));
+    printk("PCIE_PHY_TX2_MOD3     0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_TX2_MOD3(pcie_port)));
+
+    printk("RX1 REGFILE\n");
+    printk("PCIE_PHY_RX1_CTRL1    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_RX1_CTRL1(pcie_port)));
+    printk("PCIE_PHY_RX1_CTRL2    0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_RX1_CTRL2(pcie_port)));
+    printk("PCIE_PHY_RX1_CDR      0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_RX1_CDR(pcie_port)));
+    printk("PCIE_PHY_RX1_EI       0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_RX1_EI(pcie_port)));
+    printk("PCIE_PHY_RX1_A_CTRL   0x%04x\n", IFX_PCIE_PHY_REG16(PCIE_PHY_RX1_A_CTRL(pcie_port)));
+}
+#endif /* IFX_PCI_PHY_REG_DUMP */
+
+static void
+pcie_phy_comm_setup(int pcie_port)
+{
+   /* PLL Setting */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL1(pcie_port), 0x120e, 0xFFFF);
+
+    /* increase the bias reference voltage */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL2(pcie_port), 0x39D7, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL3(pcie_port), 0x0900, 0xFFFF);
+
+    /* Endcnt */
+    IFX_PCIE_PHY_REG(PCIE_PHY_RX1_EI(pcie_port), 0x0004, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_RX1_A_CTRL(pcie_port), 0x6803, 0xFFFF);
+
+    /* force */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_CTRL1(pcie_port), 0x0008, 0x0008);
+
+    /* predrv_ser_en */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_A_CTRL2(pcie_port), 0x0706, 0xFFFF);
+
+    /* ctrl_lim */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_CTRL3(pcie_port), 0x1FFF, 0xFFFF);
+
+    /* ctrl */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_A_CTRL1(pcie_port), 0x0800, 0xFF00);
+
+    /* predrv_ser_en */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX2_A_CTRL2(pcie_port), 0x4702, 0x7F00);
+
+    /* RTERM*/
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_CTRL2(pcie_port), 0x2e00, 0xFFFF);
+
+    /* Improved 100MHz clock output  */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX2_CTRL2(pcie_port), 0x3096, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX2_A_CTRL2(pcie_port), 0x4707, 0xFFFF);
+
+    /* Reduced CDR BW to avoid glitches */
+    IFX_PCIE_PHY_REG(PCIE_PHY_RX1_CDR(pcie_port), 0x0235, 0xFFFF);
+}
+
+#ifdef CONFIG_IFX_PCIE_PHY_36MHZ_MODE
+static void 
+pcie_phy_36mhz_mode_setup(int pcie_port) 
+{
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "%s pcie_port %d enter\n", __func__, pcie_port);
+#ifdef IFX_PCI_PHY_REG_DUMP
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "Initial PHY register dump\n");
+    pcie_phy_reg_dump(pcie_port);
+#endif
+
+    /* en_ext_mmd_div_ratio */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL3(pcie_port), 0x0000, 0x0002);
+
+    /* ext_mmd_div_ratio*/
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL3(pcie_port), 0x0000, 0x0070);
+
+    /* pll_ensdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x0200, 0x0200);
+
+    /* en_const_sdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x0100, 0x0100);
+
+    /* mmd */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL3(pcie_port), 0x2000, 0xe000);
+
+    /* lf_mode */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL2(pcie_port), 0x0000, 0x4000);
+
+    /* const_sdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL1(pcie_port), 0x38e4, 0xFFFF);
+
+    /* const sdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x00ee, 0x00FF);
+
+    /* pllmod */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL7(pcie_port), 0x0002, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL6(pcie_port), 0x3a04, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL5(pcie_port), 0xfae3, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL4(pcie_port), 0x1b72, 0xFFFF);
+
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "%s pcie_port %d exit\n", __func__, pcie_port);
+}
+#endif /* CONFIG_IFX_PCIE_PHY_36MHZ_MODE */
+
+#ifdef CONFIG_IFX_PCIE_PHY_36MHZ_SSC_MODE
+static void 
+pcie_phy_36mhz_ssc_mode_setup(int pcie_port) 
+{
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "%s pcie_port %d enter\n", __func__, pcie_port);
+#ifdef IFX_PCI_PHY_REG_DUMP
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "Initial PHY register dump\n");
+    pcie_phy_reg_dump(pcie_port);
+#endif
+
+    /* PLL Setting */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL1(pcie_port), 0x120e, 0xFFFF);
+
+    /* Increase the bias reference voltage */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL2(pcie_port), 0x39D7, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL3(pcie_port), 0x0900, 0xFFFF);
+
+    /* Endcnt */
+    IFX_PCIE_PHY_REG(PCIE_PHY_RX1_EI(pcie_port), 0x0004, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_RX1_A_CTRL(pcie_port), 0x6803, 0xFFFF);
+
+    /* Force */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_CTRL1(pcie_port), 0x0008, 0x0008);
+
+    /* Predrv_ser_en */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_A_CTRL2(pcie_port), 0x0706, 0xFFFF);
+
+    /* ctrl_lim */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_CTRL3(pcie_port), 0x1FFF, 0xFFFF);
+
+    /* ctrl */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_A_CTRL1(pcie_port), 0x0800, 0xFF00);
+
+    /* predrv_ser_en */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX2_A_CTRL2(pcie_port), 0x4702, 0x7F00);
+
+    /* RTERM*/
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_CTRL2(pcie_port), 0x2e00, 0xFFFF);
+
+    /* en_ext_mmd_div_ratio */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL3(pcie_port), 0x0000, 0x0002);
+
+    /* ext_mmd_div_ratio*/
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL3(pcie_port), 0x0000, 0x0070);
+
+    /* pll_ensdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x0400, 0x0400);
+
+    /* en_const_sdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x0200, 0x0200);
+
+    /* mmd */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL3(pcie_port), 0x2000, 0xe000);
+
+    /* lf_mode */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL2(pcie_port), 0x0000, 0x4000);
+
+    /* const_sdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL1(pcie_port), 0x38e4, 0xFFFF);
+
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x0000, 0x0100);
+    /* const sdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x00ee, 0x00FF);
+
+    /* pllmod */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL7(pcie_port), 0x0002, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL6(pcie_port), 0x3a04, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL5(pcie_port), 0xfae3, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL4(pcie_port), 0x1c72, 0xFFFF);
+
+    /* improved 100MHz clock output  */
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX2_CTRL2(pcie_port), 0x3096, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX2_A_CTRL2(pcie_port), 0x4707, 0xFFFF);
+
+    /* reduced CDR BW to avoid glitches */
+    IFX_PCIE_PHY_REG(PCIE_PHY_RX1_CDR(pcie_port), 0x0235, 0xFFFF);
+    
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "%s pcie_port %d exit\n", __func__, pcie_port);
+}
+#endif /* CONFIG_IFX_PCIE_PHY_36MHZ_SSC_MODE */
+
+#ifdef CONFIG_IFX_PCIE_PHY_25MHZ_MODE
+static void 
+pcie_phy_25mhz_mode_setup(int pcie_port) 
+{
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "%s pcie_port %d enter\n", __func__, pcie_port);
+#ifdef IFX_PCI_PHY_REG_DUMP
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "Initial PHY register dump\n");
+    pcie_phy_reg_dump(pcie_port);
+#endif
+    /* en_const_sdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x0100, 0x0100);
+
+    /* pll_ensdm */    
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x0000, 0x0200);
+
+    /* en_ext_mmd_div_ratio*/
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL3(pcie_port), 0x0002, 0x0002);
+
+    /* ext_mmd_div_ratio*/
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL3(pcie_port), 0x0040, 0x0070);
+
+    /* mmd */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL3(pcie_port), 0x6000, 0xe000);
+
+    /* lf_mode */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL2(pcie_port), 0x4000, 0x4000);
+
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "%s pcie_port %d exit\n", __func__, pcie_port);
+}
+#endif /* CONFIG_IFX_PCIE_PHY_25MHZ_MODE */
+
+#ifdef CONFIG_IFX_PCIE_PHY_100MHZ_MODE
+static void 
+pcie_phy_100mhz_mode_setup(int pcie_port) 
+{
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "%s pcie_port %d enter\n", __func__, pcie_port);
+#ifdef IFX_PCI_PHY_REG_DUMP
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "Initial PHY register dump\n");
+    pcie_phy_reg_dump(pcie_port);
+#endif 
+    /* en_ext_mmd_div_ratio */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL3(pcie_port), 0x0000, 0x0002);
+
+    /* ext_mmd_div_ratio*/
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL3(pcie_port), 0x0000, 0x0070);
+
+    /* pll_ensdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x0200, 0x0200);
+
+    /* en_const_sdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x0100, 0x0100);
+
+    /* mmd */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL3(pcie_port), 0x2000, 0xe000);
+
+    /* lf_mode */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_A_CTRL2(pcie_port), 0x0000, 0x4000);
+
+    /* const_sdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL1(pcie_port), 0x38e4, 0xFFFF);
+
+    /* const sdm */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL2(pcie_port), 0x00ee, 0x00FF);
+
+    /* pllmod */
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL7(pcie_port), 0x0002, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL6(pcie_port), 0x3a04, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL5(pcie_port), 0xfae3, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_PLL_CTRL4(pcie_port), 0x1b72, 0xFFFF);
+
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "%s pcie_port %d exit\n", __func__, pcie_port);
+}
+#endif /* CONFIG_IFX_PCIE_PHY_100MHZ_MODE */
+
+static int
+pcie_phy_wait_startup_ready(int pcie_port)
+{
+    int i;
+
+    for (i = 0; i < IFX_PCIE_PLL_TIMEOUT; i++) {
+        if ((IFX_PCIE_PHY_REG16(PCIE_PHY_PLL_STATUS(pcie_port)) & 0x0040) != 0) {
+            break;
+        }
+        udelay(10);
+    }
+    if (i >= IFX_PCIE_PLL_TIMEOUT) {
+        printk(KERN_ERR "%s PLL Link timeout\n", __func__);
+        return -1;
+    }
+    return 0;
+}
+
+static void 
+pcie_phy_load_enable(int pcie_port, int slice) 
+{
+    /* Set the load_en of tx/rx slice to '1' */
+    switch (slice) {
+        case 1:
+            IFX_PCIE_PHY_REG(PCIE_PHY_TX1_CTRL1(pcie_port), 0x0010, 0x0010);
+            break;
+        case 2:
+            IFX_PCIE_PHY_REG(PCIE_PHY_TX2_CTRL1(pcie_port), 0x0010, 0x0010);
+            break;
+        case 3:
+            IFX_PCIE_PHY_REG(PCIE_PHY_RX1_CTRL1(pcie_port), 0x0002, 0x0002);
+            break;
+    }
+}
+
+static void 
+pcie_phy_load_disable(int pcie_port, int slice) 
+{ 
+    /* set the load_en of tx/rx slice to '0' */ 
+    switch (slice) {
+        case 1:
+            IFX_PCIE_PHY_REG(PCIE_PHY_TX1_CTRL1(pcie_port), 0x0000, 0x0010);
+            break;
+        case 2:
+            IFX_PCIE_PHY_REG(PCIE_PHY_TX2_CTRL1(pcie_port), 0x0000, 0x0010);
+            break;
+        case 3: 
+            IFX_PCIE_PHY_REG(PCIE_PHY_RX1_CTRL1(pcie_port), 0x0000, 0x0002);
+            break;
+    }
+}
+
+static void 
+pcie_phy_load_war(int pcie_port)
+{
+    int slice;
+
+    for (slice = 1; slice < 4; slice++) {
+        pcie_phy_load_enable(pcie_port, slice);
+        udelay(1);
+        pcie_phy_load_disable(pcie_port, slice);
+    }
+}
+
+static void 
+pcie_phy_tx2_modulation(int pcie_port)
+{
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX2_MOD1(pcie_port), 0x1FFE, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX2_MOD2(pcie_port), 0xFFFE, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX2_MOD3(pcie_port), 0x0601, 0xFFFF);
+    mdelay(1);
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX2_MOD3(pcie_port), 0x0001, 0xFFFF);
+}
+
+static void 
+pcie_phy_tx1_modulation(int pcie_port)
+{
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_MOD1(pcie_port), 0x1FFE, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_MOD2(pcie_port), 0xFFFE, 0xFFFF);
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_MOD3(pcie_port), 0x0601, 0xFFFF);
+    mdelay(1);
+    IFX_PCIE_PHY_REG(PCIE_PHY_TX1_MOD3(pcie_port), 0x0001, 0xFFFF);
+}
+
+static void
+pcie_phy_tx_modulation_war(int pcie_port)
+{
+    int i;
+
+#define PCIE_PHY_MODULATION_NUM 5 
+    for (i = 0; i < PCIE_PHY_MODULATION_NUM; i++) {
+        pcie_phy_tx2_modulation(pcie_port);
+        pcie_phy_tx1_modulation(pcie_port);
+    }
+#undef PCIE_PHY_MODULATION_NUM
+}
+
+void
+pcie_phy_clock_mode_setup(int pcie_port)
+{
+    pcie_pdi_big_endian(pcie_port);
+
+    /* Enable PDI to access PCIe PHY register */
+    pcie_pdi_pmu_enable(pcie_port);
+
+    /* Configure PLL and PHY clock */
+    pcie_phy_comm_setup(pcie_port);
+
+#ifdef CONFIG_IFX_PCIE_PHY_36MHZ_MODE
+    pcie_phy_36mhz_mode_setup(pcie_port);
+#elif defined(CONFIG_IFX_PCIE_PHY_36MHZ_SSC_MODE)
+    pcie_phy_36mhz_ssc_mode_setup(pcie_port);
+#elif defined(CONFIG_IFX_PCIE_PHY_25MHZ_MODE)
+    pcie_phy_25mhz_mode_setup(pcie_port);
+#elif defined (CONFIG_IFX_PCIE_PHY_100MHZ_MODE)
+    pcie_phy_100mhz_mode_setup(pcie_port);
+#else
+    #error "PCIE PHY Clock Mode must be chosen first!!!!"
+#endif /* CONFIG_IFX_PCIE_PHY_36MHZ_MODE */
+
+    /* Enable PCIe PHY and make PLL setting take effect */
+    pcie_phy_pmu_enable(pcie_port);
+
+    /* Check if we are in startup_ready status */
+    pcie_phy_wait_startup_ready(pcie_port);
+
+    pcie_phy_load_war(pcie_port);
+
+    /* Apply TX modulation workarounds */
+    pcie_phy_tx_modulation_war(pcie_port);
+
+#ifdef IFX_PCI_PHY_REG_DUMP
+    IFX_PCIE_PRINT(PCIE_MSG_PHY, "Modified PHY register dump\n");
+    pcie_phy_reg_dump(pcie_port);
+#endif
+}
+
--- /dev/null
+++ b/arch/mips/pci/ifxmips_pcie_pm.c
@@ -0,0 +1,176 @@
+/******************************************************************************
+**
+** FILE NAME    : ifxmips_pcie_pm.c
+** PROJECT      : IFX UEIP
+** MODULES      : PCIE Root Complex Driver
+**
+** DATE         : 21 Dec 2009
+** AUTHOR       : Lei Chuanhua
+** DESCRIPTION  : PCIE Root Complex Driver Power Managment
+** COPYRIGHT    :       Copyright (c) 2009
+**                      Lantiq Deutschland GmbH
+**                      Am Campeon 3, 85579 Neubiberg, Germany
+**
+**    This program is free software; you can redistribute it and/or modify
+**    it under the terms of the GNU General Public License as published by
+**    the Free Software Foundation; either version 2 of the License, or
+**    (at your option) any later version.
+**
+** HISTORY
+** $Date        $Author         $Comment
+** 21 Dec,2009   Lei Chuanhua    First UEIP release
+*******************************************************************************/
+/*!
+  \defgroup IFX_PCIE_PM Power Management functions
+  \ingroup IFX_PCIE
+  \brief IFX PCIE Root Complex Driver power management functions
+*/
+
+/*!
+ \file ifxmips_pcie_pm.c
+ \ingroup IFX_PCIE    
+ \brief source file for PCIE Root Complex Driver Power Management
+*/
+
+#ifndef EXPORT_SYMTAB
+#define EXPORT_SYMTAB
+#endif
+#ifndef AUTOCONF_INCLUDED
+#include <linux/config.h>
+#endif /* AUTOCONF_INCLUDED */
+#include <linux/version.h>
+#include <linux/module.h>
+#include <linux/types.h>
+#include <linux/kernel.h>
+#include <asm/system.h>
+
+/* Project header */
+#include <asm/ifx/ifx_types.h>
+#include <asm/ifx/ifx_regs.h>
+#include <asm/ifx/common_routines.h>
+#include <asm/ifx/ifx_pmcu.h>
+#include "ifxmips_pcie_pm.h"
+
+/** 
+ * \fn static IFX_PMCU_RETURN_t ifx_pcie_pmcu_state_change(IFX_PMCU_STATE_t pmcuState)
+ * \brief the callback function to request pmcu state in the power management hardware-dependent module
+ *
+ * \param pmcuState This parameter is a PMCU state.
+ *
+ * \return IFX_PMCU_RETURN_SUCCESS Set Power State successfully
+ * \return IFX_PMCU_RETURN_ERROR   Failed to set power state.
+ * \return IFX_PMCU_RETURN_DENIED  Not allowed to operate power state
+ * \ingroup IFX_PCIE_PM
+ */
+static IFX_PMCU_RETURN_t 
+ifx_pcie_pmcu_state_change(IFX_PMCU_STATE_t pmcuState)
+{
+    switch(pmcuState) 
+    {
+        case IFX_PMCU_STATE_D0:
+            return IFX_PMCU_RETURN_SUCCESS;
+        case IFX_PMCU_STATE_D1: // Not Applicable
+            return IFX_PMCU_RETURN_DENIED;
+        case IFX_PMCU_STATE_D2: // Not Applicable
+            return IFX_PMCU_RETURN_DENIED;
+        case IFX_PMCU_STATE_D3: // Module clock gating and Power gating
+            return IFX_PMCU_RETURN_SUCCESS;
+        default:
+            return IFX_PMCU_RETURN_DENIED;
+    }
+}
+
+/** 
+ * \fn static IFX_PMCU_RETURN_t ifx_pcie_pmcu_state_get(IFX_PMCU_STATE_t *pmcuState)
+ * \brief the callback function to get pmcu state in the power management hardware-dependent module
+
+ * \param pmcuState Pointer to return power state.
+ *
+ * \return IFX_PMCU_RETURN_SUCCESS Set Power State successfully
+ * \return IFX_PMCU_RETURN_ERROR   Failed to set power state.
+ * \return IFX_PMCU_RETURN_DENIED  Not allowed to operate power state
+ * \ingroup IFX_PCIE_PM
+ */
+static IFX_PMCU_RETURN_t 
+ifx_pcie_pmcu_state_get(IFX_PMCU_STATE_t *pmcuState)
+{
+    return IFX_PMCU_RETURN_SUCCESS;
+}
+
+/**
+ * \fn IFX_PMCU_RETURN_t ifx_pcie_pmcu_prechange(IFX_PMCU_MODULE_t pmcuModule, IFX_PMCU_STATE_t newState, IFX_PMCU_STATE_t oldState)
+ * \brief Apply all callbacks registered to be executed before a state change for pmcuModule
+ * 
+ * \param   pmcuModule      Module
+ * \param   newState        New state
+ * \param   oldState        Old state
+ * \return  IFX_PMCU_RETURN_SUCCESS Set Power State successfully
+ * \return  IFX_PMCU_RETURN_ERROR   Failed to set power state.
+ * \ingroup IFX_PCIE_PM
+ */
+static IFX_PMCU_RETURN_t 
+ifx_pcie_pmcu_prechange(IFX_PMCU_MODULE_t pmcuModule, IFX_PMCU_STATE_t newState, IFX_PMCU_STATE_t oldState)
+{
+    return IFX_PMCU_RETURN_SUCCESS;
+}
+
+/**
+ * \fn IFX_PMCU_RETURN_t ifx_pcie_pmcu_postchange(IFX_PMCU_MODULE_t pmcuModule, IFX_PMCU_STATE_t newState, IFX_PMCU_STATE_t oldState)
+ * \brief Apply all callbacks registered to be executed before a state change for pmcuModule
+ * 
+ * \param   pmcuModule      Module
+ * \param   newState        New state
+ * \param   oldState        Old state
+ * \return IFX_PMCU_RETURN_SUCCESS Set Power State successfully
+ * \return IFX_PMCU_RETURN_ERROR   Failed to set power state.
+ * \ingroup IFX_PCIE_PM
+ */
+static IFX_PMCU_RETURN_t 
+ifx_pcie_pmcu_postchange(IFX_PMCU_MODULE_t pmcuModule, IFX_PMCU_STATE_t newState, IFX_PMCU_STATE_t oldState)
+{
+    return IFX_PMCU_RETURN_SUCCESS;
+}
+
+/** 
+ * \fn static void ifx_pcie_pmcu_init(void)
+ * \brief Register with central PMCU module
+ * \return none
+ * \ingroup IFX_PCIE_PM
+ */
+void
+ifx_pcie_pmcu_init(void)
+{
+    IFX_PMCU_REGISTER_t pmcuRegister;
+
+    /* XXX, hook driver context */
+
+    /* State function register */
+    memset(&pmcuRegister, 0, sizeof(IFX_PMCU_REGISTER_t));
+    pmcuRegister.pmcuModule = IFX_PMCU_MODULE_PCIE;
+    pmcuRegister.pmcuModuleNr = 0;
+    pmcuRegister.ifx_pmcu_state_change = ifx_pcie_pmcu_state_change;
+    pmcuRegister.ifx_pmcu_state_get = ifx_pcie_pmcu_state_get;
+    pmcuRegister.pre = ifx_pcie_pmcu_prechange;
+    pmcuRegister.post= ifx_pcie_pmcu_postchange;
+    ifx_pmcu_register(&pmcuRegister); 
+}
+
+/** 
+ * \fn static void ifx_pcie_pmcu_exit(void)
+ * \brief Unregister with central PMCU module
+ *
+ * \return none
+ * \ingroup IFX_PCIE_PM
+ */
+void
+ifx_pcie_pmcu_exit(void)
+{
+    IFX_PMCU_REGISTER_t pmcuUnRegister;
+
+   /* XXX, hook driver context */
+   
+    pmcuUnRegister.pmcuModule = IFX_PMCU_MODULE_PCIE;
+    pmcuUnRegister.pmcuModuleNr = 0;
+    ifx_pmcu_unregister(&pmcuUnRegister);
+}
+
--- /dev/null
+++ b/arch/mips/pci/ifxmips_pcie_pm.h
@@ -0,0 +1,36 @@
+/******************************************************************************
+**
+** FILE NAME    : ifxmips_pcie_pm.h
+** PROJECT      : IFX UEIP
+** MODULES      : PCIe Root Complex Driver
+**
+** DATE         : 21 Dec 2009
+** AUTHOR       : Lei Chuanhua
+** DESCRIPTION  : PCIe Root Complex Driver Power Managment
+** COPYRIGHT    :       Copyright (c) 2009
+**                      Lantiq Deutschland GmbH
+**                      Am Campeon 3, 85579 Neubiberg, Germany
+**
+**    This program is free software; you can redistribute it and/or modify
+**    it under the terms of the GNU General Public License as published by
+**    the Free Software Foundation; either version 2 of the License, or
+**    (at your option) any later version.
+**
+** HISTORY
+** $Date        $Author         $Comment
+** 21 Dec,2009   Lei Chuanhua    First UEIP release
+*******************************************************************************/
+/*!
+ \file ifxmips_pcie_pm.h
+ \ingroup IFX_PCIE 
+ \brief header file for PCIe Root Complex Driver Power Management
+*/
+
+#ifndef IFXMIPS_PCIE_PM_H
+#define IFXMIPS_PCIE_PM_H
+
+void ifx_pcie_pmcu_init(void);
+void ifx_pcie_pmcu_exit(void);
+
+#endif /* IFXMIPS_PCIE_PM_H  */
+
--- /dev/null
+++ b/arch/mips/pci/ifxmips_pcie_reg.h
@@ -0,0 +1,1001 @@
+/******************************************************************************
+**
+** FILE NAME    : ifxmips_pcie_reg.h
+** PROJECT      : IFX UEIP for VRX200
+** MODULES      : PCIe module
+**
+** DATE         : 02 Mar 2009
+** AUTHOR       : Lei Chuanhua
+** DESCRIPTION  : PCIe Root Complex Driver
+** COPYRIGHT    :       Copyright (c) 2009
+**                      Infineon Technologies AG
+**                      Am Campeon 1-12, 85579 Neubiberg, Germany
+**
+**    This program is free software; you can redistribute it and/or modify
+**    it under the terms of the GNU General Public License as published by
+**    the Free Software Foundation; either version 2 of the License, or
+**    (at your option) any later version.
+** HISTORY
+** $Version $Date        $Author         $Comment
+** 0.0.1    17 Mar,2009  Lei Chuanhua    Initial version
+*******************************************************************************/
+#ifndef IFXMIPS_PCIE_REG_H
+#define IFXMIPS_PCIE_REG_H
+/*!
+ \file ifxmips_pcie_reg.h
+ \ingroup IFX_PCIE  
+ \brief header file for PCIe module register definition
+*/
+/* PCIe Address Mapping Base */
+#define PCIE_CFG_PHY_BASE        0x1D000000UL
+#define PCIE_CFG_BASE           (KSEG1 + PCIE_CFG_PHY_BASE)
+#define PCIE_CFG_SIZE           (8 * 1024 * 1024)
+
+#define PCIE_MEM_PHY_BASE        0x1C000000UL
+#define PCIE_MEM_BASE           (KSEG1 + PCIE_MEM_PHY_BASE)
+#define PCIE_MEM_SIZE           (16 * 1024 * 1024)
+#define PCIE_MEM_PHY_END        (PCIE_MEM_PHY_BASE + PCIE_MEM_SIZE - 1)
+
+#define PCIE_IO_PHY_BASE         0x1D800000UL
+#define PCIE_IO_BASE            (KSEG1 + PCIE_IO_PHY_BASE)
+#define PCIE_IO_SIZE            (1 * 1024 * 1024)
+#define PCIE_IO_PHY_END         (PCIE_IO_PHY_BASE + PCIE_IO_SIZE - 1)
+
+#define PCIE_RC_CFG_BASE        (KSEG1 + 0x1D900000)
+#define PCIE_APP_LOGIC_REG      (KSEG1 + 0x1E100900)
+#define PCIE_MSI_PHY_BASE        0x1F600000UL
+
+#define PCIE_PDI_PHY_BASE        0x1F106800UL
+#define PCIE_PDI_BASE           (KSEG1 + PCIE_PDI_PHY_BASE)
+#define PCIE_PDI_SIZE            0x400
+
+#define PCIE1_CFG_PHY_BASE        0x19000000UL
+#define PCIE1_CFG_BASE           (KSEG1 + PCIE1_CFG_PHY_BASE)
+#define PCIE1_CFG_SIZE           (8 * 1024 * 1024)
+
+#define PCIE1_MEM_PHY_BASE        0x18000000UL
+#define PCIE1_MEM_BASE           (KSEG1 + PCIE1_MEM_PHY_BASE)
+#define PCIE1_MEM_SIZE           (16 * 1024 * 1024)
+#define PCIE1_MEM_PHY_END        (PCIE1_MEM_PHY_BASE + PCIE1_MEM_SIZE - 1)
+
+#define PCIE1_IO_PHY_BASE         0x19800000UL
+#define PCIE1_IO_BASE            (KSEG1 + PCIE1_IO_PHY_BASE)
+#define PCIE1_IO_SIZE            (1 * 1024 * 1024)
+#define PCIE1_IO_PHY_END         (PCIE1_IO_PHY_BASE + PCIE1_IO_SIZE - 1)
+
+#define PCIE1_RC_CFG_BASE        (KSEG1 + 0x19900000)
+#define PCIE1_APP_LOGIC_REG      (KSEG1 + 0x1E100700)
+#define PCIE1_MSI_PHY_BASE        0x1F400000UL
+
+#define PCIE1_PDI_PHY_BASE        0x1F700400UL
+#define PCIE1_PDI_BASE           (KSEG1 + PCIE1_PDI_PHY_BASE)
+#define PCIE1_PDI_SIZE            0x400
+
+#define PCIE_CFG_PORT_TO_BASE(X)     ((X) > 0 ? (PCIE1_CFG_BASE) : (PCIE_CFG_BASE))
+#define PCIE_MEM_PORT_TO_BASE(X)     ((X) > 0 ? (PCIE1_MEM_BASE) : (PCIE_MEM_BASE))
+#define PCIE_IO_PORT_TO_BASE(X)      ((X) > 0 ? (PCIE1_IO_BASE) : (PCIE_IO_BASE))
+#define PCIE_MEM_PHY_PORT_TO_BASE(X) ((X) > 0 ? (PCIE1_MEM_PHY_BASE) : (PCIE_MEM_PHY_BASE))
+#define PCIE_MEM_PHY_PORT_TO_END(X)  ((X) > 0 ? (PCIE1_MEM_PHY_END) : (PCIE_MEM_PHY_END))
+#define PCIE_IO_PHY_PORT_TO_BASE(X)  ((X) > 0 ? (PCIE1_IO_PHY_BASE) : (PCIE_IO_PHY_BASE))
+#define PCIE_IO_PHY_PORT_TO_END(X)   ((X) > 0 ? (PCIE1_IO_PHY_END) : (PCIE_IO_PHY_END))
+#define PCIE_APP_PORT_TO_BASE(X)     ((X) > 0 ? (PCIE1_APP_LOGIC_REG) : (PCIE_APP_LOGIC_REG))
+#define PCIE_RC_PORT_TO_BASE(X)      ((X) > 0 ? (PCIE1_RC_CFG_BASE) : (PCIE_RC_CFG_BASE))
+#define PCIE_PHY_PORT_TO_BASE(X)     ((X) > 0 ? (PCIE1_PDI_BASE) : (PCIE_PDI_BASE))
+
+/* PCIe Application Logic Register */
+/* RC Core Control Register */
+#define PCIE_RC_CCR(X)                      (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x10)
+/* This should be enabled after initializing configuratin registers
+ * Also should check link status retraining bit
+ */
+#define PCIE_RC_CCR_LTSSM_ENABLE             0x00000001    /* Enable LTSSM to continue link establishment */
+
+/* RC Core Debug Register */
+#define PCIE_RC_DR(X)                       (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x14)
+#define PCIE_RC_DR_DLL_UP                    0x00000001  /* Data Link Layer Up */
+#define PCIE_RC_DR_CURRENT_POWER_STATE       0x0000000E  /* Current Power State */
+#define PCIE_RC_DR_CURRENT_POWER_STATE_S     1
+#define PCIE_RC_DR_CURRENT_LTSSM_STATE       0x000001F0  /* Current LTSSM State */
+#define PCIE_RC_DR_CURRENT_LTSSM_STATE_S     4
+
+#define PCIE_RC_DR_PM_DEV_STATE              0x00000E00  /* Power Management D-State */
+#define PCIE_RC_DR_PM_DEV_STATE_S            9
+
+#define PCIE_RC_DR_PM_ENABLED                0x00001000  /* Power Management State from PMU */
+#define PCIE_RC_DR_PME_EVENT_ENABLED         0x00002000  /* Power Management Event Enable State */
+#define PCIE_RC_DR_AUX_POWER_ENABLED         0x00004000  /* Auxiliary Power Enable */
+
+/* Current Power State Definition */
+enum {
+    PCIE_RC_DR_D0 = 0,
+    PCIE_RC_DR_D1,   /* Not supported */
+    PCIE_RC_DR_D2,   /* Not supported */
+    PCIE_RC_DR_D3,
+    PCIE_RC_DR_UN,
+};
+
+/* PHY Link Status Register */
+#define PCIE_PHY_SR(X)                      (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x18)
+#define PCIE_PHY_SR_PHY_LINK_UP              0x00000001   /* PHY Link Up/Down Indicator */
+
+/* Electromechanical Control Register */
+#define PCIE_EM_CR(X)                       (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x1C)
+#define PCIE_EM_CR_CARD_IS_PRESENT           0x00000001  /* Card Presence Detect State */
+#define PCIE_EM_CR_MRL_OPEN                  0x00000002  /* MRL Sensor State */
+#define PCIE_EM_CR_POWER_FAULT_SET           0x00000004  /* Power Fault Detected */
+#define PCIE_EM_CR_MRL_SENSOR_SET            0x00000008  /* MRL Sensor Changed */
+#define PCIE_EM_CR_PRESENT_DETECT_SET        0x00000010  /* Card Presense Detect Changed */
+#define PCIE_EM_CR_CMD_CPL_INT_SET           0x00000020  /* Command Complete Interrupt */
+#define PCIE_EM_CR_SYS_INTERLOCK_SET         0x00000040  /* System Electromechanical IterLock Engaged */
+#define PCIE_EM_CR_ATTENTION_BUTTON_SET      0x00000080  /* Attention Button Pressed */
+
+/* Interrupt Status Register */
+#define PCIE_IR_SR(X)                       (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x20)
+#define PCIE_IR_SR_PME_CAUSE_MSI             0x00000002  /* MSI caused by PME */
+#define PCIE_IR_SR_HP_PME_WAKE_GEN           0x00000004  /* Hotplug PME Wake Generation */
+#define PCIE_IR_SR_HP_MSI                    0x00000008  /* Hotplug MSI */
+#define PCIE_IR_SR_AHB_LU_ERR                0x00000030  /* AHB Bridge Lookup Error Signals */
+#define PCIE_IR_SR_AHB_LU_ERR_S              4
+#define PCIE_IR_SR_INT_MSG_NUM               0x00003E00  /* Interrupt Message Number */
+#define PCIE_IR_SR_INT_MSG_NUM_S             9
+#define PCIE_IR_SR_AER_INT_MSG_NUM           0xF8000000  /* Advanced Error Interrupt Message Number */
+#define PCIE_IR_SR_AER_INT_MSG_NUM_S         27
+
+/* Message Control Register */
+#define PCIE_MSG_CR(X)                      (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x30)
+#define PCIE_MSG_CR_GEN_PME_TURN_OFF_MSG     0x00000001  /* Generate PME Turn Off Message */
+#define PCIE_MSG_CR_GEN_UNLOCK_MSG           0x00000002  /* Generate Unlock Message */
+
+#define PCIE_VDM_DR(X)                      (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x34)
+
+/* Vendor-Defined Message Requester ID Register */
+#define PCIE_VDM_RID(X)                     (PCIE_APP_PORT_TO_BASE (X) + 0x38)
+#define PCIE_VDM_RID_VENROR_MSG_REQ_ID       0x0000FFFF
+#define PCIE_VDM_RID_VDMRID_S                0
+
+/* ASPM Control Register */
+#define PCIE_ASPM_CR(X)                     (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x40)
+#define PCIE_ASPM_CR_HOT_RST                 0x00000001  /* Hot Reset Request to the downstream device */
+#define PCIE_ASPM_CR_REQ_EXIT_L1             0x00000002  /* Request to Exit L1 */
+#define PCIE_ASPM_CR_REQ_ENTER_L1            0x00000004  /* Request to Enter L1 */
+
+/* Vendor Message DW0 Register */
+#define PCIE_VM_MSG_DW0(X)                  (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x50)
+#define PCIE_VM_MSG_DW0_TYPE                 0x0000001F  /* Message type */
+#define PCIE_VM_MSG_DW0_TYPE_S               0
+#define PCIE_VM_MSG_DW0_FORMAT               0x00000060  /* Format */
+#define PCIE_VM_MSG_DW0_FORMAT_S             5
+#define PCIE_VM_MSG_DW0_TC                   0x00007000  /* Traffic Class */
+#define PCIE_VM_MSG_DW0_TC_S                 12
+#define PCIE_VM_MSG_DW0_ATTR                 0x000C0000  /* Atrributes */
+#define PCIE_VM_MSG_DW0_ATTR_S               18
+#define PCIE_VM_MSG_DW0_EP_TLP               0x00100000  /* Poisoned TLP */
+#define PCIE_VM_MSG_DW0_TD                   0x00200000  /* TLP Digest */
+#define PCIE_VM_MSG_DW0_LEN                  0xFFC00000  /* Length */
+#define PCIE_VM_MSG_DW0_LEN_S                22
+
+/* Format Definition */
+enum {
+    PCIE_VM_MSG_FORMAT_00 = 0,  /* 3DW Hdr, no data*/
+    PCIE_VM_MSG_FORMAT_01,      /* 4DW Hdr, no data */
+    PCIE_VM_MSG_FORMAT_10,      /* 3DW Hdr, with data */
+    PCIE_VM_MSG_FORMAT_11,      /* 4DW Hdr, with data */
+};
+
+/* Traffic Class Definition */
+enum {
+    PCIE_VM_MSG_TC0 = 0,
+    PCIE_VM_MSG_TC1,
+    PCIE_VM_MSG_TC2,
+    PCIE_VM_MSG_TC3,
+    PCIE_VM_MSG_TC4,
+    PCIE_VM_MSG_TC5,
+    PCIE_VM_MSG_TC6,
+    PCIE_VM_MSG_TC7,
+};
+
+/* Attributes Definition */
+enum {
+    PCIE_VM_MSG_ATTR_00 = 0,   /* RO and No Snoop cleared */
+    PCIE_VM_MSG_ATTR_01,       /* RO cleared , No Snoop set */
+    PCIE_VM_MSG_ATTR_10,       /* RO set, No Snoop cleared*/
+    PCIE_VM_MSG_ATTR_11,       /* RO and No Snoop set */
+};
+
+/* Payload Size Definition */
+#define PCIE_VM_MSG_LEN_MIN  0
+#define PCIE_VM_MSG_LEN_MAX  1024
+
+/* Vendor Message DW1 Register */
+#define PCIE_VM_MSG_DW1(X)                 (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x54)
+#define PCIE_VM_MSG_DW1_FUNC_NUM            0x00000070  /* Function Number */
+#define PCIE_VM_MSG_DW1_FUNC_NUM_S          8
+#define PCIE_VM_MSG_DW1_CODE                0x00FF0000  /* Message Code */
+#define PCIE_VM_MSG_DW1_CODE_S              16
+#define PCIE_VM_MSG_DW1_TAG                 0xFF000000  /* Tag */
+#define PCIE_VM_MSG_DW1_TAG_S               24
+
+#define PCIE_VM_MSG_DW2(X)                  (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x58)
+#define PCIE_VM_MSG_DW3(X)                  (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x5C)
+
+/* Vendor Message Request Register */
+#define PCIE_VM_MSG_REQR(X)                 (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x60)
+#define PCIE_VM_MSG_REQR_REQ                 0x00000001  /* Vendor Message Request */
+
+
+/* AHB Slave Side Band Control Register */
+#define PCIE_AHB_SSB(X)                     (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x70)
+#define PCIE_AHB_SSB_REQ_BCM                0x00000001 /* Slave Reques BCM filed */
+#define PCIE_AHB_SSB_REQ_EP                 0x00000002 /* Slave Reques EP filed */
+#define PCIE_AHB_SSB_REQ_TD                 0x00000004 /* Slave Reques TD filed */
+#define PCIE_AHB_SSB_REQ_ATTR               0x00000018 /* Slave Reques Attribute number */
+#define PCIE_AHB_SSB_REQ_ATTR_S             3
+#define PCIE_AHB_SSB_REQ_TC                 0x000000E0 /* Slave Request TC Field */
+#define PCIE_AHB_SSB_REQ_TC_S               5
+
+/* AHB Master SideBand Ctrl Register */
+#define PCIE_AHB_MSB(X)                     (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x74)
+#define PCIE_AHB_MSB_RESP_ATTR               0x00000003 /* Master Response Attribute number */
+#define PCIE_AHB_MSB_RESP_ATTR_S             0
+#define PCIE_AHB_MSB_RESP_BAD_EOT            0x00000004 /* Master Response Badeot filed */
+#define PCIE_AHB_MSB_RESP_BCM                0x00000008 /* Master Response BCM filed */
+#define PCIE_AHB_MSB_RESP_EP                 0x00000010 /* Master Response EP filed */
+#define PCIE_AHB_MSB_RESP_TD                 0x00000020 /* Master Response TD filed */
+#define PCIE_AHB_MSB_RESP_FUN_NUM            0x000003C0 /* Master Response Function number */
+#define PCIE_AHB_MSB_RESP_FUN_NUM_S          6
+
+/* AHB Control Register, fixed bus enumeration exception */
+#define PCIE_AHB_CTRL(X)                     (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x78)
+#define PCIE_AHB_CTRL_BUS_ERROR_SUPPRESS     0x00000001 
+
+/* Interrupt Enalbe Register */
+#define PCIE_IRNEN(X)                        (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0xF4)
+#define PCIE_IRNCR(X)                        (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0xF8)
+#define PCIE_IRNICR(X)                       (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0xFC)
+
+/* PCIe interrupt enable/control/capture register definition */
+#define PCIE_IRN_AER_REPORT                 0x00000001  /* AER Interrupt */
+#define PCIE_IRN_AER_MSIX                   0x00000002  /* Advanced Error MSI-X Interrupt */
+#define PCIE_IRN_PME                        0x00000004  /* PME Interrupt */
+#define PCIE_IRN_HOTPLUG                    0x00000008  /* Hotplug Interrupt */
+#define PCIE_IRN_RX_VDM_MSG                 0x00000010  /* Vendor-Defined Message Interrupt */
+#define PCIE_IRN_RX_CORRECTABLE_ERR_MSG     0x00000020  /* Correctable Error Message Interrupt */
+#define PCIE_IRN_RX_NON_FATAL_ERR_MSG       0x00000040  /* Non-fatal Error Message */
+#define PCIE_IRN_RX_FATAL_ERR_MSG           0x00000080  /* Fatal Error Message */
+#define PCIE_IRN_RX_PME_MSG                 0x00000100  /* PME Message Interrupt */
+#define PCIE_IRN_RX_PME_TURNOFF_ACK         0x00000200  /* PME Turnoff Ack Message Interrupt */
+#define PCIE_IRN_AHB_BR_FATAL_ERR           0x00000400  /* AHB Fatal Error Interrupt */
+#define PCIE_IRN_LINK_AUTO_BW_STATUS        0x00000800  /* Link Auto Bandwidth Status Interrupt */
+#define PCIE_IRN_BW_MGT                     0x00001000  /* Bandwidth Managment Interrupt */
+#define PCIE_IRN_INTA                       0x00002000  /* INTA */
+#define PCIE_IRN_INTB                       0x00004000  /* INTB */
+#define PCIE_IRN_INTC                       0x00008000  /* INTC */
+#define PCIE_IRN_INTD                       0x00010000  /* INTD */
+#define PCIE_IRN_WAKEUP                     0x00020000  /* Wake up Interrupt */
+
+#define PCIE_RC_CORE_COMBINED_INT    (PCIE_IRN_AER_REPORT |  PCIE_IRN_AER_MSIX | PCIE_IRN_PME | \
+                                      PCIE_IRN_HOTPLUG | PCIE_IRN_RX_VDM_MSG | PCIE_IRN_RX_CORRECTABLE_ERR_MSG |\
+                                      PCIE_IRN_RX_NON_FATAL_ERR_MSG | PCIE_IRN_RX_FATAL_ERR_MSG | \
+                                      PCIE_IRN_RX_PME_MSG | PCIE_IRN_RX_PME_TURNOFF_ACK | PCIE_IRN_AHB_BR_FATAL_ERR | \
+                                      PCIE_IRN_LINK_AUTO_BW_STATUS | PCIE_IRN_BW_MGT)
+/* PCIe RC Configuration Register */
+#define PCIE_VDID(X)                (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x00)
+
+/* Bit definition from pci_reg.h */
+#define PCIE_PCICMDSTS(X)           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x04)
+#define PCIE_CCRID(X)               (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x08)
+#define PCIE_CLSLTHTBR(X)           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x0C) /* EP only */
+/* BAR0, BAR1,Only necessary if the bridges implements a device-specific register set or memory buffer */
+#define PCIE_BAR0(X)                (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x10) /* Not used*/
+#define PCIE_BAR1(X)                (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x14) /* Not used */
+
+#define PCIE_BNR(X)                 (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x18) /* Mandatory */
+/* Bus Number Register bits */
+#define PCIE_BNR_PRIMARY_BUS_NUM             0x000000FF
+#define PCIE_BNR_PRIMARY_BUS_NUM_S           0
+#define PCIE_PNR_SECONDARY_BUS_NUM           0x0000FF00
+#define PCIE_PNR_SECONDARY_BUS_NUM_S         8
+#define PCIE_PNR_SUB_BUS_NUM                 0x00FF0000
+#define PCIE_PNR_SUB_BUS_NUM_S               16
+
+/* IO Base/Limit Register bits */
+#define PCIE_IOBLSECS(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x1C)  /* RC only */
+#define PCIE_IOBLSECS_32BIT_IO_ADDR             0x00000001
+#define PCIE_IOBLSECS_IO_BASE_ADDR              0x000000F0
+#define PCIE_IOBLSECS_IO_BASE_ADDR_S            4
+#define PCIE_IOBLSECS_32BIT_IOLIMT              0x00000100
+#define PCIE_IOBLSECS_IO_LIMIT_ADDR             0x0000F000
+#define PCIE_IOBLSECS_IO_LIMIT_ADDR_S           12
+
+/* Non-prefetchable Memory Base/Limit Register bit */
+#define PCIE_MBML(X)                           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x20)  /* RC only */
+#define PCIE_MBML_MEM_BASE_ADDR                 0x0000FFF0
+#define PCIE_MBML_MEM_BASE_ADDR_S               4
+#define PCIE_MBML_MEM_LIMIT_ADDR                0xFFF00000
+#define PCIE_MBML_MEM_LIMIT_ADDR_S              20
+
+/* Prefetchable Memory Base/Limit Register bit */
+#define PCIE_PMBL(X)                           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x24)  /* RC only */
+#define PCIE_PMBL_64BIT_ADDR                    0x00000001
+#define PCIE_PMBL_UPPER_12BIT                   0x0000FFF0
+#define PCIE_PMBL_UPPER_12BIT_S                 4
+#define PCIE_PMBL_E64MA                         0x00010000
+#define PCIE_PMBL_END_ADDR                      0xFFF00000
+#define PCIE_PMBL_END_ADDR_S                    20
+#define PCIE_PMBU32(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x28)  /* RC only */
+#define PCIE_PMLU32(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x2C)  /* RC only */
+
+/* I/O Base/Limit Upper 16 bits register */
+#define PCIE_IO_BANDL(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x30)  /* RC only */
+#define PCIE_IO_BANDL_UPPER_16BIT_IO_BASE        0x0000FFFF
+#define PCIE_IO_BANDL_UPPER_16BIT_IO_BASE_S      0
+#define PCIE_IO_BANDL_UPPER_16BIT_IO_LIMIT       0xFFFF0000
+#define PCIE_IO_BANDL_UPPER_16BIT_IO_LIMIT_S     16
+
+#define PCIE_CPR(X)                            (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x34)
+#define PCIE_EBBAR(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x38)
+
+/* Interrupt and Secondary Bridge Control Register */
+#define PCIE_INTRBCTRL(X)                      (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x3C)
+
+#define PCIE_INTRBCTRL_INT_LINE                 0x000000FF
+#define PCIE_INTRBCTRL_INT_LINE_S               0
+#define PCIE_INTRBCTRL_INT_PIN                  0x0000FF00
+#define PCIE_INTRBCTRL_INT_PIN_S                8
+#define PCIE_INTRBCTRL_PARITY_ERR_RESP_ENABLE   0x00010000    /* #PERR */
+#define PCIE_INTRBCTRL_SERR_ENABLE              0x00020000    /* #SERR */
+#define PCIE_INTRBCTRL_ISA_ENABLE               0x00040000    /* ISA enable, IO 64KB only */
+#define PCIE_INTRBCTRL_VGA_ENABLE               0x00080000    /* VGA enable */
+#define PCIE_INTRBCTRL_VGA_16BIT_DECODE         0x00100000    /* VGA 16bit decode */
+#define PCIE_INTRBCTRL_RST_SECONDARY_BUS        0x00400000    /* Secondary bus rest, hot rest, 1ms */
+/* Others are read only */
+enum {
+    PCIE_INTRBCTRL_INT_NON = 0,
+    PCIE_INTRBCTRL_INTA,
+    PCIE_INTRBCTRL_INTB,
+    PCIE_INTRBCTRL_INTC,
+    PCIE_INTRBCTRL_INTD,
+};
+
+#define PCIE_PM_CAPR(X)                  (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x40)
+
+/* Power Management Control and Status Register */
+#define PCIE_PM_CSR(X)                   (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x44)
+
+#define PCIE_PM_CSR_POWER_STATE           0x00000003   /* Power State */
+#define PCIE_PM_CSR_POWER_STATE_S         0
+#define PCIE_PM_CSR_SW_RST                0x00000008   /* Soft Reset Enabled */
+#define PCIE_PM_CSR_PME_ENABLE            0x00000100   /* PME Enable */
+#define PCIE_PM_CSR_PME_STATUS            0x00008000   /* PME status */
+
+/* MSI Capability Register for EP */
+#define PCIE_MCAPR(X)                    (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x50)
+
+#define PCIE_MCAPR_MSI_CAP_ID             0x000000FF  /* MSI Capability ID */
+#define PCIE_MCAPR_MSI_CAP_ID_S           0
+#define PCIE_MCAPR_MSI_NEXT_CAP_PTR       0x0000FF00  /* Next Capability Pointer */
+#define PCIE_MCAPR_MSI_NEXT_CAP_PTR_S     8
+#define PCIE_MCAPR_MSI_ENABLE             0x00010000  /* MSI Enable */
+#define PCIE_MCAPR_MULTI_MSG_CAP          0x000E0000  /* Multiple Message Capable */
+#define PCIE_MCAPR_MULTI_MSG_CAP_S        17
+#define PCIE_MCAPR_MULTI_MSG_ENABLE       0x00700000  /* Multiple Message Enable */
+#define PCIE_MCAPR_MULTI_MSG_ENABLE_S     20
+#define PCIE_MCAPR_ADDR64_CAP             0X00800000  /* 64-bit Address Capable */
+
+/* MSI Message Address Register */
+#define PCIE_MA(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x54)
+
+#define PCIE_MA_ADDR_MASK                 0xFFFFFFFC  /* Message Address */
+
+/* MSI Message Upper Address Register */
+#define PCIE_MUA(X)                      (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x58)
+
+/* MSI Message Data Register */
+#define PCIE_MD(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x5C)
+
+#define PCIE_MD_DATA                      0x0000FFFF  /* Message Data */
+#define PCIE_MD_DATA_S                    0
+
+/* PCI Express Capability Register */
+#define PCIE_XCAP(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x70)
+
+#define PCIE_XCAP_ID                      0x000000FF  /* PCI Express Capability ID */
+#define PCIE_XCAP_ID_S                    0
+#define PCIE_XCAP_NEXT_CAP                0x0000FF00  /* Next Capability Pointer */
+#define PCIE_XCAP_NEXT_CAP_S              8
+#define PCIE_XCAP_VER                     0x000F0000  /* PCI Express Capability Version */
+#define PCIE_XCAP_VER_S                   16
+#define PCIE_XCAP_DEV_PORT_TYPE           0x00F00000  /* Device Port Type */
+#define PCIE_XCAP_DEV_PORT_TYPE_S         20
+#define PCIE_XCAP_SLOT_IMPLEMENTED        0x01000000  /* Slot Implemented */
+#define PCIE_XCAP_MSG_INT_NUM             0x3E000000  /* Interrupt Message Number */
+#define PCIE_XCAP_MSG_INT_NUM_S           25
+
+/* Device Capability Register */
+#define PCIE_DCAP(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x74)
+
+#define PCIE_DCAP_MAX_PAYLOAD_SIZE        0x00000007   /* Max Payload size */
+#define PCIE_DCAP_MAX_PAYLOAD_SIZE_S      0
+#define PCIE_DCAP_PHANTOM_FUNC            0x00000018   /* Phanton Function, not supported */
+#define PCIE_DCAP_PHANTOM_FUNC_S          3
+#define PCIE_DCAP_EXT_TAG                 0x00000020   /* Extended Tag Field */
+#define PCIE_DCAP_EP_L0S_LATENCY          0x000001C0   /* EP L0s latency only */
+#define PCIE_DCAP_EP_L0S_LATENCY_S        6
+#define PCIE_DCAP_EP_L1_LATENCY           0x00000E00   /* EP L1 latency only */
+#define PCIE_DCAP_EP_L1_LATENCY_S         9
+#define PCIE_DCAP_ROLE_BASE_ERR_REPORT    0x00008000   /* Role Based ERR */
+
+/* Maximum payload size supported */
+enum {
+    PCIE_MAX_PAYLOAD_128 = 0,
+    PCIE_MAX_PAYLOAD_256,
+    PCIE_MAX_PAYLOAD_512,
+    PCIE_MAX_PAYLOAD_1024,
+    PCIE_MAX_PAYLOAD_2048,
+    PCIE_MAX_PAYLOAD_4096,
+};
+
+/* Device Control and Status Register */
+#define PCIE_DCTLSTS(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x78)
+
+#define PCIE_DCTLSTS_CORRECTABLE_ERR_EN        0x00000001   /* COR-ERR */
+#define PCIE_DCTLSTS_NONFATAL_ERR_EN           0x00000002   /* Non-fatal ERR */
+#define PCIE_DCTLSTS_FATAL_ERR_EN              0x00000004   /* Fatal ERR */
+#define PCIE_DCTLSYS_UR_REQ_EN                 0x00000008   /* UR ERR */
+#define PCIE_DCTLSTS_RELAXED_ORDERING_EN       0x00000010   /* Enable relaxing ordering */
+#define PCIE_DCTLSTS_MAX_PAYLOAD_SIZE          0x000000E0   /* Max payload mask */
+#define PCIE_DCTLSTS_MAX_PAYLOAD_SIZE_S        5
+#define PCIE_DCTLSTS_EXT_TAG_EN                0x00000100   /* Extended tag field */
+#define PCIE_DCTLSTS_PHANTOM_FUNC_EN           0x00000200   /* Phantom Function Enable */
+#define PCIE_DCTLSTS_AUX_PM_EN                 0x00000400   /* AUX Power PM Enable */
+#define PCIE_DCTLSTS_NO_SNOOP_EN               0x00000800   /* Enable no snoop, except root port*/
+#define PCIE_DCTLSTS_MAX_READ_SIZE             0x00007000   /* Max Read Request size*/
+#define PCIE_DCTLSTS_MAX_READ_SIZE_S           12
+#define PCIE_DCTLSTS_CORRECTABLE_ERR           0x00010000   /* COR-ERR Detected */
+#define PCIE_DCTLSTS_NONFATAL_ERR              0x00020000   /* Non-Fatal ERR Detected */
+#define PCIE_DCTLSTS_FATAL_ER                  0x00040000   /* Fatal ERR Detected */
+#define PCIE_DCTLSTS_UNSUPPORTED_REQ           0x00080000   /* UR Detected */
+#define PCIE_DCTLSTS_AUX_POWER                 0x00100000   /* Aux Power Detected */
+#define PCIE_DCTLSTS_TRANSACT_PENDING          0x00200000   /* Transaction pending */
+
+#define PCIE_DCTLSTS_ERR_EN      (PCIE_DCTLSTS_CORRECTABLE_ERR_EN | \
+                                  PCIE_DCTLSTS_NONFATAL_ERR_EN | PCIE_DCTLSTS_FATAL_ERR_EN | \
+                                  PCIE_DCTLSYS_UR_REQ_EN)
+
+/* Link Capability Register */
+#define PCIE_LCAP(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x7C)
+#define PCIE_LCAP_MAX_LINK_SPEED               0x0000000F  /* Max link speed, 0x1 by default */
+#define PCIE_LCAP_MAX_LINK_SPEED_S             0
+#define PCIE_LCAP_MAX_LENGTH_WIDTH             0x000003F0  /* Maxium Length Width */
+#define PCIE_LCAP_MAX_LENGTH_WIDTH_S           4
+#define PCIE_LCAP_ASPM_LEVEL                   0x00000C00  /* Active State Link PM Support */
+#define PCIE_LCAP_ASPM_LEVEL_S                 10
+#define PCIE_LCAP_L0S_EIXT_LATENCY             0x00007000  /* L0s Exit Latency */
+#define PCIE_LCAP_L0S_EIXT_LATENCY_S           12
+#define PCIE_LCAP_L1_EXIT_LATENCY              0x00038000  /* L1 Exit Latency */
+#define PCIE_LCAP_L1_EXIT_LATENCY_S            15
+#define PCIE_LCAP_CLK_PM                       0x00040000  /* Clock Power Management */
+#define PCIE_LCAP_SDER                         0x00080000  /* Surprise Down Error Reporting */
+#define PCIE_LCAP_DLL_ACTIVE_REPROT            0x00100000  /* Data Link Layer Active Reporting Capable */
+#define PCIE_LCAP_PORT_NUM                     0xFF0000000  /* Port number */
+#define PCIE_LCAP_PORT_NUM_S                   24
+
+/* Maximum Length width definition */
+#define PCIE_MAX_LENGTH_WIDTH_RES  0x00
+#define PCIE_MAX_LENGTH_WIDTH_X1   0x01  /* Default */
+#define PCIE_MAX_LENGTH_WIDTH_X2   0x02
+#define PCIE_MAX_LENGTH_WIDTH_X4   0x04
+#define PCIE_MAX_LENGTH_WIDTH_X8   0x08
+#define PCIE_MAX_LENGTH_WIDTH_X12  0x0C
+#define PCIE_MAX_LENGTH_WIDTH_X16  0x10
+#define PCIE_MAX_LENGTH_WIDTH_X32  0x20
+
+/* Active State Link PM definition */
+enum {
+    PCIE_ASPM_RES0                = 0,
+    PCIE_ASPM_L0S_ENTRY_SUPPORT,        /* L0s */
+    PCIE_ASPM_RES1,
+    PCIE_ASPM_L0S_L1_ENTRY_SUPPORT,     /* L0s and L1, default */
+};
+
+/* L0s Exit Latency definition */
+enum {
+    PCIE_L0S_EIXT_LATENCY_L64NS    = 0, /* < 64 ns */
+    PCIE_L0S_EIXT_LATENCY_B64A128,      /* > 64 ns < 128 ns */
+    PCIE_L0S_EIXT_LATENCY_B128A256,     /* > 128 ns < 256 ns */
+    PCIE_L0S_EIXT_LATENCY_B256A512,     /* > 256 ns < 512 ns */
+    PCIE_L0S_EIXT_LATENCY_B512TO1U,     /* > 512 ns < 1 us */
+    PCIE_L0S_EIXT_LATENCY_B1A2U,        /* > 1 us < 2 us */
+    PCIE_L0S_EIXT_LATENCY_B2A4U,        /* > 2 us < 4 us */
+    PCIE_L0S_EIXT_LATENCY_M4US,         /* > 4 us  */
+};
+
+/* L1 Exit Latency definition */
+enum {
+    PCIE_L1_EXIT_LATENCY_L1US  = 0,  /* < 1 us */
+    PCIE_L1_EXIT_LATENCY_B1A2,       /* > 1 us < 2 us */
+    PCIE_L1_EXIT_LATENCY_B2A4,       /* > 2 us < 4 us */
+    PCIE_L1_EXIT_LATENCY_B4A8,       /* > 4 us < 8 us */
+    PCIE_L1_EXIT_LATENCY_B8A16,      /* > 8 us < 16 us */
+    PCIE_L1_EXIT_LATENCY_B16A32,     /* > 16 us < 32 us */
+    PCIE_L1_EXIT_LATENCY_B32A64,     /* > 32 us < 64 us */
+    PCIE_L1_EXIT_LATENCY_M64US,      /* > 64 us */
+};
+
+/* Link Control and Status Register */
+#define PCIE_LCTLSTS(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x80)
+#define PCIE_LCTLSTS_ASPM_ENABLE            0x00000003  /* Active State Link PM Control */
+#define PCIE_LCTLSTS_ASPM_ENABLE_S          0
+#define PCIE_LCTLSTS_RCB128                 0x00000008  /* Read Completion Boundary 128*/
+#define PCIE_LCTLSTS_LINK_DISABLE           0x00000010  /* Link Disable */
+#define PCIE_LCTLSTS_RETRIAN_LINK           0x00000020  /* Retrain Link */
+#define PCIE_LCTLSTS_COM_CLK_CFG            0x00000040  /* Common Clock Configuration */
+#define PCIE_LCTLSTS_EXT_SYNC               0x00000080  /* Extended Synch */
+#define PCIE_LCTLSTS_CLK_PM_EN              0x00000100  /* Enable Clock Powerm Management */
+#define PCIE_LCTLSTS_LINK_SPEED             0x000F0000  /* Link Speed */
+#define PCIE_LCTLSTS_LINK_SPEED_S           16
+#define PCIE_LCTLSTS_NEGOTIATED_LINK_WIDTH  0x03F00000  /* Negotiated Link Width */
+#define PCIE_LCTLSTS_NEGOTIATED_LINK_WIDTH_S 20
+#define PCIE_LCTLSTS_RETRAIN_PENDING        0x08000000  /* Link training is ongoing */
+#define PCIE_LCTLSTS_SLOT_CLK_CFG           0x10000000  /* Slot Clock Configuration */
+#define PCIE_LCTLSTS_DLL_ACTIVE             0x20000000  /* Data Link Layer Active */
+
+/* Slot Capabilities Register */
+#define PCIE_SLCAP(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x84)
+
+/* Slot Capabilities */
+#define PCIE_SLCTLSTS(X)                    (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x88)
+
+/* Root Control and Capability Register */
+#define PCIE_RCTLCAP(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x8C)
+#define PCIE_RCTLCAP_SERR_ON_CORRECTABLE_ERR  0x00000001   /* #SERR on COR-ERR */
+#define PCIE_RCTLCAP_SERR_ON_NONFATAL_ERR     0x00000002   /* #SERR on Non-Fatal ERR */
+#define PCIE_RCTLCAP_SERR_ON_FATAL_ERR        0x00000004   /* #SERR on Fatal ERR */
+#define PCIE_RCTLCAP_PME_INT_EN               0x00000008   /* PME Interrupt Enable */
+#define PCIE_RCTLCAP_SERR_ENABLE    (PCIE_RCTLCAP_SERR_ON_CORRECTABLE_ERR | \
+                                     PCIE_RCTLCAP_SERR_ON_NONFATAL_ERR | PCIE_RCTLCAP_SERR_ON_FATAL_ERR)
+/* Root Status Register */
+#define PCIE_RSTS(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x90)
+#define PCIE_RSTS_PME_REQ_ID                   0x0000FFFF   /* PME Request ID */
+#define PCIE_RSTS_PME_REQ_ID_S                 0
+#define PCIE_RSTS_PME_STATUS                   0x00010000   /* PME Status */
+#define PCIE_RSTS_PME_PENDING                  0x00020000   /* PME Pending */
+
+/* PCI Express Enhanced Capability Header */
+#define PCIE_ENHANCED_CAP(X)                (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x100)
+#define PCIE_ENHANCED_CAP_ID                 0x0000FFFF  /* PCI Express Extended Capability ID */
+#define PCIE_ENHANCED_CAP_ID_S               0
+#define PCIE_ENHANCED_CAP_VER                0x000F0000  /* Capability Version */
+#define PCIE_ENHANCED_CAP_VER_S              16
+#define PCIE_ENHANCED_CAP_NEXT_OFFSET        0xFFF00000  /* Next Capability Offset */
+#define PCIE_ENHANCED_CAP_NEXT_OFFSET_S      20
+
+/* Uncorrectable Error Status Register */
+#define PCIE_UES_R(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x104)
+#define PCIE_DATA_LINK_PROTOCOL_ERR          0x00000010  /* Data Link Protocol Error Status */
+#define PCIE_SURPRISE_DOWN_ERROR             0x00000020  /* Surprise Down Error Status */
+#define PCIE_POISONED_TLP                    0x00001000  /* Poisoned TLP Status */
+#define PCIE_FC_PROTOCOL_ERR                 0x00002000  /* Flow Control Protocol Error Status */
+#define PCIE_COMPLETION_TIMEOUT              0x00004000  /* Completion Timeout Status */
+#define PCIE_COMPLETOR_ABORT                 0x00008000  /* Completer Abort Error */
+#define PCIE_UNEXPECTED_COMPLETION           0x00010000  /* Unexpected Completion Status */
+#define PCIE_RECEIVER_OVERFLOW               0x00020000  /* Receive Overflow Status */
+#define PCIE_MALFORNED_TLP                   0x00040000  /* Malformed TLP Stauts */
+#define PCIE_ECRC_ERR                        0x00080000  /* ECRC Error Stauts */
+#define PCIE_UR_REQ                          0x00100000  /* Unsupported Request Error Status */
+#define PCIE_ALL_UNCORRECTABLE_ERR    (PCIE_DATA_LINK_PROTOCOL_ERR | PCIE_SURPRISE_DOWN_ERROR | \
+                         PCIE_POISONED_TLP | PCIE_FC_PROTOCOL_ERR | PCIE_COMPLETION_TIMEOUT |   \
+                         PCIE_COMPLETOR_ABORT | PCIE_UNEXPECTED_COMPLETION | PCIE_RECEIVER_OVERFLOW |\
+                         PCIE_MALFORNED_TLP | PCIE_ECRC_ERR | PCIE_UR_REQ)
+
+/* Uncorrectable Error Mask Register, Mask means no report */
+#define PCIE_UEMR(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x108)
+
+/* Uncorrectable Error Severity Register */
+#define PCIE_UESR(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x10C)
+
+/* Correctable Error Status Register */
+#define PCIE_CESR(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x110)
+#define PCIE_RX_ERR                          0x00000001  /* Receive Error Status */
+#define PCIE_BAD_TLP                         0x00000040  /* Bad TLP Status */
+#define PCIE_BAD_DLLP                        0x00000080  /* Bad DLLP Status */
+#define PCIE_REPLAY_NUM_ROLLOVER             0x00000100  /* Replay Number Rollover Status */
+#define PCIE_REPLAY_TIMER_TIMEOUT_ERR        0x00001000  /* Reply Timer Timeout Status */
+#define PCIE_ADVISORY_NONFTAL_ERR            0x00002000  /* Advisory Non-Fatal Error Status */
+#define PCIE_CORRECTABLE_ERR        (PCIE_RX_ERR | PCIE_BAD_TLP | PCIE_BAD_DLLP | PCIE_REPLAY_NUM_ROLLOVER |\
+                                     PCIE_REPLAY_TIMER_TIMEOUT_ERR | PCIE_ADVISORY_NONFTAL_ERR)
+
+/* Correctable Error Mask Register */
+#define PCIE_CEMR(X)                        (volatile u32*)(PCIE_RC_CFG_BASE + 0x114)
+
+/* Advanced Error Capabilities and Control Register */
+#define PCIE_AECCR(X)                       (volatile u32*)(PCIE_RC_CFG_BASE + 0x118)
+#define PCIE_AECCR_FIRST_ERR_PTR            0x0000001F  /* First Error Pointer */
+#define PCIE_AECCR_FIRST_ERR_PTR_S          0
+#define PCIE_AECCR_ECRC_GEN_CAP             0x00000020  /* ECRC Generation Capable */
+#define PCIE_AECCR_ECRC_GEN_EN              0x00000040  /* ECRC Generation Enable */
+#define PCIE_AECCR_ECRC_CHECK_CAP           0x00000080  /* ECRC Check Capable */
+#define PCIE_AECCR_ECRC_CHECK_EN            0x00000100  /* ECRC Check Enable */
+
+/* Header Log Register 1 */
+#define PCIE_HLR1(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x11C)
+
+/* Header Log Register 2 */
+#define PCIE_HLR2(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x120)
+
+/* Header Log Register 3 */
+#define PCIE_HLR3(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x124)
+
+/* Header Log Register 4 */
+#define PCIE_HLR4(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x128)
+
+/* Root Error Command Register */
+#define PCIE_RECR(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x12C)
+#define PCIE_RECR_CORRECTABLE_ERR_REPORT_EN  0x00000001 /* COR-ERR */
+#define PCIE_RECR_NONFATAL_ERR_REPORT_EN     0x00000002 /* Non-Fatal ERR */
+#define PCIE_RECR_FATAL_ERR_REPORT_EN        0x00000004 /* Fatal ERR */
+#define PCIE_RECR_ERR_REPORT_EN  (PCIE_RECR_CORRECTABLE_ERR_REPORT_EN | \
+                PCIE_RECR_NONFATAL_ERR_REPORT_EN | PCIE_RECR_FATAL_ERR_REPORT_EN)
+
+/* Root Error Status Register */
+#define PCIE_RESR(X)                            (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x130)
+#define PCIE_RESR_CORRECTABLE_ERR                0x00000001   /* COR-ERR Receveid */
+#define PCIE_RESR_MULTI_CORRECTABLE_ERR          0x00000002   /* Multiple COR-ERR Received */
+#define PCIE_RESR_FATAL_NOFATAL_ERR              0x00000004   /* ERR Fatal/Non-Fatal Received */
+#define PCIE_RESR_MULTI_FATAL_NOFATAL_ERR        0x00000008   /* Multiple ERR Fatal/Non-Fatal Received */
+#define PCIE_RESR_FIRST_UNCORRECTABLE_FATAL_ERR  0x00000010   /* First UN-COR Fatal */
+#define PCIR_RESR_NON_FATAL_ERR                  0x00000020   /* Non-Fatal Error Message Received */
+#define PCIE_RESR_FATAL_ERR                      0x00000040   /* Fatal Message Received */
+#define PCIE_RESR_AER_INT_MSG_NUM                0xF8000000   /* Advanced Error Interrupt Message Number */
+#define PCIE_RESR_AER_INT_MSG_NUM_S              27
+
+/* Error Source Indentification Register */
+#define PCIE_ESIR(X)                            (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x134)
+#define PCIE_ESIR_CORRECTABLE_ERR_SRC_ID         0x0000FFFF
+#define PCIE_ESIR_CORRECTABLE_ERR_SRC_ID_S       0
+#define PCIE_ESIR_FATAL_NON_FATAL_SRC_ID         0xFFFF0000
+#define PCIE_ESIR_FATAL_NON_FATAL_SRC_ID_S       16
+
+/* VC Enhanced Capability Header */
+#define PCIE_VC_ECH(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x140)
+
+/* Port VC Capability Register */
+#define PCIE_PVC1(X)                            (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x144)
+#define PCIE_PVC1_EXT_VC_CNT                    0x00000007  /* Extended VC Count */
+#define PCIE_PVC1_EXT_VC_CNT_S                  0
+#define PCIE_PVC1_LOW_PRI_EXT_VC_CNT            0x00000070  /* Low Priority Extended VC Count */
+#define PCIE_PVC1_LOW_PRI_EXT_VC_CNT_S          4
+#define PCIE_PVC1_REF_CLK                       0x00000300  /* Reference Clock */
+#define PCIE_PVC1_REF_CLK_S                     8
+#define PCIE_PVC1_PORT_ARB_TAB_ENTRY_SIZE       0x00000C00  /* Port Arbitration Table Entry Size */
+#define PCIE_PVC1_PORT_ARB_TAB_ENTRY_SIZE_S     10
+
+/* Extended Virtual Channel Count Defintion */
+#define PCIE_EXT_VC_CNT_MIN   0
+#define PCIE_EXT_VC_CNT_MAX   7
+
+/* Port Arbitration Table Entry Size Definition */
+enum {
+    PCIE_PORT_ARB_TAB_ENTRY_SIZE_S1BIT = 0,
+    PCIE_PORT_ARB_TAB_ENTRY_SIZE_S2BIT,
+    PCIE_PORT_ARB_TAB_ENTRY_SIZE_S4BIT,
+    PCIE_PORT_ARB_TAB_ENTRY_SIZE_S8BIT,
+};
+
+/* Port VC Capability Register 2 */
+#define PCIE_PVC2(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x148)
+#define PCIE_PVC2_VC_ARB_16P_FIXED_WRR      0x00000001  /* HW Fixed arbitration, 16 phase WRR */
+#define PCIE_PVC2_VC_ARB_32P_WRR            0x00000002  /* 32 phase WRR */
+#define PCIE_PVC2_VC_ARB_64P_WRR            0x00000004  /* 64 phase WRR */
+#define PCIE_PVC2_VC_ARB_128P_WRR           0x00000008  /* 128 phase WRR */
+#define PCIE_PVC2_VC_ARB_WRR                0x0000000F
+#define PCIE_PVC2_VC_ARB_TAB_OFFSET         0xFF000000  /* VC arbitration table offset, not support */
+#define PCIE_PVC2_VC_ARB_TAB_OFFSET_S       24
+
+/* Port VC Control and Status Register */     
+#define PCIE_PVCCRSR(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x14C)
+#define PCIE_PVCCRSR_LOAD_VC_ARB_TAB         0x00000001  /* Load VC Arbitration Table */
+#define PCIE_PVCCRSR_VC_ARB_SEL              0x0000000E  /* VC Arbitration Select */
+#define PCIE_PVCCRSR_VC_ARB_SEL_S            1
+#define PCIE_PVCCRSR_VC_ARB_TAB_STATUS       0x00010000  /* Arbitration Status */
+
+/* VC0 Resource Capability Register */
+#define PCIE_VC0_RC(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x150)
+#define PCIE_VC0_RC_PORT_ARB_HW_FIXED        0x00000001  /* HW Fixed arbitration */
+#define PCIE_VC0_RC_PORT_ARB_32P_WRR         0x00000002  /* 32 phase WRR */
+#define PCIE_VC0_RC_PORT_ARB_64P_WRR         0x00000004  /* 64 phase WRR */
+#define PCIE_VC0_RC_PORT_ARB_128P_WRR        0x00000008  /* 128 phase WRR */
+#define PCIE_VC0_RC_PORT_ARB_TM_128P_WRR     0x00000010  /* Time-based 128 phase WRR */
+#define PCIE_VC0_RC_PORT_ARB_TM_256P_WRR     0x00000020  /* Time-based 256 phase WRR */
+#define PCIE_VC0_RC_PORT_ARB          (PCIE_VC0_RC_PORT_ARB_HW_FIXED | PCIE_VC0_RC_PORT_ARB_32P_WRR |\
+                        PCIE_VC0_RC_PORT_ARB_64P_WRR | PCIE_VC0_RC_PORT_ARB_128P_WRR | \
+                        PCIE_VC0_RC_PORT_ARB_TM_128P_WRR | PCIE_VC0_RC_PORT_ARB_TM_256P_WRR)
+
+#define PCIE_VC0_RC_REJECT_SNOOP             0x00008000  /* Reject Snoop Transactioin */
+#define PCIE_VC0_RC_MAX_TIMESLOTS            0x007F0000  /* Maximum time Slots */
+#define PCIE_VC0_RC_MAX_TIMESLOTS_S          16
+#define PCIE_VC0_RC_PORT_ARB_TAB_OFFSET      0xFF000000  /* Port Arbitration Table Offset */
+#define PCIE_VC0_RC_PORT_ARB_TAB_OFFSET_S    24
+
+/* VC0 Resource Control Register */
+#define PCIE_VC0_RC0(X)                      (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x154)
+#define PCIE_VC0_RC0_TVM0                    0x00000001  /* TC0 and VC0 */
+#define PCIE_VC0_RC0_TVM1                    0x00000002  /* TC1 and VC1 */
+#define PCIE_VC0_RC0_TVM2                    0x00000004  /* TC2 and VC2 */
+#define PCIE_VC0_RC0_TVM3                    0x00000008  /* TC3 and VC3 */
+#define PCIE_VC0_RC0_TVM4                    0x00000010  /* TC4 and VC4 */
+#define PCIE_VC0_RC0_TVM5                    0x00000020  /* TC5 and VC5 */
+#define PCIE_VC0_RC0_TVM6                    0x00000040  /* TC6 and VC6 */
+#define PCIE_VC0_RC0_TVM7                    0x00000080  /* TC7 and VC7 */
+#define PCIE_VC0_RC0_TC_VC                   0x000000FF  /* TC/VC mask */
+
+#define PCIE_VC0_RC0_LOAD_PORT_ARB_TAB       0x00010000  /* Load Port Arbitration Table */
+#define PCIE_VC0_RC0_PORT_ARB_SEL            0x000E0000  /* Port Arbitration Select */
+#define PCIE_VC0_RC0_PORT_ARB_SEL_S          17
+#define PCIE_VC0_RC0_VC_ID                   0x07000000  /* VC ID */
+#define PCIE_VC0_RC0_VC_ID_S                 24
+#define PCIE_VC0_RC0_VC_EN                   0x80000000  /* VC Enable */
+
+/* VC0 Resource Status Register */
+#define PCIE_VC0_RSR0(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x158)
+#define PCIE_VC0_RSR0_PORT_ARB_TAB_STATUS    0x00010000  /* Port Arbitration Table Status,not used */
+#define PCIE_VC0_RSR0_VC_NEG_PENDING         0x00020000  /* VC Negotiation Pending */
+
+/* Ack Latency Timer and Replay Timer Register */
+#define PCIE_ALTRT(X)                         (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x700)
+#define PCIE_ALTRT_ROUND_TRIP_LATENCY_LIMIT   0x0000FFFF  /* Round Trip Latency Time Limit */
+#define PCIE_ALTRT_ROUND_TRIP_LATENCY_LIMIT_S 0
+#define PCIE_ALTRT_REPLAY_TIME_LIMIT          0xFFFF0000  /* Replay Time Limit */
+#define PCIE_ALTRT_REPLAY_TIME_LIMIT_S        16
+
+/* Other Message Register */
+#define PCIE_OMR(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x704)
+
+/* Port Force Link Register */
+#define PCIE_PFLR(X)                         (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x708)
+#define PCIE_PFLR_LINK_NUM                   0x000000FF  /* Link Number */
+#define PCIE_PFLR_LINK_NUM_S                 0
+#define PCIE_PFLR_FORCE_LINK                 0x00008000  /* Force link */
+#define PCIE_PFLR_LINK_STATE                 0x003F0000  /* Link State */
+#define PCIE_PFLR_LINK_STATE_S               16
+#define PCIE_PFLR_LOW_POWER_ENTRY_CNT        0xFF000000  /* Low Power Entrance Count, only for EP */
+#define PCIE_PFLR_LOW_POWER_ENTRY_CNT_S      24
+
+/* Ack Frequency Register */
+#define PCIE_AFR(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x70C)
+#define PCIE_AFR_AF                          0x000000FF  /* Ack Frequency */
+#define PCIE_AFR_AF_S                        0
+#define PCIE_AFR_FTS_NUM                     0x0000FF00  /* The number of Fast Training Sequence from L0S to L0 */
+#define PCIE_AFR_FTS_NUM_S                   8
+#define PCIE_AFR_COM_FTS_NUM                 0x00FF0000  /* N_FTS; when common clock is used*/
+#define PCIE_AFR_COM_FTS_NUM_S               16
+#define PCIE_AFR_L0S_ENTRY_LATENCY           0x07000000  /* L0s Entrance Latency */
+#define PCIE_AFR_L0S_ENTRY_LATENCY_S         24
+#define PCIE_AFR_L1_ENTRY_LATENCY            0x38000000  /* L1 Entrance Latency */
+#define PCIE_AFR_L1_ENTRY_LATENCY_S          27
+#define PCIE_AFR_FTS_NUM_DEFAULT             32
+#define PCIE_AFR_L0S_ENTRY_LATENCY_DEFAULT   7
+#define PCIE_AFR_L1_ENTRY_LATENCY_DEFAULT    5
+
+/* Port Link Control Register */
+#define PCIE_PLCR(X)                         (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x710)
+#define PCIE_PLCR_OTHER_MSG_REQ              0x00000001  /* Other Message Request */
+#define PCIE_PLCR_SCRAMBLE_DISABLE           0x00000002  /* Scramble Disable */  
+#define PCIE_PLCR_LOOPBACK_EN                0x00000004  /* Loopback Enable */
+#define PCIE_PLCR_LTSSM_HOT_RST              0x00000008  /* Force LTSSM to the hot reset */
+#define PCIE_PLCR_DLL_LINK_EN                0x00000020  /* Enable Link initialization */
+#define PCIE_PLCR_FAST_LINK_SIM_EN           0x00000080  /* Sets all internal timers to fast mode for simulation purposes */
+#define PCIE_PLCR_LINK_MODE                  0x003F0000  /* Link Mode Enable Mask */
+#define PCIE_PLCR_LINK_MODE_S                16
+#define PCIE_PLCR_CORRUPTED_CRC_EN           0x02000000  /* Enabled Corrupt CRC */
+
+/* Lane Skew Register */
+#define PCIE_LSR(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x714)
+#define PCIE_LSR_LANE_SKEW_NUM               0x00FFFFFF  /* Insert Lane Skew for Transmit, not applicable */
+#define PCIE_LSR_LANE_SKEW_NUM_S             0
+#define PCIE_LSR_FC_DISABLE                  0x01000000  /* Disable of Flow Control */
+#define PCIE_LSR_ACKNAK_DISABLE              0x02000000  /* Disable of Ack/Nak */
+#define PCIE_LSR_LANE_DESKEW_DISABLE         0x80000000  /* Disable of Lane-to-Lane Skew */
+
+/* Symbol Number Register */
+#define PCIE_SNR(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x718)
+#define PCIE_SNR_TS                          0x0000000F  /* Number of TS Symbol */
+#define PCIE_SNR_TS_S                        0
+#define PCIE_SNR_SKP                         0x00000700  /* Number of SKP Symbol */
+#define PCIE_SNR_SKP_S                       8
+#define PCIE_SNR_REPLAY_TIMER                0x0007C000  /* Timer Modifier for Replay Timer */
+#define PCIE_SNR_REPLAY_TIMER_S              14
+#define PCIE_SNR_ACKNAK_LATENCY_TIMER        0x00F80000  /* Timer Modifier for Ack/Nak Latency Timer */
+#define PCIE_SNR_ACKNAK_LATENCY_TIMER_S      19
+#define PCIE_SNR_FC_TIMER                    0x1F000000  /* Timer Modifier for Flow Control Watchdog Timer */
+#define PCIE_SNR_FC_TIMER_S                  28
+
+/* Symbol Timer Register and Filter Mask Register 1 */
+#define PCIE_STRFMR(X)                      (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x71C)
+#define PCIE_STRFMR_SKP_INTERVAL            0x000007FF  /* SKP lnterval Value */
+#define PCIE_STRFMR_SKP_INTERVAL_S          0
+#define PCIE_STRFMR_FC_WDT_DISABLE          0x00008000  /* Disable of FC Watchdog Timer */
+#define PCIE_STRFMR_TLP_FUNC_MISMATCH_OK    0x00010000  /* Mask Function Mismatch Filtering for Incoming Requests */
+#define PCIE_STRFMR_POISONED_TLP_OK         0x00020000  /* Mask Poisoned TLP Filtering */
+#define PCIE_STRFMR_BAR_MATCH_OK            0x00040000  /* Mask BAR Match Filtering */
+#define PCIE_STRFMR_TYPE1_CFG_REQ_OK        0x00080000  /* Mask Type 1 Configuration Request Filtering */
+#define PCIE_STRFMR_LOCKED_REQ_OK           0x00100000  /* Mask Locked Request Filtering */
+#define PCIE_STRFMR_CPL_TAG_ERR_RULES_OK    0x00200000  /* Mask Tag Error Rules for Received Completions */
+#define PCIE_STRFMR_CPL_REQUESTOR_ID_MISMATCH_OK 0x00400000  /* Mask Requester ID Mismatch Error for Received Completions */
+#define PCIE_STRFMR_CPL_FUNC_MISMATCH_OK         0x00800000  /* Mask Function Mismatch Error for Received Completions */
+#define PCIE_STRFMR_CPL_TC_MISMATCH_OK           0x01000000  /* Mask Traffic Class Mismatch Error for Received Completions */
+#define PCIE_STRFMR_CPL_ATTR_MISMATCH_OK         0x02000000  /* Mask Attribute Mismatch Error for Received Completions */
+#define PCIE_STRFMR_CPL_LENGTH_MISMATCH_OK       0x04000000  /* Mask Length Mismatch Error for Received Completions */
+#define PCIE_STRFMR_TLP_ECRC_ERR_OK              0x08000000  /* Mask ECRC Error Filtering */
+#define PCIE_STRFMR_CPL_TLP_ECRC_OK              0x10000000  /* Mask ECRC Error Filtering for Completions */
+#define PCIE_STRFMR_RX_TLP_MSG_NO_DROP           0x20000000  /* Send Message TLPs */
+#define PCIE_STRFMR_RX_IO_TRANS_ENABLE           0x40000000  /* Mask Filtering of received I/O Requests */
+#define PCIE_STRFMR_RX_CFG_TRANS_ENABLE          0x80000000  /* Mask Filtering of Received Configuration Requests */
+
+#define PCIE_DEF_SKP_INTERVAL    700             /* 1180 ~1538 , 125MHz * 2, 250MHz * 1 */
+
+/* Filter Masker Register 2 */
+#define PCIE_FMR2(X)                             (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x720)
+#define PCIE_FMR2_VENDOR_MSG0_PASSED_TO_TRGT1    0x00000001  /* Mask RADM Filtering and Error Handling Rules */
+#define PCIE_FMR2_VENDOR_MSG1_PASSED_TO_TRGT1    0x00000002  /* Mask RADM Filtering and Error Handling Rules */
+
+/* Debug Register 0 */
+#define PCIE_DBR0(X)                              (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x728)
+
+/* Debug Register 1 */
+#define PCIE_DBR1(X)                              (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x72C)
+
+/* Transmit Posted FC Credit Status Register */
+#define PCIE_TPFCS(X)                             (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x730)
+#define PCIE_TPFCS_TX_P_DATA_FC_CREDITS           0x00000FFF /* Transmit Posted Data FC Credits */
+#define PCIE_TPFCS_TX_P_DATA_FC_CREDITS_S         0
+#define PCIE_TPFCS_TX_P_HDR_FC_CREDITS            0x000FF000 /* Transmit Posted Header FC Credits */
+#define PCIE_TPFCS_TX_P_HDR_FC_CREDITS_S          12
+
+/* Transmit Non-Posted FC Credit Status */
+#define PCIE_TNPFCS(X)                            (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x734)
+#define PCIE_TNPFCS_TX_NP_DATA_FC_CREDITS         0x00000FFF /* Transmit Non-Posted Data FC Credits */
+#define PCIE_TNPFCS_TX_NP_DATA_FC_CREDITS_S       0
+#define PCIE_TNPFCS_TX_NP_HDR_FC_CREDITS          0x000FF000 /* Transmit Non-Posted Header FC Credits */
+#define PCIE_TNPFCS_TX_NP_HDR_FC_CREDITS_S        12
+
+/* Transmit Complete FC Credit Status Register */
+#define PCIE_TCFCS(X)                             (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x738)
+#define PCIE_TCFCS_TX_CPL_DATA_FC_CREDITS         0x00000FFF /* Transmit Completion Data FC Credits */
+#define PCIE_TCFCS_TX_CPL_DATA_FC_CREDITS_S       0
+#define PCIE_TCFCS_TX_CPL_HDR_FC_CREDITS          0x000FF000 /* Transmit Completion Header FC Credits */
+#define PCIE_TCFCS_TX_CPL_HDR_FC_CREDITS_S        12
+
+/* Queue Status Register */
+#define PCIE_QSR(X)                              (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x73C)
+#define PCIE_QSR_WAIT_UPDATE_FC_DLL               0x00000001 /* Received TLP FC Credits Not Returned */
+#define PCIE_QSR_TX_RETRY_BUF_NOT_EMPTY           0x00000002 /* Transmit Retry Buffer Not Empty */
+#define PCIE_QSR_RX_QUEUE_NOT_EMPTY               0x00000004 /* Received Queue Not Empty */
+
+/* VC Transmit Arbitration Register 1 */
+#define PCIE_VCTAR1(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x740)
+#define PCIE_VCTAR1_WRR_WEIGHT_VC0               0x000000FF /* WRR Weight for VC0 */
+#define PCIE_VCTAR1_WRR_WEIGHT_VC1               0x0000FF00 /* WRR Weight for VC1 */
+#define PCIE_VCTAR1_WRR_WEIGHT_VC2               0x00FF0000 /* WRR Weight for VC2 */
+#define PCIE_VCTAR1_WRR_WEIGHT_VC3               0xFF000000 /* WRR Weight for VC3 */
+
+/* VC Transmit Arbitration Register 2 */
+#define PCIE_VCTAR2(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x744)
+#define PCIE_VCTAR2_WRR_WEIGHT_VC4               0x000000FF /* WRR Weight for VC4 */
+#define PCIE_VCTAR2_WRR_WEIGHT_VC5               0x0000FF00 /* WRR Weight for VC5 */
+#define PCIE_VCTAR2_WRR_WEIGHT_VC6               0x00FF0000 /* WRR Weight for VC6 */
+#define PCIE_VCTAR2_WRR_WEIGHT_VC7               0xFF000000 /* WRR Weight for VC7 */
+
+/* VC0 Posted Receive Queue Control Register */
+#define PCIE_VC0_PRQCR(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x748)
+#define PCIE_VC0_PRQCR_P_DATA_CREDITS            0x00000FFF /* VC0 Posted Data Credits */
+#define PCIE_VC0_PRQCR_P_DATA_CREDITS_S          0
+#define PCIE_VC0_PRQCR_P_HDR_CREDITS             0x000FF000 /* VC0 Posted Header Credits */
+#define PCIE_VC0_PRQCR_P_HDR_CREDITS_S           12
+#define PCIE_VC0_PRQCR_P_TLP_QUEUE_MODE          0x00E00000 /* VC0 Posted TLP Queue Mode */
+#define PCIE_VC0_PRQCR_P_TLP_QUEUE_MODE_S        20
+#define PCIE_VC0_PRQCR_TLP_RELAX_ORDER           0x40000000 /* TLP Type Ordering for VC0 */    
+#define PCIE_VC0_PRQCR_VC_STRICT_ORDER           0x80000000 /* VC0 Ordering for Receive Queues */
+
+/* VC0 Non-Posted Receive Queue Control */
+#define PCIE_VC0_NPRQCR(X)                      (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x74C)
+#define PCIE_VC0_NPRQCR_NP_DATA_CREDITS          0x00000FFF /* VC0 Non-Posted Data Credits */
+#define PCIE_VC0_NPRQCR_NP_DATA_CREDITS_S        0
+#define PCIE_VC0_NPRQCR_NP_HDR_CREDITS           0x000FF000 /* VC0 Non-Posted Header Credits */
+#define PCIE_VC0_NPRQCR_NP_HDR_CREDITS_S         12
+#define PCIE_VC0_NPRQCR_NP_TLP_QUEUE_MODE        0x00E00000 /* VC0 Non-Posted TLP Queue Mode */
+#define PCIE_VC0_NPRQCR_NP_TLP_QUEUE_MODE_S      20
+
+/* VC0 Completion Receive Queue Control */
+#define PCIE_VC0_CRQCR(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x750)
+#define PCIE_VC0_CRQCR_CPL_DATA_CREDITS          0x00000FFF /* VC0 Completion TLP Queue Mode */
+#define PCIE_VC0_CRQCR_CPL_DATA_CREDITS_S        0
+#define PCIE_VC0_CRQCR_CPL_HDR_CREDITS           0x000FF000 /* VC0 Completion Header Credits */
+#define PCIE_VC0_CRQCR_CPL_HDR_CREDITS_S         12
+#define PCIE_VC0_CRQCR_CPL_TLP_QUEUE_MODE        0x00E00000 /* VC0 Completion Data Credits */
+#define PCIE_VC0_CRQCR_CPL_TLP_QUEUE_MODE_S      21
+
+/* Applicable to the above three registers */
+enum {
+    PCIE_VC0_TLP_QUEUE_MODE_STORE_FORWARD = 1,
+    PCIE_VC0_TLP_QUEUE_MODE_CUT_THROUGH   = 2,
+    PCIE_VC0_TLP_QUEUE_MODE_BYPASS        = 4,
+};
+
+/* VC0 Posted Buffer Depth Register */
+#define PCIE_VC0_PBD(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x7A8)
+#define PCIE_VC0_PBD_P_DATA_QUEUE_ENTRIES       0x00003FFF /* VC0 Posted Data Queue Depth */
+#define PCIE_VC0_PBD_P_DATA_QUEUE_ENTRIES_S     0
+#define PCIE_VC0_PBD_P_HDR_QUEUE_ENTRIES        0x03FF0000 /* VC0 Posted Header Queue Depth */
+#define PCIE_VC0_PBD_P_HDR_QUEUE_ENTRIES_S      16
+
+/* VC0 Non-Posted Buffer Depth Register */
+#define PCIE_VC0_NPBD(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x7AC)
+#define PCIE_VC0_NPBD_NP_DATA_QUEUE_ENTRIES     0x00003FFF /* VC0 Non-Posted Data Queue Depth */
+#define PCIE_VC0_NPBD_NP_DATA_QUEUE_ENTRIES_S   0
+#define PCIE_VC0_NPBD_NP_HDR_QUEUE_ENTRIES      0x03FF0000 /* VC0 Non-Posted Header Queue Depth */
+#define PCIE_VC0_NPBD_NP_HDR_QUEUE_ENTRIES_S    16
+
+/* VC0 Completion Buffer Depth Register */
+#define PCIE_VC0_CBD(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x7B0)
+#define PCIE_VC0_CBD_CPL_DATA_QUEUE_ENTRIES     0x00003FFF /* C0 Completion Data Queue Depth */
+#define PCIE_VC0_CBD_CPL_DATA_QUEUE_ENTRIES_S   0
+#define PCIE_VC0_CBD_CPL_HDR_QUEUE_ENTRIES      0x03FF0000 /* VC0 Completion Header Queue Depth */
+#define PCIE_VC0_CBD_CPL_HDR_QUEUE_ENTRIES_S    16
+
+/* PHY Status Register, all zeros in VR9 */
+#define PCIE_PHYSR(X)                           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x810)
+
+/* PHY Control Register, all zeros in VR9 */
+#define PCIE_PHYCR(X)                           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x814)
+
+/* 
+ * PCIe PDI PHY register definition, suppose all the following 
+ * stuff is confidential. 
+ * XXX, detailed bit definition
+ */
+#define	PCIE_PHY_PLL_CTRL1(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x22 << 1))
+#define	PCIE_PHY_PLL_CTRL2(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x23 << 1))
+#define	PCIE_PHY_PLL_CTRL3(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x24 << 1))
+#define	PCIE_PHY_PLL_CTRL4(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x25 << 1))
+#define	PCIE_PHY_PLL_CTRL5(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x26 << 1))
+#define	PCIE_PHY_PLL_CTRL6(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x27 << 1))
+#define	PCIE_PHY_PLL_CTRL7(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x28 << 1))
+#define	PCIE_PHY_PLL_A_CTRL1(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x29 << 1))
+#define	PCIE_PHY_PLL_A_CTRL2(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x2A << 1))
+#define	PCIE_PHY_PLL_A_CTRL3(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x2B << 1))
+#define	PCIE_PHY_PLL_STATUS(X)      (PCIE_PHY_PORT_TO_BASE(X) + (0x2C << 1))
+ 
+#define PCIE_PHY_TX1_CTRL1(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x30 << 1))
+#define PCIE_PHY_TX1_CTRL2(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x31 << 1))
+#define PCIE_PHY_TX1_CTRL3(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x32 << 1))
+#define PCIE_PHY_TX1_A_CTRL1(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x33 << 1))
+#define PCIE_PHY_TX1_A_CTRL2(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x34 << 1))
+#define PCIE_PHY_TX1_MOD1(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x35 << 1))
+#define PCIE_PHY_TX1_MOD2(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x36 << 1))
+#define PCIE_PHY_TX1_MOD3(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x37 << 1))
+
+#define PCIE_PHY_TX2_CTRL1(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x38 << 1))
+#define PCIE_PHY_TX2_CTRL2(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x39 << 1))
+#define PCIE_PHY_TX2_A_CTRL1(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x3B << 1))
+#define PCIE_PHY_TX2_A_CTRL2(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x3C << 1))
+#define PCIE_PHY_TX2_MOD1(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x3D << 1))
+#define PCIE_PHY_TX2_MOD2(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x3E << 1))
+#define PCIE_PHY_TX2_MOD3(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x3F << 1))
+
+#define PCIE_PHY_RX1_CTRL1(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x50 << 1))
+#define PCIE_PHY_RX1_CTRL2(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x51 << 1))
+#define PCIE_PHY_RX1_CDR(X)         (PCIE_PHY_PORT_TO_BASE(X) + (0x52 << 1))
+#define PCIE_PHY_RX1_EI(X)          (PCIE_PHY_PORT_TO_BASE(X) + (0x53 << 1))
+#define PCIE_PHY_RX1_A_CTRL(X)      (PCIE_PHY_PORT_TO_BASE(X) + (0x55 << 1))
+
+/* Interrupt related stuff */
+#define PCIE_LEGACY_DISABLE 0
+#define PCIE_LEGACY_INTA  1
+#define PCIE_LEGACY_INTB  2
+#define PCIE_LEGACY_INTC  3
+#define PCIE_LEGACY_INTD  4
+#define PCIE_LEGACY_INT_MAX PCIE_LEGACY_INTD
+
+#endif /* IFXMIPS_PCIE_REG_H */
+
--- /dev/null
+++ b/arch/mips/pci/ifxmips_pcie_vr9.h
@@ -0,0 +1,271 @@
+/****************************************************************************
+                              Copyright (c) 2010
+                            Lantiq Deutschland GmbH
+                     Am Campeon 3; 85579 Neubiberg, Germany
+
+  For licensing information, see the file 'LICENSE' in the root folder of
+  this software module.
+
+ *****************************************************************************/
+/*!
+  \file ifxmips_pcie_vr9.h
+  \ingroup IFX_PCIE
+  \brief PCIe RC driver vr9 specific file
+*/
+
+#ifndef IFXMIPS_PCIE_VR9_H
+#define IFXMIPS_PCIE_VR9_H
+
+#include <linux/types.h>
+#include <linux/delay.h>
+
+#include <linux/gpio.h>
+#include <lantiq_soc.h>
+
+#define IFX_PCIE_GPIO_RESET  238
+
+#define IFX_REG_R32    ltq_r32
+#define IFX_REG_W32    ltq_w32
+#define CONFIG_IFX_PCIE_HW_SWAP
+#define IFX_RCU_AHB_ENDIAN                      ((volatile u32*)(IFX_RCU + 0x004C))
+#define IFX_RCU_RST_REQ                         ((volatile u32*)(IFX_RCU + 0x0010))
+#define IFX_RCU_AHB_BE_PCIE_PDI                  0x00000080  /* Configure PCIE PDI module in big endian*/
+
+#define IFX_RCU                                 (KSEG1 | 0x1F203000)
+#define IFX_RCU_AHB_BE_PCIE_M                    0x00000001  /* Configure AHB master port that connects to PCIe RC in big endian */
+#define IFX_RCU_AHB_BE_PCIE_S                    0x00000010  /* Configure AHB slave port that connects to PCIe RC in little endian */
+#define IFX_RCU_AHB_BE_XBAR_M                    0x00000002  /* Configure AHB master port that connects to XBAR in big endian */
+#define CONFIG_IFX_PCIE_PHY_36MHZ_MODE
+
+#define IFX_PMU1_MODULE_PCIE_PHY   (0)
+#define IFX_PMU1_MODULE_PCIE_CTRL  (1)
+#define IFX_PMU1_MODULE_PDI        (4)
+#define IFX_PMU1_MODULE_MSI        (5)
+
+#define IFX_PMU_MODULE_PCIE_L0_CLK (31)
+
+
+#define IFX_GPIO				(KSEG1 | 0x1E100B00)
+#define ALT0			((volatile u32*)(IFX_GPIO + 0x007c))
+#define ALT1			((volatile u32*)(IFX_GPIO + 0x0080))
+#define OD			((volatile u32*)(IFX_GPIO + 0x0084))
+#define DIR			((volatile u32*)(IFX_GPIO + 0x0078))
+#define OUT			((volatile u32*)(IFX_GPIO + 0x0070))
+
+
+static inline void pcie_ep_gpio_rst_init(int pcie_port)
+{
+
+	gpio_request(IFX_PCIE_GPIO_RESET, "pcie-reset");
+	gpio_direction_output(IFX_PCIE_GPIO_RESET, 1);
+	gpio_set_value(IFX_PCIE_GPIO_RESET, 1);
+
+/*    ifx_gpio_pin_reserve(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
+    ifx_gpio_output_set(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
+    ifx_gpio_dir_out_set(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
+    ifx_gpio_altsel0_clear(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
+    ifx_gpio_altsel1_clear(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
+    ifx_gpio_open_drain_set(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);*/
+}
+
+static inline void pcie_ahb_pmu_setup(void) 
+{
+	/* Enable AHB bus master/slave */
+	struct clk *clk;
+	clk = clk_get_sys("1d900000.pcie", "ahb");
+	clk_enable(clk);
+
+    //AHBM_PMU_SETUP(IFX_PMU_ENABLE);
+    //AHBS_PMU_SETUP(IFX_PMU_ENABLE);
+}
+
+static inline void pcie_rcu_endian_setup(int pcie_port)
+{
+    u32 reg;
+
+    reg = IFX_REG_R32(IFX_RCU_AHB_ENDIAN);
+#ifdef CONFIG_IFX_PCIE_HW_SWAP
+    reg |= IFX_RCU_AHB_BE_PCIE_M;
+    reg |= IFX_RCU_AHB_BE_PCIE_S;
+    reg &= ~IFX_RCU_AHB_BE_XBAR_M;
+#else 
+    reg |= IFX_RCU_AHB_BE_PCIE_M;
+    reg &= ~IFX_RCU_AHB_BE_PCIE_S;
+    reg &= ~IFX_RCU_AHB_BE_XBAR_M;
+#endif /* CONFIG_IFX_PCIE_HW_SWAP */
+    IFX_REG_W32(reg, IFX_RCU_AHB_ENDIAN);
+    IFX_PCIE_PRINT(PCIE_MSG_REG, "%s IFX_RCU_AHB_ENDIAN: 0x%08x\n", __func__, IFX_REG_R32(IFX_RCU_AHB_ENDIAN));
+}
+
+static inline void pcie_phy_pmu_enable(int pcie_port)
+{
+	struct clk *clk;
+	clk = clk_get_sys("1d900000.pcie", "phy");
+	clk_enable(clk);
+
+	//PCIE_PHY_PMU_SETUP(IFX_PMU_ENABLE);
+}
+
+static inline void pcie_phy_pmu_disable(int pcie_port)
+{
+	struct clk *clk;
+	clk = clk_get_sys("1d900000.pcie", "phy");
+	clk_disable(clk);
+
+//    PCIE_PHY_PMU_SETUP(IFX_PMU_DISABLE);
+}
+
+static inline void pcie_pdi_big_endian(int pcie_port)
+{
+    u32 reg;
+
+    /* SRAM2PDI endianness control. */
+    reg = IFX_REG_R32(IFX_RCU_AHB_ENDIAN);
+    /* Config AHB->PCIe and PDI endianness */
+    reg |= IFX_RCU_AHB_BE_PCIE_PDI;
+    IFX_REG_W32(reg, IFX_RCU_AHB_ENDIAN);
+}
+
+static inline void pcie_pdi_pmu_enable(int pcie_port)
+{
+    /* Enable PDI to access PCIe PHY register */
+	struct clk *clk;
+	clk = clk_get_sys("1d900000.pcie", "pdi");
+	clk_enable(clk);
+    //PDI_PMU_SETUP(IFX_PMU_ENABLE);
+}
+
+static inline void pcie_core_rst_assert(int pcie_port)
+{
+    u32 reg;
+
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+
+    /* Reset PCIe PHY & Core, bit 22, bit 26 may be affected if write it directly  */
+    reg |= 0x00400000;
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_core_rst_deassert(int pcie_port)
+{
+    u32 reg;
+
+    /* Make sure one micro-second delay */
+    udelay(1);
+
+    /* Reset PCIe PHY & Core, bit 22 */
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+    reg &= ~0x00400000;
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_phy_rst_assert(int pcie_port)
+{
+    u32 reg;
+
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+    reg |= 0x00001000; /* Bit 12 */
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_phy_rst_deassert(int pcie_port)
+{
+    u32 reg;
+
+    /* Make sure one micro-second delay */
+    udelay(1);
+
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+    reg &= ~0x00001000; /* Bit 12 */
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_device_rst_assert(int pcie_port)
+{
+	printk("%s:%s[%d]\n", __FILE__, __func__, __LINE__);
+	gpio_set_value(IFX_PCIE_GPIO_RESET, 0);
+//    ifx_gpio_output_clear(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
+}
+
+static inline void pcie_device_rst_deassert(int pcie_port)
+{
+    mdelay(100);
+    printk("%s:%s[%d]\n", __FILE__, __func__, __LINE__);
+	gpio_direction_output(IFX_PCIE_GPIO_RESET, 1);
+//    gpio_set_value(IFX_PCIE_GPIO_RESET, 1);
+    //ifx_gpio_output_set(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
+}
+
+static inline void pcie_core_pmu_setup(int pcie_port)
+{
+	struct clk *clk;
+	clk = clk_get_sys("1d900000.pcie", "ctl");
+	clk_enable(clk);
+	clk = clk_get_sys("1d900000.pcie", "bus");
+	clk_enable(clk);
+
+    /* PCIe Core controller enabled */
+//    PCIE_CTRL_PMU_SETUP(IFX_PMU_ENABLE);
+
+    /* Enable PCIe L0 Clock */
+//  PCIE_L0_CLK_PMU_SETUP(IFX_PMU_ENABLE);
+}
+
+static inline void pcie_msi_init(int pcie_port)
+{
+	struct clk *clk;
+	pcie_msi_pic_init(pcie_port);
+	clk = clk_get_sys("ltq_pcie", "msi");
+	clk_enable(clk);
+//    MSI_PMU_SETUP(IFX_PMU_ENABLE);
+}
+
+static inline u32
+ifx_pcie_bus_nr_deduct(u32 bus_number, int pcie_port)
+{
+    u32 tbus_number = bus_number;
+
+#ifdef CONFIG_IFX_PCI
+    if (pcibios_host_nr() > 1) {
+        tbus_number -= pcibios_1st_host_bus_nr();
+    }
+#endif /* CONFIG_IFX_PCI */
+    return tbus_number;
+}
+
+static inline u32
+ifx_pcie_bus_enum_hack(struct pci_bus *bus, u32 devfn, int where, u32 value, int pcie_port, int read)
+{
+    struct pci_dev *pdev;
+    u32 tvalue = value;
+
+    /* Sanity check */
+    pdev = pci_get_slot(bus, devfn);
+    if (pdev == NULL) {
+        return tvalue;
+    }
+
+    /* Only care about PCI bridge */
+    if (pdev->hdr_type != PCI_HEADER_TYPE_BRIDGE) {
+        return tvalue;
+    }
+
+    if (read) { /* Read hack */
+    #ifdef CONFIG_IFX_PCI
+        if (pcibios_host_nr() > 1) {
+            tvalue = ifx_pcie_bus_enum_read_hack(where, tvalue);
+        }
+    #endif /* CONFIG_IFX_PCI */  
+    }
+    else { /* Write hack */
+    #ifdef CONFIG_IFX_PCI    
+        if (pcibios_host_nr() > 1) {
+            tvalue = ifx_pcie_bus_enum_write_hack(where, tvalue);
+        }
+    #endif
+    }
+    return tvalue;
+}
+
+#endif /* IFXMIPS_PCIE_VR9_H */
+
--- a/arch/mips/pci/pci.c
+++ b/arch/mips/pci/pci.c
@@ -266,6 +266,31 @@ static int __init pcibios_init(void)
 
 subsys_initcall(pcibios_init);
 
+int pcibios_host_nr(void)
+{
+    int count;
+    struct pci_controller *hose;
+    for (count = 0, hose = hose_head; hose; hose = hose->next, count++) {
+        ;
+    }
+    return count;
+}
+EXPORT_SYMBOL(pcibios_host_nr);
+
+int pcibios_1st_host_bus_nr(void)
+{
+    int bus_nr = 0;
+    struct pci_controller *hose = hose_head;
+
+    if (hose != NULL) {
+        if (hose->bus != NULL) {
+            bus_nr = hose->bus->number + 1;
+        }
+    }
+    return bus_nr;
+}
+EXPORT_SYMBOL(pcibios_1st_host_bus_nr);
+
 static int pcibios_enable_resources(struct pci_dev *dev, int mask)
 {
 	u16 cmd, old_cmd;
--- /dev/null
+++ b/arch/mips/pci/pcie-lantiq.h
@@ -0,0 +1,1305 @@
+/******************************************************************************
+**
+** FILE NAME    : ifxmips_pcie_reg.h
+** PROJECT      : IFX UEIP for VRX200
+** MODULES      : PCIe module
+**
+** DATE         : 02 Mar 2009
+** AUTHOR       : Lei Chuanhua
+** DESCRIPTION  : PCIe Root Complex Driver
+** COPYRIGHT    :       Copyright (c) 2009
+**                      Infineon Technologies AG
+**                      Am Campeon 1-12, 85579 Neubiberg, Germany
+**
+**    This program is free software; you can redistribute it and/or modify
+**    it under the terms of the GNU General Public License as published by
+**    the Free Software Foundation; either version 2 of the License, or
+**    (at your option) any later version.
+** HISTORY
+** $Version $Date        $Author         $Comment
+** 0.0.1    17 Mar,2009  Lei Chuanhua    Initial version
+*******************************************************************************/
+#ifndef IFXMIPS_PCIE_REG_H
+#define IFXMIPS_PCIE_REG_H
+#include <linux/version.h>
+#include <linux/types.h>
+#include <linux/pci.h>
+#include <linux/interrupt.h>
+/*!
+ \file ifxmips_pcie_reg.h
+ \ingroup IFX_PCIE  
+ \brief header file for PCIe module register definition
+*/
+/* PCIe Address Mapping Base */
+#define PCIE_CFG_PHY_BASE        0x1D000000UL
+#define PCIE_CFG_BASE           (KSEG1 + PCIE_CFG_PHY_BASE)
+#define PCIE_CFG_SIZE           (8 * 1024 * 1024)
+
+#define PCIE_MEM_PHY_BASE        0x1C000000UL
+#define PCIE_MEM_BASE           (KSEG1 + PCIE_MEM_PHY_BASE)
+#define PCIE_MEM_SIZE           (16 * 1024 * 1024)
+#define PCIE_MEM_PHY_END        (PCIE_MEM_PHY_BASE + PCIE_MEM_SIZE - 1)
+
+#define PCIE_IO_PHY_BASE         0x1D800000UL
+#define PCIE_IO_BASE            (KSEG1 + PCIE_IO_PHY_BASE)
+#define PCIE_IO_SIZE            (1 * 1024 * 1024)
+#define PCIE_IO_PHY_END         (PCIE_IO_PHY_BASE + PCIE_IO_SIZE - 1)
+
+#define PCIE_RC_CFG_BASE        (KSEG1 + 0x1D900000)
+#define PCIE_APP_LOGIC_REG      (KSEG1 + 0x1E100900)
+#define PCIE_MSI_PHY_BASE        0x1F600000UL
+
+#define PCIE_PDI_PHY_BASE        0x1F106800UL
+#define PCIE_PDI_BASE           (KSEG1 + PCIE_PDI_PHY_BASE)
+#define PCIE_PDI_SIZE            0x400
+
+#define PCIE1_CFG_PHY_BASE        0x19000000UL
+#define PCIE1_CFG_BASE           (KSEG1 + PCIE1_CFG_PHY_BASE)
+#define PCIE1_CFG_SIZE           (8 * 1024 * 1024)
+
+#define PCIE1_MEM_PHY_BASE        0x18000000UL
+#define PCIE1_MEM_BASE           (KSEG1 + PCIE1_MEM_PHY_BASE)
+#define PCIE1_MEM_SIZE           (16 * 1024 * 1024)
+#define PCIE1_MEM_PHY_END        (PCIE1_MEM_PHY_BASE + PCIE1_MEM_SIZE - 1)
+
+#define PCIE1_IO_PHY_BASE         0x19800000UL
+#define PCIE1_IO_BASE            (KSEG1 + PCIE1_IO_PHY_BASE)
+#define PCIE1_IO_SIZE            (1 * 1024 * 1024)
+#define PCIE1_IO_PHY_END         (PCIE1_IO_PHY_BASE + PCIE1_IO_SIZE - 1)
+
+#define PCIE1_RC_CFG_BASE        (KSEG1 + 0x19900000)
+#define PCIE1_APP_LOGIC_REG      (KSEG1 + 0x1E100700)
+#define PCIE1_MSI_PHY_BASE        0x1F400000UL
+
+#define PCIE1_PDI_PHY_BASE        0x1F700400UL
+#define PCIE1_PDI_BASE           (KSEG1 + PCIE1_PDI_PHY_BASE)
+#define PCIE1_PDI_SIZE            0x400
+
+#define PCIE_CFG_PORT_TO_BASE(X)     ((X) > 0 ? (PCIE1_CFG_BASE) : (PCIE_CFG_BASE))
+#define PCIE_MEM_PORT_TO_BASE(X)     ((X) > 0 ? (PCIE1_MEM_BASE) : (PCIE_MEM_BASE))
+#define PCIE_IO_PORT_TO_BASE(X)      ((X) > 0 ? (PCIE1_IO_BASE) : (PCIE_IO_BASE))
+#define PCIE_MEM_PHY_PORT_TO_BASE(X) ((X) > 0 ? (PCIE1_MEM_PHY_BASE) : (PCIE_MEM_PHY_BASE))
+#define PCIE_MEM_PHY_PORT_TO_END(X)  ((X) > 0 ? (PCIE1_MEM_PHY_END) : (PCIE_MEM_PHY_END))
+#define PCIE_IO_PHY_PORT_TO_BASE(X)  ((X) > 0 ? (PCIE1_IO_PHY_BASE) : (PCIE_IO_PHY_BASE))
+#define PCIE_IO_PHY_PORT_TO_END(X)   ((X) > 0 ? (PCIE1_IO_PHY_END) : (PCIE_IO_PHY_END))
+#define PCIE_APP_PORT_TO_BASE(X)     ((X) > 0 ? (PCIE1_APP_LOGIC_REG) : (PCIE_APP_LOGIC_REG))
+#define PCIE_RC_PORT_TO_BASE(X)      ((X) > 0 ? (PCIE1_RC_CFG_BASE) : (PCIE_RC_CFG_BASE))
+#define PCIE_PHY_PORT_TO_BASE(X)     ((X) > 0 ? (PCIE1_PDI_BASE) : (PCIE_PDI_BASE))
+
+/* PCIe Application Logic Register */
+/* RC Core Control Register */
+#define PCIE_RC_CCR(X)                      (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x10)
+/* This should be enabled after initializing configuratin registers
+ * Also should check link status retraining bit
+ */
+#define PCIE_RC_CCR_LTSSM_ENABLE             0x00000001    /* Enable LTSSM to continue link establishment */
+
+/* RC Core Debug Register */
+#define PCIE_RC_DR(X)                       (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x14)
+#define PCIE_RC_DR_DLL_UP                    0x00000001  /* Data Link Layer Up */
+#define PCIE_RC_DR_CURRENT_POWER_STATE       0x0000000E  /* Current Power State */
+#define PCIE_RC_DR_CURRENT_POWER_STATE_S     1
+#define PCIE_RC_DR_CURRENT_LTSSM_STATE       0x000001F0  /* Current LTSSM State */
+#define PCIE_RC_DR_CURRENT_LTSSM_STATE_S     4
+
+#define PCIE_RC_DR_PM_DEV_STATE              0x00000E00  /* Power Management D-State */
+#define PCIE_RC_DR_PM_DEV_STATE_S            9
+
+#define PCIE_RC_DR_PM_ENABLED                0x00001000  /* Power Management State from PMU */
+#define PCIE_RC_DR_PME_EVENT_ENABLED         0x00002000  /* Power Management Event Enable State */
+#define PCIE_RC_DR_AUX_POWER_ENABLED         0x00004000  /* Auxiliary Power Enable */
+
+/* Current Power State Definition */
+enum {
+    PCIE_RC_DR_D0 = 0,
+    PCIE_RC_DR_D1,   /* Not supported */
+    PCIE_RC_DR_D2,   /* Not supported */
+    PCIE_RC_DR_D3,
+    PCIE_RC_DR_UN,
+};
+
+/* PHY Link Status Register */
+#define PCIE_PHY_SR(X)                      (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x18)
+#define PCIE_PHY_SR_PHY_LINK_UP              0x00000001   /* PHY Link Up/Down Indicator */
+
+/* Electromechanical Control Register */
+#define PCIE_EM_CR(X)                       (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x1C)
+#define PCIE_EM_CR_CARD_IS_PRESENT           0x00000001  /* Card Presence Detect State */
+#define PCIE_EM_CR_MRL_OPEN                  0x00000002  /* MRL Sensor State */
+#define PCIE_EM_CR_POWER_FAULT_SET           0x00000004  /* Power Fault Detected */
+#define PCIE_EM_CR_MRL_SENSOR_SET            0x00000008  /* MRL Sensor Changed */
+#define PCIE_EM_CR_PRESENT_DETECT_SET        0x00000010  /* Card Presense Detect Changed */
+#define PCIE_EM_CR_CMD_CPL_INT_SET           0x00000020  /* Command Complete Interrupt */
+#define PCIE_EM_CR_SYS_INTERLOCK_SET         0x00000040  /* System Electromechanical IterLock Engaged */
+#define PCIE_EM_CR_ATTENTION_BUTTON_SET      0x00000080  /* Attention Button Pressed */
+
+/* Interrupt Status Register */
+#define PCIE_IR_SR(X)                       (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x20)
+#define PCIE_IR_SR_PME_CAUSE_MSI             0x00000002  /* MSI caused by PME */
+#define PCIE_IR_SR_HP_PME_WAKE_GEN           0x00000004  /* Hotplug PME Wake Generation */
+#define PCIE_IR_SR_HP_MSI                    0x00000008  /* Hotplug MSI */
+#define PCIE_IR_SR_AHB_LU_ERR                0x00000030  /* AHB Bridge Lookup Error Signals */
+#define PCIE_IR_SR_AHB_LU_ERR_S              4
+#define PCIE_IR_SR_INT_MSG_NUM               0x00003E00  /* Interrupt Message Number */
+#define PCIE_IR_SR_INT_MSG_NUM_S             9
+#define PCIE_IR_SR_AER_INT_MSG_NUM           0xF8000000  /* Advanced Error Interrupt Message Number */
+#define PCIE_IR_SR_AER_INT_MSG_NUM_S         27
+
+/* Message Control Register */
+#define PCIE_MSG_CR(X)                      (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x30)
+#define PCIE_MSG_CR_GEN_PME_TURN_OFF_MSG     0x00000001  /* Generate PME Turn Off Message */
+#define PCIE_MSG_CR_GEN_UNLOCK_MSG           0x00000002  /* Generate Unlock Message */
+
+#define PCIE_VDM_DR(X)                      (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x34)
+
+/* Vendor-Defined Message Requester ID Register */
+#define PCIE_VDM_RID(X)                     (PCIE_APP_PORT_TO_BASE (X) + 0x38)
+#define PCIE_VDM_RID_VENROR_MSG_REQ_ID       0x0000FFFF
+#define PCIE_VDM_RID_VDMRID_S                0
+
+/* ASPM Control Register */
+#define PCIE_ASPM_CR(X)                     (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x40)
+#define PCIE_ASPM_CR_HOT_RST                 0x00000001  /* Hot Reset Request to the downstream device */
+#define PCIE_ASPM_CR_REQ_EXIT_L1             0x00000002  /* Request to Exit L1 */
+#define PCIE_ASPM_CR_REQ_ENTER_L1            0x00000004  /* Request to Enter L1 */
+
+/* Vendor Message DW0 Register */
+#define PCIE_VM_MSG_DW0(X)                  (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x50)
+#define PCIE_VM_MSG_DW0_TYPE                 0x0000001F  /* Message type */
+#define PCIE_VM_MSG_DW0_TYPE_S               0
+#define PCIE_VM_MSG_DW0_FORMAT               0x00000060  /* Format */
+#define PCIE_VM_MSG_DW0_FORMAT_S             5
+#define PCIE_VM_MSG_DW0_TC                   0x00007000  /* Traffic Class */
+#define PCIE_VM_MSG_DW0_TC_S                 12
+#define PCIE_VM_MSG_DW0_ATTR                 0x000C0000  /* Atrributes */
+#define PCIE_VM_MSG_DW0_ATTR_S               18
+#define PCIE_VM_MSG_DW0_EP_TLP               0x00100000  /* Poisoned TLP */
+#define PCIE_VM_MSG_DW0_TD                   0x00200000  /* TLP Digest */
+#define PCIE_VM_MSG_DW0_LEN                  0xFFC00000  /* Length */
+#define PCIE_VM_MSG_DW0_LEN_S                22
+
+/* Format Definition */
+enum {
+    PCIE_VM_MSG_FORMAT_00 = 0,  /* 3DW Hdr, no data*/
+    PCIE_VM_MSG_FORMAT_01,      /* 4DW Hdr, no data */
+    PCIE_VM_MSG_FORMAT_10,      /* 3DW Hdr, with data */
+    PCIE_VM_MSG_FORMAT_11,      /* 4DW Hdr, with data */
+};
+
+/* Traffic Class Definition */
+enum {
+    PCIE_VM_MSG_TC0 = 0,
+    PCIE_VM_MSG_TC1,
+    PCIE_VM_MSG_TC2,
+    PCIE_VM_MSG_TC3,
+    PCIE_VM_MSG_TC4,
+    PCIE_VM_MSG_TC5,
+    PCIE_VM_MSG_TC6,
+    PCIE_VM_MSG_TC7,
+};
+
+/* Attributes Definition */
+enum {
+    PCIE_VM_MSG_ATTR_00 = 0,   /* RO and No Snoop cleared */
+    PCIE_VM_MSG_ATTR_01,       /* RO cleared , No Snoop set */
+    PCIE_VM_MSG_ATTR_10,       /* RO set, No Snoop cleared*/
+    PCIE_VM_MSG_ATTR_11,       /* RO and No Snoop set */
+};
+
+/* Payload Size Definition */
+#define PCIE_VM_MSG_LEN_MIN  0
+#define PCIE_VM_MSG_LEN_MAX  1024
+
+/* Vendor Message DW1 Register */
+#define PCIE_VM_MSG_DW1(X)                 (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x54)
+#define PCIE_VM_MSG_DW1_FUNC_NUM            0x00000070  /* Function Number */
+#define PCIE_VM_MSG_DW1_FUNC_NUM_S          8
+#define PCIE_VM_MSG_DW1_CODE                0x00FF0000  /* Message Code */
+#define PCIE_VM_MSG_DW1_CODE_S              16
+#define PCIE_VM_MSG_DW1_TAG                 0xFF000000  /* Tag */
+#define PCIE_VM_MSG_DW1_TAG_S               24
+
+#define PCIE_VM_MSG_DW2(X)                  (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x58)
+#define PCIE_VM_MSG_DW3(X)                  (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x5C)
+
+/* Vendor Message Request Register */
+#define PCIE_VM_MSG_REQR(X)                 (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x60)
+#define PCIE_VM_MSG_REQR_REQ                 0x00000001  /* Vendor Message Request */
+
+
+/* AHB Slave Side Band Control Register */
+#define PCIE_AHB_SSB(X)                     (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x70)
+#define PCIE_AHB_SSB_REQ_BCM                0x00000001 /* Slave Reques BCM filed */
+#define PCIE_AHB_SSB_REQ_EP                 0x00000002 /* Slave Reques EP filed */
+#define PCIE_AHB_SSB_REQ_TD                 0x00000004 /* Slave Reques TD filed */
+#define PCIE_AHB_SSB_REQ_ATTR               0x00000018 /* Slave Reques Attribute number */
+#define PCIE_AHB_SSB_REQ_ATTR_S             3
+#define PCIE_AHB_SSB_REQ_TC                 0x000000E0 /* Slave Request TC Field */
+#define PCIE_AHB_SSB_REQ_TC_S               5
+
+/* AHB Master SideBand Ctrl Register */
+#define PCIE_AHB_MSB(X)                     (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x74)
+#define PCIE_AHB_MSB_RESP_ATTR               0x00000003 /* Master Response Attribute number */
+#define PCIE_AHB_MSB_RESP_ATTR_S             0
+#define PCIE_AHB_MSB_RESP_BAD_EOT            0x00000004 /* Master Response Badeot filed */
+#define PCIE_AHB_MSB_RESP_BCM                0x00000008 /* Master Response BCM filed */
+#define PCIE_AHB_MSB_RESP_EP                 0x00000010 /* Master Response EP filed */
+#define PCIE_AHB_MSB_RESP_TD                 0x00000020 /* Master Response TD filed */
+#define PCIE_AHB_MSB_RESP_FUN_NUM            0x000003C0 /* Master Response Function number */
+#define PCIE_AHB_MSB_RESP_FUN_NUM_S          6
+
+/* AHB Control Register, fixed bus enumeration exception */
+#define PCIE_AHB_CTRL(X)                     (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0x78)
+#define PCIE_AHB_CTRL_BUS_ERROR_SUPPRESS     0x00000001 
+
+/* Interrupt Enalbe Register */
+#define PCIE_IRNEN(X)                        (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0xF4)
+#define PCIE_IRNCR(X)                        (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0xF8)
+#define PCIE_IRNICR(X)                       (volatile u32*)(PCIE_APP_PORT_TO_BASE(X) + 0xFC)
+
+/* PCIe interrupt enable/control/capture register definition */
+#define PCIE_IRN_AER_REPORT                 0x00000001  /* AER Interrupt */
+#define PCIE_IRN_AER_MSIX                   0x00000002  /* Advanced Error MSI-X Interrupt */
+#define PCIE_IRN_PME                        0x00000004  /* PME Interrupt */
+#define PCIE_IRN_HOTPLUG                    0x00000008  /* Hotplug Interrupt */
+#define PCIE_IRN_RX_VDM_MSG                 0x00000010  /* Vendor-Defined Message Interrupt */
+#define PCIE_IRN_RX_CORRECTABLE_ERR_MSG     0x00000020  /* Correctable Error Message Interrupt */
+#define PCIE_IRN_RX_NON_FATAL_ERR_MSG       0x00000040  /* Non-fatal Error Message */
+#define PCIE_IRN_RX_FATAL_ERR_MSG           0x00000080  /* Fatal Error Message */
+#define PCIE_IRN_RX_PME_MSG                 0x00000100  /* PME Message Interrupt */
+#define PCIE_IRN_RX_PME_TURNOFF_ACK         0x00000200  /* PME Turnoff Ack Message Interrupt */
+#define PCIE_IRN_AHB_BR_FATAL_ERR           0x00000400  /* AHB Fatal Error Interrupt */
+#define PCIE_IRN_LINK_AUTO_BW_STATUS        0x00000800  /* Link Auto Bandwidth Status Interrupt */
+#define PCIE_IRN_BW_MGT                     0x00001000  /* Bandwidth Managment Interrupt */
+#define PCIE_IRN_INTA                       0x00002000  /* INTA */
+#define PCIE_IRN_INTB                       0x00004000  /* INTB */
+#define PCIE_IRN_INTC                       0x00008000  /* INTC */
+#define PCIE_IRN_INTD                       0x00010000  /* INTD */
+#define PCIE_IRN_WAKEUP                     0x00020000  /* Wake up Interrupt */
+
+#define PCIE_RC_CORE_COMBINED_INT    (PCIE_IRN_AER_REPORT |  PCIE_IRN_AER_MSIX | PCIE_IRN_PME | \
+                                      PCIE_IRN_HOTPLUG | PCIE_IRN_RX_VDM_MSG | PCIE_IRN_RX_CORRECTABLE_ERR_MSG |\
+                                      PCIE_IRN_RX_NON_FATAL_ERR_MSG | PCIE_IRN_RX_FATAL_ERR_MSG | \
+                                      PCIE_IRN_RX_PME_MSG | PCIE_IRN_RX_PME_TURNOFF_ACK | PCIE_IRN_AHB_BR_FATAL_ERR | \
+                                      PCIE_IRN_LINK_AUTO_BW_STATUS | PCIE_IRN_BW_MGT)
+/* PCIe RC Configuration Register */
+#define PCIE_VDID(X)                (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x00)
+
+/* Bit definition from pci_reg.h */
+#define PCIE_PCICMDSTS(X)           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x04)
+#define PCIE_CCRID(X)               (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x08)
+#define PCIE_CLSLTHTBR(X)           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x0C) /* EP only */
+/* BAR0, BAR1,Only necessary if the bridges implements a device-specific register set or memory buffer */
+#define PCIE_BAR0(X)                (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x10) /* Not used*/
+#define PCIE_BAR1(X)                (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x14) /* Not used */
+
+#define PCIE_BNR(X)                 (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x18) /* Mandatory */
+/* Bus Number Register bits */
+#define PCIE_BNR_PRIMARY_BUS_NUM             0x000000FF
+#define PCIE_BNR_PRIMARY_BUS_NUM_S           0
+#define PCIE_PNR_SECONDARY_BUS_NUM           0x0000FF00
+#define PCIE_PNR_SECONDARY_BUS_NUM_S         8
+#define PCIE_PNR_SUB_BUS_NUM                 0x00FF0000
+#define PCIE_PNR_SUB_BUS_NUM_S               16
+
+/* IO Base/Limit Register bits */
+#define PCIE_IOBLSECS(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x1C)  /* RC only */
+#define PCIE_IOBLSECS_32BIT_IO_ADDR             0x00000001
+#define PCIE_IOBLSECS_IO_BASE_ADDR              0x000000F0
+#define PCIE_IOBLSECS_IO_BASE_ADDR_S            4
+#define PCIE_IOBLSECS_32BIT_IOLIMT              0x00000100
+#define PCIE_IOBLSECS_IO_LIMIT_ADDR             0x0000F000
+#define PCIE_IOBLSECS_IO_LIMIT_ADDR_S           12
+
+/* Non-prefetchable Memory Base/Limit Register bit */
+#define PCIE_MBML(X)                           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x20)  /* RC only */
+#define PCIE_MBML_MEM_BASE_ADDR                 0x0000FFF0
+#define PCIE_MBML_MEM_BASE_ADDR_S               4
+#define PCIE_MBML_MEM_LIMIT_ADDR                0xFFF00000
+#define PCIE_MBML_MEM_LIMIT_ADDR_S              20
+
+/* Prefetchable Memory Base/Limit Register bit */
+#define PCIE_PMBL(X)                           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x24)  /* RC only */
+#define PCIE_PMBL_64BIT_ADDR                    0x00000001
+#define PCIE_PMBL_UPPER_12BIT                   0x0000FFF0
+#define PCIE_PMBL_UPPER_12BIT_S                 4
+#define PCIE_PMBL_E64MA                         0x00010000
+#define PCIE_PMBL_END_ADDR                      0xFFF00000
+#define PCIE_PMBL_END_ADDR_S                    20
+#define PCIE_PMBU32(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x28)  /* RC only */
+#define PCIE_PMLU32(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x2C)  /* RC only */
+
+/* I/O Base/Limit Upper 16 bits register */
+#define PCIE_IO_BANDL(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x30)  /* RC only */
+#define PCIE_IO_BANDL_UPPER_16BIT_IO_BASE        0x0000FFFF
+#define PCIE_IO_BANDL_UPPER_16BIT_IO_BASE_S      0
+#define PCIE_IO_BANDL_UPPER_16BIT_IO_LIMIT       0xFFFF0000
+#define PCIE_IO_BANDL_UPPER_16BIT_IO_LIMIT_S     16
+
+#define PCIE_CPR(X)                            (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x34)
+#define PCIE_EBBAR(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x38)
+
+/* Interrupt and Secondary Bridge Control Register */
+#define PCIE_INTRBCTRL(X)                      (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x3C)
+
+#define PCIE_INTRBCTRL_INT_LINE                 0x000000FF
+#define PCIE_INTRBCTRL_INT_LINE_S               0
+#define PCIE_INTRBCTRL_INT_PIN                  0x0000FF00
+#define PCIE_INTRBCTRL_INT_PIN_S                8
+#define PCIE_INTRBCTRL_PARITY_ERR_RESP_ENABLE   0x00010000    /* #PERR */
+#define PCIE_INTRBCTRL_SERR_ENABLE              0x00020000    /* #SERR */
+#define PCIE_INTRBCTRL_ISA_ENABLE               0x00040000    /* ISA enable, IO 64KB only */
+#define PCIE_INTRBCTRL_VGA_ENABLE               0x00080000    /* VGA enable */
+#define PCIE_INTRBCTRL_VGA_16BIT_DECODE         0x00100000    /* VGA 16bit decode */
+#define PCIE_INTRBCTRL_RST_SECONDARY_BUS        0x00400000    /* Secondary bus rest, hot rest, 1ms */
+/* Others are read only */
+enum {
+    PCIE_INTRBCTRL_INT_NON = 0,
+    PCIE_INTRBCTRL_INTA,
+    PCIE_INTRBCTRL_INTB,
+    PCIE_INTRBCTRL_INTC,
+    PCIE_INTRBCTRL_INTD,
+};
+
+#define PCIE_PM_CAPR(X)                  (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x40)
+
+/* Power Management Control and Status Register */
+#define PCIE_PM_CSR(X)                   (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x44)
+
+#define PCIE_PM_CSR_POWER_STATE           0x00000003   /* Power State */
+#define PCIE_PM_CSR_POWER_STATE_S         0
+#define PCIE_PM_CSR_SW_RST                0x00000008   /* Soft Reset Enabled */
+#define PCIE_PM_CSR_PME_ENABLE            0x00000100   /* PME Enable */
+#define PCIE_PM_CSR_PME_STATUS            0x00008000   /* PME status */
+
+/* MSI Capability Register for EP */
+#define PCIE_MCAPR(X)                    (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x50)
+
+#define PCIE_MCAPR_MSI_CAP_ID             0x000000FF  /* MSI Capability ID */
+#define PCIE_MCAPR_MSI_CAP_ID_S           0
+#define PCIE_MCAPR_MSI_NEXT_CAP_PTR       0x0000FF00  /* Next Capability Pointer */
+#define PCIE_MCAPR_MSI_NEXT_CAP_PTR_S     8
+#define PCIE_MCAPR_MSI_ENABLE             0x00010000  /* MSI Enable */
+#define PCIE_MCAPR_MULTI_MSG_CAP          0x000E0000  /* Multiple Message Capable */
+#define PCIE_MCAPR_MULTI_MSG_CAP_S        17
+#define PCIE_MCAPR_MULTI_MSG_ENABLE       0x00700000  /* Multiple Message Enable */
+#define PCIE_MCAPR_MULTI_MSG_ENABLE_S     20
+#define PCIE_MCAPR_ADDR64_CAP             0X00800000  /* 64-bit Address Capable */
+
+/* MSI Message Address Register */
+#define PCIE_MA(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x54)
+
+#define PCIE_MA_ADDR_MASK                 0xFFFFFFFC  /* Message Address */
+
+/* MSI Message Upper Address Register */
+#define PCIE_MUA(X)                      (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x58)
+
+/* MSI Message Data Register */
+#define PCIE_MD(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x5C)
+
+#define PCIE_MD_DATA                      0x0000FFFF  /* Message Data */
+#define PCIE_MD_DATA_S                    0
+
+/* PCI Express Capability Register */
+#define PCIE_XCAP(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x70)
+
+#define PCIE_XCAP_ID                      0x000000FF  /* PCI Express Capability ID */
+#define PCIE_XCAP_ID_S                    0
+#define PCIE_XCAP_NEXT_CAP                0x0000FF00  /* Next Capability Pointer */
+#define PCIE_XCAP_NEXT_CAP_S              8
+#define PCIE_XCAP_VER                     0x000F0000  /* PCI Express Capability Version */
+#define PCIE_XCAP_VER_S                   16
+#define PCIE_XCAP_DEV_PORT_TYPE           0x00F00000  /* Device Port Type */
+#define PCIE_XCAP_DEV_PORT_TYPE_S         20
+#define PCIE_XCAP_SLOT_IMPLEMENTED        0x01000000  /* Slot Implemented */
+#define PCIE_XCAP_MSG_INT_NUM             0x3E000000  /* Interrupt Message Number */
+#define PCIE_XCAP_MSG_INT_NUM_S           25
+
+/* Device Capability Register */
+#define PCIE_DCAP(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x74)
+
+#define PCIE_DCAP_MAX_PAYLOAD_SIZE        0x00000007   /* Max Payload size */
+#define PCIE_DCAP_MAX_PAYLOAD_SIZE_S      0
+#define PCIE_DCAP_PHANTOM_FUNC            0x00000018   /* Phanton Function, not supported */
+#define PCIE_DCAP_PHANTOM_FUNC_S          3
+#define PCIE_DCAP_EXT_TAG                 0x00000020   /* Extended Tag Field */
+#define PCIE_DCAP_EP_L0S_LATENCY          0x000001C0   /* EP L0s latency only */
+#define PCIE_DCAP_EP_L0S_LATENCY_S        6
+#define PCIE_DCAP_EP_L1_LATENCY           0x00000E00   /* EP L1 latency only */
+#define PCIE_DCAP_EP_L1_LATENCY_S         9
+#define PCIE_DCAP_ROLE_BASE_ERR_REPORT    0x00008000   /* Role Based ERR */
+
+/* Maximum payload size supported */
+enum {
+    PCIE_MAX_PAYLOAD_128 = 0,
+    PCIE_MAX_PAYLOAD_256,
+    PCIE_MAX_PAYLOAD_512,
+    PCIE_MAX_PAYLOAD_1024,
+    PCIE_MAX_PAYLOAD_2048,
+    PCIE_MAX_PAYLOAD_4096,
+};
+
+/* Device Control and Status Register */
+#define PCIE_DCTLSTS(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x78)
+
+#define PCIE_DCTLSTS_CORRECTABLE_ERR_EN        0x00000001   /* COR-ERR */
+#define PCIE_DCTLSTS_NONFATAL_ERR_EN           0x00000002   /* Non-fatal ERR */
+#define PCIE_DCTLSTS_FATAL_ERR_EN              0x00000004   /* Fatal ERR */
+#define PCIE_DCTLSYS_UR_REQ_EN                 0x00000008   /* UR ERR */
+#define PCIE_DCTLSTS_RELAXED_ORDERING_EN       0x00000010   /* Enable relaxing ordering */
+#define PCIE_DCTLSTS_MAX_PAYLOAD_SIZE          0x000000E0   /* Max payload mask */
+#define PCIE_DCTLSTS_MAX_PAYLOAD_SIZE_S        5
+#define PCIE_DCTLSTS_EXT_TAG_EN                0x00000100   /* Extended tag field */
+#define PCIE_DCTLSTS_PHANTOM_FUNC_EN           0x00000200   /* Phantom Function Enable */
+#define PCIE_DCTLSTS_AUX_PM_EN                 0x00000400   /* AUX Power PM Enable */
+#define PCIE_DCTLSTS_NO_SNOOP_EN               0x00000800   /* Enable no snoop, except root port*/
+#define PCIE_DCTLSTS_MAX_READ_SIZE             0x00007000   /* Max Read Request size*/
+#define PCIE_DCTLSTS_MAX_READ_SIZE_S           12
+#define PCIE_DCTLSTS_CORRECTABLE_ERR           0x00010000   /* COR-ERR Detected */
+#define PCIE_DCTLSTS_NONFATAL_ERR              0x00020000   /* Non-Fatal ERR Detected */
+#define PCIE_DCTLSTS_FATAL_ER                  0x00040000   /* Fatal ERR Detected */
+#define PCIE_DCTLSTS_UNSUPPORTED_REQ           0x00080000   /* UR Detected */
+#define PCIE_DCTLSTS_AUX_POWER                 0x00100000   /* Aux Power Detected */
+#define PCIE_DCTLSTS_TRANSACT_PENDING          0x00200000   /* Transaction pending */
+
+#define PCIE_DCTLSTS_ERR_EN      (PCIE_DCTLSTS_CORRECTABLE_ERR_EN | \
+                                  PCIE_DCTLSTS_NONFATAL_ERR_EN | PCIE_DCTLSTS_FATAL_ERR_EN | \
+                                  PCIE_DCTLSYS_UR_REQ_EN)
+
+/* Link Capability Register */
+#define PCIE_LCAP(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x7C)
+#define PCIE_LCAP_MAX_LINK_SPEED               0x0000000F  /* Max link speed, 0x1 by default */
+#define PCIE_LCAP_MAX_LINK_SPEED_S             0
+#define PCIE_LCAP_MAX_LENGTH_WIDTH             0x000003F0  /* Maxium Length Width */
+#define PCIE_LCAP_MAX_LENGTH_WIDTH_S           4
+#define PCIE_LCAP_ASPM_LEVEL                   0x00000C00  /* Active State Link PM Support */
+#define PCIE_LCAP_ASPM_LEVEL_S                 10
+#define PCIE_LCAP_L0S_EIXT_LATENCY             0x00007000  /* L0s Exit Latency */
+#define PCIE_LCAP_L0S_EIXT_LATENCY_S           12
+#define PCIE_LCAP_L1_EXIT_LATENCY              0x00038000  /* L1 Exit Latency */
+#define PCIE_LCAP_L1_EXIT_LATENCY_S            15
+#define PCIE_LCAP_CLK_PM                       0x00040000  /* Clock Power Management */
+#define PCIE_LCAP_SDER                         0x00080000  /* Surprise Down Error Reporting */
+#define PCIE_LCAP_DLL_ACTIVE_REPROT            0x00100000  /* Data Link Layer Active Reporting Capable */
+#define PCIE_LCAP_PORT_NUM                     0xFF0000000  /* Port number */
+#define PCIE_LCAP_PORT_NUM_S                   24
+
+/* Maximum Length width definition */
+#define PCIE_MAX_LENGTH_WIDTH_RES  0x00
+#define PCIE_MAX_LENGTH_WIDTH_X1   0x01  /* Default */
+#define PCIE_MAX_LENGTH_WIDTH_X2   0x02
+#define PCIE_MAX_LENGTH_WIDTH_X4   0x04
+#define PCIE_MAX_LENGTH_WIDTH_X8   0x08
+#define PCIE_MAX_LENGTH_WIDTH_X12  0x0C
+#define PCIE_MAX_LENGTH_WIDTH_X16  0x10
+#define PCIE_MAX_LENGTH_WIDTH_X32  0x20
+
+/* Active State Link PM definition */
+enum {
+    PCIE_ASPM_RES0                = 0,
+    PCIE_ASPM_L0S_ENTRY_SUPPORT,        /* L0s */
+    PCIE_ASPM_RES1,
+    PCIE_ASPM_L0S_L1_ENTRY_SUPPORT,     /* L0s and L1, default */
+};
+
+/* L0s Exit Latency definition */
+enum {
+    PCIE_L0S_EIXT_LATENCY_L64NS    = 0, /* < 64 ns */
+    PCIE_L0S_EIXT_LATENCY_B64A128,      /* > 64 ns < 128 ns */
+    PCIE_L0S_EIXT_LATENCY_B128A256,     /* > 128 ns < 256 ns */
+    PCIE_L0S_EIXT_LATENCY_B256A512,     /* > 256 ns < 512 ns */
+    PCIE_L0S_EIXT_LATENCY_B512TO1U,     /* > 512 ns < 1 us */
+    PCIE_L0S_EIXT_LATENCY_B1A2U,        /* > 1 us < 2 us */
+    PCIE_L0S_EIXT_LATENCY_B2A4U,        /* > 2 us < 4 us */
+    PCIE_L0S_EIXT_LATENCY_M4US,         /* > 4 us  */
+};
+
+/* L1 Exit Latency definition */
+enum {
+    PCIE_L1_EXIT_LATENCY_L1US  = 0,  /* < 1 us */
+    PCIE_L1_EXIT_LATENCY_B1A2,       /* > 1 us < 2 us */
+    PCIE_L1_EXIT_LATENCY_B2A4,       /* > 2 us < 4 us */
+    PCIE_L1_EXIT_LATENCY_B4A8,       /* > 4 us < 8 us */
+    PCIE_L1_EXIT_LATENCY_B8A16,      /* > 8 us < 16 us */
+    PCIE_L1_EXIT_LATENCY_B16A32,     /* > 16 us < 32 us */
+    PCIE_L1_EXIT_LATENCY_B32A64,     /* > 32 us < 64 us */
+    PCIE_L1_EXIT_LATENCY_M64US,      /* > 64 us */
+};
+
+/* Link Control and Status Register */
+#define PCIE_LCTLSTS(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x80)
+#define PCIE_LCTLSTS_ASPM_ENABLE            0x00000003  /* Active State Link PM Control */
+#define PCIE_LCTLSTS_ASPM_ENABLE_S          0
+#define PCIE_LCTLSTS_RCB128                 0x00000008  /* Read Completion Boundary 128*/
+#define PCIE_LCTLSTS_LINK_DISABLE           0x00000010  /* Link Disable */
+#define PCIE_LCTLSTS_RETRIAN_LINK           0x00000020  /* Retrain Link */
+#define PCIE_LCTLSTS_COM_CLK_CFG            0x00000040  /* Common Clock Configuration */
+#define PCIE_LCTLSTS_EXT_SYNC               0x00000080  /* Extended Synch */
+#define PCIE_LCTLSTS_CLK_PM_EN              0x00000100  /* Enable Clock Powerm Management */
+#define PCIE_LCTLSTS_LINK_SPEED             0x000F0000  /* Link Speed */
+#define PCIE_LCTLSTS_LINK_SPEED_S           16
+#define PCIE_LCTLSTS_NEGOTIATED_LINK_WIDTH  0x03F00000  /* Negotiated Link Width */
+#define PCIE_LCTLSTS_NEGOTIATED_LINK_WIDTH_S 20
+#define PCIE_LCTLSTS_RETRAIN_PENDING        0x08000000  /* Link training is ongoing */
+#define PCIE_LCTLSTS_SLOT_CLK_CFG           0x10000000  /* Slot Clock Configuration */
+#define PCIE_LCTLSTS_DLL_ACTIVE             0x20000000  /* Data Link Layer Active */
+
+/* Slot Capabilities Register */
+#define PCIE_SLCAP(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x84)
+
+/* Slot Capabilities */
+#define PCIE_SLCTLSTS(X)                    (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x88)
+
+/* Root Control and Capability Register */
+#define PCIE_RCTLCAP(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x8C)
+#define PCIE_RCTLCAP_SERR_ON_CORRECTABLE_ERR  0x00000001   /* #SERR on COR-ERR */
+#define PCIE_RCTLCAP_SERR_ON_NONFATAL_ERR     0x00000002   /* #SERR on Non-Fatal ERR */
+#define PCIE_RCTLCAP_SERR_ON_FATAL_ERR        0x00000004   /* #SERR on Fatal ERR */
+#define PCIE_RCTLCAP_PME_INT_EN               0x00000008   /* PME Interrupt Enable */
+#define PCIE_RCTLCAP_SERR_ENABLE    (PCIE_RCTLCAP_SERR_ON_CORRECTABLE_ERR | \
+                                     PCIE_RCTLCAP_SERR_ON_NONFATAL_ERR | PCIE_RCTLCAP_SERR_ON_FATAL_ERR)
+/* Root Status Register */
+#define PCIE_RSTS(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x90)
+#define PCIE_RSTS_PME_REQ_ID                   0x0000FFFF   /* PME Request ID */
+#define PCIE_RSTS_PME_REQ_ID_S                 0
+#define PCIE_RSTS_PME_STATUS                   0x00010000   /* PME Status */
+#define PCIE_RSTS_PME_PENDING                  0x00020000   /* PME Pending */
+
+/* PCI Express Enhanced Capability Header */
+#define PCIE_ENHANCED_CAP(X)                (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x100)
+#define PCIE_ENHANCED_CAP_ID                 0x0000FFFF  /* PCI Express Extended Capability ID */
+#define PCIE_ENHANCED_CAP_ID_S               0
+#define PCIE_ENHANCED_CAP_VER                0x000F0000  /* Capability Version */
+#define PCIE_ENHANCED_CAP_VER_S              16
+#define PCIE_ENHANCED_CAP_NEXT_OFFSET        0xFFF00000  /* Next Capability Offset */
+#define PCIE_ENHANCED_CAP_NEXT_OFFSET_S      20
+
+/* Uncorrectable Error Status Register */
+#define PCIE_UES_R(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x104)
+#define PCIE_DATA_LINK_PROTOCOL_ERR          0x00000010  /* Data Link Protocol Error Status */
+#define PCIE_SURPRISE_DOWN_ERROR             0x00000020  /* Surprise Down Error Status */
+#define PCIE_POISONED_TLP                    0x00001000  /* Poisoned TLP Status */
+#define PCIE_FC_PROTOCOL_ERR                 0x00002000  /* Flow Control Protocol Error Status */
+#define PCIE_COMPLETION_TIMEOUT              0x00004000  /* Completion Timeout Status */
+#define PCIE_COMPLETOR_ABORT                 0x00008000  /* Completer Abort Error */
+#define PCIE_UNEXPECTED_COMPLETION           0x00010000  /* Unexpected Completion Status */
+#define PCIE_RECEIVER_OVERFLOW               0x00020000  /* Receive Overflow Status */
+#define PCIE_MALFORNED_TLP                   0x00040000  /* Malformed TLP Stauts */
+#define PCIE_ECRC_ERR                        0x00080000  /* ECRC Error Stauts */
+#define PCIE_UR_REQ                          0x00100000  /* Unsupported Request Error Status */
+#define PCIE_ALL_UNCORRECTABLE_ERR    (PCIE_DATA_LINK_PROTOCOL_ERR | PCIE_SURPRISE_DOWN_ERROR | \
+                         PCIE_POISONED_TLP | PCIE_FC_PROTOCOL_ERR | PCIE_COMPLETION_TIMEOUT |   \
+                         PCIE_COMPLETOR_ABORT | PCIE_UNEXPECTED_COMPLETION | PCIE_RECEIVER_OVERFLOW |\
+                         PCIE_MALFORNED_TLP | PCIE_ECRC_ERR | PCIE_UR_REQ)
+
+/* Uncorrectable Error Mask Register, Mask means no report */
+#define PCIE_UEMR(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x108)
+
+/* Uncorrectable Error Severity Register */
+#define PCIE_UESR(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x10C)
+
+/* Correctable Error Status Register */
+#define PCIE_CESR(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x110)
+#define PCIE_RX_ERR                          0x00000001  /* Receive Error Status */
+#define PCIE_BAD_TLP                         0x00000040  /* Bad TLP Status */
+#define PCIE_BAD_DLLP                        0x00000080  /* Bad DLLP Status */
+#define PCIE_REPLAY_NUM_ROLLOVER             0x00000100  /* Replay Number Rollover Status */
+#define PCIE_REPLAY_TIMER_TIMEOUT_ERR        0x00001000  /* Reply Timer Timeout Status */
+#define PCIE_ADVISORY_NONFTAL_ERR            0x00002000  /* Advisory Non-Fatal Error Status */
+#define PCIE_CORRECTABLE_ERR        (PCIE_RX_ERR | PCIE_BAD_TLP | PCIE_BAD_DLLP | PCIE_REPLAY_NUM_ROLLOVER |\
+                                     PCIE_REPLAY_TIMER_TIMEOUT_ERR | PCIE_ADVISORY_NONFTAL_ERR)
+
+/* Correctable Error Mask Register */
+#define PCIE_CEMR(X)                        (volatile u32*)(PCIE_RC_CFG_BASE + 0x114)
+
+/* Advanced Error Capabilities and Control Register */
+#define PCIE_AECCR(X)                       (volatile u32*)(PCIE_RC_CFG_BASE + 0x118)
+#define PCIE_AECCR_FIRST_ERR_PTR            0x0000001F  /* First Error Pointer */
+#define PCIE_AECCR_FIRST_ERR_PTR_S          0
+#define PCIE_AECCR_ECRC_GEN_CAP             0x00000020  /* ECRC Generation Capable */
+#define PCIE_AECCR_ECRC_GEN_EN              0x00000040  /* ECRC Generation Enable */
+#define PCIE_AECCR_ECRC_CHECK_CAP           0x00000080  /* ECRC Check Capable */
+#define PCIE_AECCR_ECRC_CHECK_EN            0x00000100  /* ECRC Check Enable */
+
+/* Header Log Register 1 */
+#define PCIE_HLR1(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x11C)
+
+/* Header Log Register 2 */
+#define PCIE_HLR2(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x120)
+
+/* Header Log Register 3 */
+#define PCIE_HLR3(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x124)
+
+/* Header Log Register 4 */
+#define PCIE_HLR4(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x128)
+
+/* Root Error Command Register */
+#define PCIE_RECR(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x12C)
+#define PCIE_RECR_CORRECTABLE_ERR_REPORT_EN  0x00000001 /* COR-ERR */
+#define PCIE_RECR_NONFATAL_ERR_REPORT_EN     0x00000002 /* Non-Fatal ERR */
+#define PCIE_RECR_FATAL_ERR_REPORT_EN        0x00000004 /* Fatal ERR */
+#define PCIE_RECR_ERR_REPORT_EN  (PCIE_RECR_CORRECTABLE_ERR_REPORT_EN | \
+                PCIE_RECR_NONFATAL_ERR_REPORT_EN | PCIE_RECR_FATAL_ERR_REPORT_EN)
+
+/* Root Error Status Register */
+#define PCIE_RESR(X)                            (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x130)
+#define PCIE_RESR_CORRECTABLE_ERR                0x00000001   /* COR-ERR Receveid */
+#define PCIE_RESR_MULTI_CORRECTABLE_ERR          0x00000002   /* Multiple COR-ERR Received */
+#define PCIE_RESR_FATAL_NOFATAL_ERR              0x00000004   /* ERR Fatal/Non-Fatal Received */
+#define PCIE_RESR_MULTI_FATAL_NOFATAL_ERR        0x00000008   /* Multiple ERR Fatal/Non-Fatal Received */
+#define PCIE_RESR_FIRST_UNCORRECTABLE_FATAL_ERR  0x00000010   /* First UN-COR Fatal */
+#define PCIR_RESR_NON_FATAL_ERR                  0x00000020   /* Non-Fatal Error Message Received */
+#define PCIE_RESR_FATAL_ERR                      0x00000040   /* Fatal Message Received */
+#define PCIE_RESR_AER_INT_MSG_NUM                0xF8000000   /* Advanced Error Interrupt Message Number */
+#define PCIE_RESR_AER_INT_MSG_NUM_S              27
+
+/* Error Source Indentification Register */
+#define PCIE_ESIR(X)                            (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x134)
+#define PCIE_ESIR_CORRECTABLE_ERR_SRC_ID         0x0000FFFF
+#define PCIE_ESIR_CORRECTABLE_ERR_SRC_ID_S       0
+#define PCIE_ESIR_FATAL_NON_FATAL_SRC_ID         0xFFFF0000
+#define PCIE_ESIR_FATAL_NON_FATAL_SRC_ID_S       16
+
+/* VC Enhanced Capability Header */
+#define PCIE_VC_ECH(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x140)
+
+/* Port VC Capability Register */
+#define PCIE_PVC1(X)                            (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x144)
+#define PCIE_PVC1_EXT_VC_CNT                    0x00000007  /* Extended VC Count */
+#define PCIE_PVC1_EXT_VC_CNT_S                  0
+#define PCIE_PVC1_LOW_PRI_EXT_VC_CNT            0x00000070  /* Low Priority Extended VC Count */
+#define PCIE_PVC1_LOW_PRI_EXT_VC_CNT_S          4
+#define PCIE_PVC1_REF_CLK                       0x00000300  /* Reference Clock */
+#define PCIE_PVC1_REF_CLK_S                     8
+#define PCIE_PVC1_PORT_ARB_TAB_ENTRY_SIZE       0x00000C00  /* Port Arbitration Table Entry Size */
+#define PCIE_PVC1_PORT_ARB_TAB_ENTRY_SIZE_S     10
+
+/* Extended Virtual Channel Count Defintion */
+#define PCIE_EXT_VC_CNT_MIN   0
+#define PCIE_EXT_VC_CNT_MAX   7
+
+/* Port Arbitration Table Entry Size Definition */
+enum {
+    PCIE_PORT_ARB_TAB_ENTRY_SIZE_S1BIT = 0,
+    PCIE_PORT_ARB_TAB_ENTRY_SIZE_S2BIT,
+    PCIE_PORT_ARB_TAB_ENTRY_SIZE_S4BIT,
+    PCIE_PORT_ARB_TAB_ENTRY_SIZE_S8BIT,
+};
+
+/* Port VC Capability Register 2 */
+#define PCIE_PVC2(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x148)
+#define PCIE_PVC2_VC_ARB_16P_FIXED_WRR      0x00000001  /* HW Fixed arbitration, 16 phase WRR */
+#define PCIE_PVC2_VC_ARB_32P_WRR            0x00000002  /* 32 phase WRR */
+#define PCIE_PVC2_VC_ARB_64P_WRR            0x00000004  /* 64 phase WRR */
+#define PCIE_PVC2_VC_ARB_128P_WRR           0x00000008  /* 128 phase WRR */
+#define PCIE_PVC2_VC_ARB_WRR                0x0000000F
+#define PCIE_PVC2_VC_ARB_TAB_OFFSET         0xFF000000  /* VC arbitration table offset, not support */
+#define PCIE_PVC2_VC_ARB_TAB_OFFSET_S       24
+
+/* Port VC Control and Status Register */     
+#define PCIE_PVCCRSR(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x14C)
+#define PCIE_PVCCRSR_LOAD_VC_ARB_TAB         0x00000001  /* Load VC Arbitration Table */
+#define PCIE_PVCCRSR_VC_ARB_SEL              0x0000000E  /* VC Arbitration Select */
+#define PCIE_PVCCRSR_VC_ARB_SEL_S            1
+#define PCIE_PVCCRSR_VC_ARB_TAB_STATUS       0x00010000  /* Arbitration Status */
+
+/* VC0 Resource Capability Register */
+#define PCIE_VC0_RC(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x150)
+#define PCIE_VC0_RC_PORT_ARB_HW_FIXED        0x00000001  /* HW Fixed arbitration */
+#define PCIE_VC0_RC_PORT_ARB_32P_WRR         0x00000002  /* 32 phase WRR */
+#define PCIE_VC0_RC_PORT_ARB_64P_WRR         0x00000004  /* 64 phase WRR */
+#define PCIE_VC0_RC_PORT_ARB_128P_WRR        0x00000008  /* 128 phase WRR */
+#define PCIE_VC0_RC_PORT_ARB_TM_128P_WRR     0x00000010  /* Time-based 128 phase WRR */
+#define PCIE_VC0_RC_PORT_ARB_TM_256P_WRR     0x00000020  /* Time-based 256 phase WRR */
+#define PCIE_VC0_RC_PORT_ARB          (PCIE_VC0_RC_PORT_ARB_HW_FIXED | PCIE_VC0_RC_PORT_ARB_32P_WRR |\
+                        PCIE_VC0_RC_PORT_ARB_64P_WRR | PCIE_VC0_RC_PORT_ARB_128P_WRR | \
+                        PCIE_VC0_RC_PORT_ARB_TM_128P_WRR | PCIE_VC0_RC_PORT_ARB_TM_256P_WRR)
+
+#define PCIE_VC0_RC_REJECT_SNOOP             0x00008000  /* Reject Snoop Transactioin */
+#define PCIE_VC0_RC_MAX_TIMESLOTS            0x007F0000  /* Maximum time Slots */
+#define PCIE_VC0_RC_MAX_TIMESLOTS_S          16
+#define PCIE_VC0_RC_PORT_ARB_TAB_OFFSET      0xFF000000  /* Port Arbitration Table Offset */
+#define PCIE_VC0_RC_PORT_ARB_TAB_OFFSET_S    24
+
+/* VC0 Resource Control Register */
+#define PCIE_VC0_RC0(X)                      (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x154)
+#define PCIE_VC0_RC0_TVM0                    0x00000001  /* TC0 and VC0 */
+#define PCIE_VC0_RC0_TVM1                    0x00000002  /* TC1 and VC1 */
+#define PCIE_VC0_RC0_TVM2                    0x00000004  /* TC2 and VC2 */
+#define PCIE_VC0_RC0_TVM3                    0x00000008  /* TC3 and VC3 */
+#define PCIE_VC0_RC0_TVM4                    0x00000010  /* TC4 and VC4 */
+#define PCIE_VC0_RC0_TVM5                    0x00000020  /* TC5 and VC5 */
+#define PCIE_VC0_RC0_TVM6                    0x00000040  /* TC6 and VC6 */
+#define PCIE_VC0_RC0_TVM7                    0x00000080  /* TC7 and VC7 */
+#define PCIE_VC0_RC0_TC_VC                   0x000000FF  /* TC/VC mask */
+
+#define PCIE_VC0_RC0_LOAD_PORT_ARB_TAB       0x00010000  /* Load Port Arbitration Table */
+#define PCIE_VC0_RC0_PORT_ARB_SEL            0x000E0000  /* Port Arbitration Select */
+#define PCIE_VC0_RC0_PORT_ARB_SEL_S          17
+#define PCIE_VC0_RC0_VC_ID                   0x07000000  /* VC ID */
+#define PCIE_VC0_RC0_VC_ID_S                 24
+#define PCIE_VC0_RC0_VC_EN                   0x80000000  /* VC Enable */
+
+/* VC0 Resource Status Register */
+#define PCIE_VC0_RSR0(X)                     (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x158)
+#define PCIE_VC0_RSR0_PORT_ARB_TAB_STATUS    0x00010000  /* Port Arbitration Table Status,not used */
+#define PCIE_VC0_RSR0_VC_NEG_PENDING         0x00020000  /* VC Negotiation Pending */
+
+/* Ack Latency Timer and Replay Timer Register */
+#define PCIE_ALTRT(X)                         (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x700)
+#define PCIE_ALTRT_ROUND_TRIP_LATENCY_LIMIT   0x0000FFFF  /* Round Trip Latency Time Limit */
+#define PCIE_ALTRT_ROUND_TRIP_LATENCY_LIMIT_S 0
+#define PCIE_ALTRT_REPLAY_TIME_LIMIT          0xFFFF0000  /* Replay Time Limit */
+#define PCIE_ALTRT_REPLAY_TIME_LIMIT_S        16
+
+/* Other Message Register */
+#define PCIE_OMR(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x704)
+
+/* Port Force Link Register */
+#define PCIE_PFLR(X)                         (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x708)
+#define PCIE_PFLR_LINK_NUM                   0x000000FF  /* Link Number */
+#define PCIE_PFLR_LINK_NUM_S                 0
+#define PCIE_PFLR_FORCE_LINK                 0x00008000  /* Force link */
+#define PCIE_PFLR_LINK_STATE                 0x003F0000  /* Link State */
+#define PCIE_PFLR_LINK_STATE_S               16
+#define PCIE_PFLR_LOW_POWER_ENTRY_CNT        0xFF000000  /* Low Power Entrance Count, only for EP */
+#define PCIE_PFLR_LOW_POWER_ENTRY_CNT_S      24
+
+/* Ack Frequency Register */
+#define PCIE_AFR(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x70C)
+#define PCIE_AFR_AF                          0x000000FF  /* Ack Frequency */
+#define PCIE_AFR_AF_S                        0
+#define PCIE_AFR_FTS_NUM                     0x0000FF00  /* The number of Fast Training Sequence from L0S to L0 */
+#define PCIE_AFR_FTS_NUM_S                   8
+#define PCIE_AFR_COM_FTS_NUM                 0x00FF0000  /* N_FTS; when common clock is used*/
+#define PCIE_AFR_COM_FTS_NUM_S               16
+#define PCIE_AFR_L0S_ENTRY_LATENCY           0x07000000  /* L0s Entrance Latency */
+#define PCIE_AFR_L0S_ENTRY_LATENCY_S         24
+#define PCIE_AFR_L1_ENTRY_LATENCY            0x38000000  /* L1 Entrance Latency */
+#define PCIE_AFR_L1_ENTRY_LATENCY_S          27
+#define PCIE_AFR_FTS_NUM_DEFAULT             32
+#define PCIE_AFR_L0S_ENTRY_LATENCY_DEFAULT   7
+#define PCIE_AFR_L1_ENTRY_LATENCY_DEFAULT    5
+
+/* Port Link Control Register */
+#define PCIE_PLCR(X)                         (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x710)
+#define PCIE_PLCR_OTHER_MSG_REQ              0x00000001  /* Other Message Request */
+#define PCIE_PLCR_SCRAMBLE_DISABLE           0x00000002  /* Scramble Disable */  
+#define PCIE_PLCR_LOOPBACK_EN                0x00000004  /* Loopback Enable */
+#define PCIE_PLCR_LTSSM_HOT_RST              0x00000008  /* Force LTSSM to the hot reset */
+#define PCIE_PLCR_DLL_LINK_EN                0x00000020  /* Enable Link initialization */
+#define PCIE_PLCR_FAST_LINK_SIM_EN           0x00000080  /* Sets all internal timers to fast mode for simulation purposes */
+#define PCIE_PLCR_LINK_MODE                  0x003F0000  /* Link Mode Enable Mask */
+#define PCIE_PLCR_LINK_MODE_S                16
+#define PCIE_PLCR_CORRUPTED_CRC_EN           0x02000000  /* Enabled Corrupt CRC */
+
+/* Lane Skew Register */
+#define PCIE_LSR(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x714)
+#define PCIE_LSR_LANE_SKEW_NUM               0x00FFFFFF  /* Insert Lane Skew for Transmit, not applicable */
+#define PCIE_LSR_LANE_SKEW_NUM_S             0
+#define PCIE_LSR_FC_DISABLE                  0x01000000  /* Disable of Flow Control */
+#define PCIE_LSR_ACKNAK_DISABLE              0x02000000  /* Disable of Ack/Nak */
+#define PCIE_LSR_LANE_DESKEW_DISABLE         0x80000000  /* Disable of Lane-to-Lane Skew */
+
+/* Symbol Number Register */
+#define PCIE_SNR(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x718)
+#define PCIE_SNR_TS                          0x0000000F  /* Number of TS Symbol */
+#define PCIE_SNR_TS_S                        0
+#define PCIE_SNR_SKP                         0x00000700  /* Number of SKP Symbol */
+#define PCIE_SNR_SKP_S                       8
+#define PCIE_SNR_REPLAY_TIMER                0x0007C000  /* Timer Modifier for Replay Timer */
+#define PCIE_SNR_REPLAY_TIMER_S              14
+#define PCIE_SNR_ACKNAK_LATENCY_TIMER        0x00F80000  /* Timer Modifier for Ack/Nak Latency Timer */
+#define PCIE_SNR_ACKNAK_LATENCY_TIMER_S      19
+#define PCIE_SNR_FC_TIMER                    0x1F000000  /* Timer Modifier for Flow Control Watchdog Timer */
+#define PCIE_SNR_FC_TIMER_S                  28
+
+/* Symbol Timer Register and Filter Mask Register 1 */
+#define PCIE_STRFMR(X)                      (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x71C)
+#define PCIE_STRFMR_SKP_INTERVAL            0x000007FF  /* SKP lnterval Value */
+#define PCIE_STRFMR_SKP_INTERVAL_S          0
+#define PCIE_STRFMR_FC_WDT_DISABLE          0x00008000  /* Disable of FC Watchdog Timer */
+#define PCIE_STRFMR_TLP_FUNC_MISMATCH_OK    0x00010000  /* Mask Function Mismatch Filtering for Incoming Requests */
+#define PCIE_STRFMR_POISONED_TLP_OK         0x00020000  /* Mask Poisoned TLP Filtering */
+#define PCIE_STRFMR_BAR_MATCH_OK            0x00040000  /* Mask BAR Match Filtering */
+#define PCIE_STRFMR_TYPE1_CFG_REQ_OK        0x00080000  /* Mask Type 1 Configuration Request Filtering */
+#define PCIE_STRFMR_LOCKED_REQ_OK           0x00100000  /* Mask Locked Request Filtering */
+#define PCIE_STRFMR_CPL_TAG_ERR_RULES_OK    0x00200000  /* Mask Tag Error Rules for Received Completions */
+#define PCIE_STRFMR_CPL_REQUESTOR_ID_MISMATCH_OK 0x00400000  /* Mask Requester ID Mismatch Error for Received Completions */
+#define PCIE_STRFMR_CPL_FUNC_MISMATCH_OK         0x00800000  /* Mask Function Mismatch Error for Received Completions */
+#define PCIE_STRFMR_CPL_TC_MISMATCH_OK           0x01000000  /* Mask Traffic Class Mismatch Error for Received Completions */
+#define PCIE_STRFMR_CPL_ATTR_MISMATCH_OK         0x02000000  /* Mask Attribute Mismatch Error for Received Completions */
+#define PCIE_STRFMR_CPL_LENGTH_MISMATCH_OK       0x04000000  /* Mask Length Mismatch Error for Received Completions */
+#define PCIE_STRFMR_TLP_ECRC_ERR_OK              0x08000000  /* Mask ECRC Error Filtering */
+#define PCIE_STRFMR_CPL_TLP_ECRC_OK              0x10000000  /* Mask ECRC Error Filtering for Completions */
+#define PCIE_STRFMR_RX_TLP_MSG_NO_DROP           0x20000000  /* Send Message TLPs */
+#define PCIE_STRFMR_RX_IO_TRANS_ENABLE           0x40000000  /* Mask Filtering of received I/O Requests */
+#define PCIE_STRFMR_RX_CFG_TRANS_ENABLE          0x80000000  /* Mask Filtering of Received Configuration Requests */
+
+#define PCIE_DEF_SKP_INTERVAL    700             /* 1180 ~1538 , 125MHz * 2, 250MHz * 1 */
+
+/* Filter Masker Register 2 */
+#define PCIE_FMR2(X)                             (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x720)
+#define PCIE_FMR2_VENDOR_MSG0_PASSED_TO_TRGT1    0x00000001  /* Mask RADM Filtering and Error Handling Rules */
+#define PCIE_FMR2_VENDOR_MSG1_PASSED_TO_TRGT1    0x00000002  /* Mask RADM Filtering and Error Handling Rules */
+
+/* Debug Register 0 */
+#define PCIE_DBR0(X)                              (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x728)
+
+/* Debug Register 1 */
+#define PCIE_DBR1(X)                              (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x72C)
+
+/* Transmit Posted FC Credit Status Register */
+#define PCIE_TPFCS(X)                             (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x730)
+#define PCIE_TPFCS_TX_P_DATA_FC_CREDITS           0x00000FFF /* Transmit Posted Data FC Credits */
+#define PCIE_TPFCS_TX_P_DATA_FC_CREDITS_S         0
+#define PCIE_TPFCS_TX_P_HDR_FC_CREDITS            0x000FF000 /* Transmit Posted Header FC Credits */
+#define PCIE_TPFCS_TX_P_HDR_FC_CREDITS_S          12
+
+/* Transmit Non-Posted FC Credit Status */
+#define PCIE_TNPFCS(X)                            (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x734)
+#define PCIE_TNPFCS_TX_NP_DATA_FC_CREDITS         0x00000FFF /* Transmit Non-Posted Data FC Credits */
+#define PCIE_TNPFCS_TX_NP_DATA_FC_CREDITS_S       0
+#define PCIE_TNPFCS_TX_NP_HDR_FC_CREDITS          0x000FF000 /* Transmit Non-Posted Header FC Credits */
+#define PCIE_TNPFCS_TX_NP_HDR_FC_CREDITS_S        12
+
+/* Transmit Complete FC Credit Status Register */
+#define PCIE_TCFCS(X)                             (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x738)
+#define PCIE_TCFCS_TX_CPL_DATA_FC_CREDITS         0x00000FFF /* Transmit Completion Data FC Credits */
+#define PCIE_TCFCS_TX_CPL_DATA_FC_CREDITS_S       0
+#define PCIE_TCFCS_TX_CPL_HDR_FC_CREDITS          0x000FF000 /* Transmit Completion Header FC Credits */
+#define PCIE_TCFCS_TX_CPL_HDR_FC_CREDITS_S        12
+
+/* Queue Status Register */
+#define PCIE_QSR(X)                              (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x73C)
+#define PCIE_QSR_WAIT_UPDATE_FC_DLL               0x00000001 /* Received TLP FC Credits Not Returned */
+#define PCIE_QSR_TX_RETRY_BUF_NOT_EMPTY           0x00000002 /* Transmit Retry Buffer Not Empty */
+#define PCIE_QSR_RX_QUEUE_NOT_EMPTY               0x00000004 /* Received Queue Not Empty */
+
+/* VC Transmit Arbitration Register 1 */
+#define PCIE_VCTAR1(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x740)
+#define PCIE_VCTAR1_WRR_WEIGHT_VC0               0x000000FF /* WRR Weight for VC0 */
+#define PCIE_VCTAR1_WRR_WEIGHT_VC1               0x0000FF00 /* WRR Weight for VC1 */
+#define PCIE_VCTAR1_WRR_WEIGHT_VC2               0x00FF0000 /* WRR Weight for VC2 */
+#define PCIE_VCTAR1_WRR_WEIGHT_VC3               0xFF000000 /* WRR Weight for VC3 */
+
+/* VC Transmit Arbitration Register 2 */
+#define PCIE_VCTAR2(X)                          (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x744)
+#define PCIE_VCTAR2_WRR_WEIGHT_VC4               0x000000FF /* WRR Weight for VC4 */
+#define PCIE_VCTAR2_WRR_WEIGHT_VC5               0x0000FF00 /* WRR Weight for VC5 */
+#define PCIE_VCTAR2_WRR_WEIGHT_VC6               0x00FF0000 /* WRR Weight for VC6 */
+#define PCIE_VCTAR2_WRR_WEIGHT_VC7               0xFF000000 /* WRR Weight for VC7 */
+
+/* VC0 Posted Receive Queue Control Register */
+#define PCIE_VC0_PRQCR(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x748)
+#define PCIE_VC0_PRQCR_P_DATA_CREDITS            0x00000FFF /* VC0 Posted Data Credits */
+#define PCIE_VC0_PRQCR_P_DATA_CREDITS_S          0
+#define PCIE_VC0_PRQCR_P_HDR_CREDITS             0x000FF000 /* VC0 Posted Header Credits */
+#define PCIE_VC0_PRQCR_P_HDR_CREDITS_S           12
+#define PCIE_VC0_PRQCR_P_TLP_QUEUE_MODE          0x00E00000 /* VC0 Posted TLP Queue Mode */
+#define PCIE_VC0_PRQCR_P_TLP_QUEUE_MODE_S        20
+#define PCIE_VC0_PRQCR_TLP_RELAX_ORDER           0x40000000 /* TLP Type Ordering for VC0 */    
+#define PCIE_VC0_PRQCR_VC_STRICT_ORDER           0x80000000 /* VC0 Ordering for Receive Queues */
+
+/* VC0 Non-Posted Receive Queue Control */
+#define PCIE_VC0_NPRQCR(X)                      (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x74C)
+#define PCIE_VC0_NPRQCR_NP_DATA_CREDITS          0x00000FFF /* VC0 Non-Posted Data Credits */
+#define PCIE_VC0_NPRQCR_NP_DATA_CREDITS_S        0
+#define PCIE_VC0_NPRQCR_NP_HDR_CREDITS           0x000FF000 /* VC0 Non-Posted Header Credits */
+#define PCIE_VC0_NPRQCR_NP_HDR_CREDITS_S         12
+#define PCIE_VC0_NPRQCR_NP_TLP_QUEUE_MODE        0x00E00000 /* VC0 Non-Posted TLP Queue Mode */
+#define PCIE_VC0_NPRQCR_NP_TLP_QUEUE_MODE_S      20
+
+/* VC0 Completion Receive Queue Control */
+#define PCIE_VC0_CRQCR(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x750)
+#define PCIE_VC0_CRQCR_CPL_DATA_CREDITS          0x00000FFF /* VC0 Completion TLP Queue Mode */
+#define PCIE_VC0_CRQCR_CPL_DATA_CREDITS_S        0
+#define PCIE_VC0_CRQCR_CPL_HDR_CREDITS           0x000FF000 /* VC0 Completion Header Credits */
+#define PCIE_VC0_CRQCR_CPL_HDR_CREDITS_S         12
+#define PCIE_VC0_CRQCR_CPL_TLP_QUEUE_MODE        0x00E00000 /* VC0 Completion Data Credits */
+#define PCIE_VC0_CRQCR_CPL_TLP_QUEUE_MODE_S      21
+
+/* Applicable to the above three registers */
+enum {
+    PCIE_VC0_TLP_QUEUE_MODE_STORE_FORWARD = 1,
+    PCIE_VC0_TLP_QUEUE_MODE_CUT_THROUGH   = 2,
+    PCIE_VC0_TLP_QUEUE_MODE_BYPASS        = 4,
+};
+
+/* VC0 Posted Buffer Depth Register */
+#define PCIE_VC0_PBD(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x7A8)
+#define PCIE_VC0_PBD_P_DATA_QUEUE_ENTRIES       0x00003FFF /* VC0 Posted Data Queue Depth */
+#define PCIE_VC0_PBD_P_DATA_QUEUE_ENTRIES_S     0
+#define PCIE_VC0_PBD_P_HDR_QUEUE_ENTRIES        0x03FF0000 /* VC0 Posted Header Queue Depth */
+#define PCIE_VC0_PBD_P_HDR_QUEUE_ENTRIES_S      16
+
+/* VC0 Non-Posted Buffer Depth Register */
+#define PCIE_VC0_NPBD(X)                       (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x7AC)
+#define PCIE_VC0_NPBD_NP_DATA_QUEUE_ENTRIES     0x00003FFF /* VC0 Non-Posted Data Queue Depth */
+#define PCIE_VC0_NPBD_NP_DATA_QUEUE_ENTRIES_S   0
+#define PCIE_VC0_NPBD_NP_HDR_QUEUE_ENTRIES      0x03FF0000 /* VC0 Non-Posted Header Queue Depth */
+#define PCIE_VC0_NPBD_NP_HDR_QUEUE_ENTRIES_S    16
+
+/* VC0 Completion Buffer Depth Register */
+#define PCIE_VC0_CBD(X)                        (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x7B0)
+#define PCIE_VC0_CBD_CPL_DATA_QUEUE_ENTRIES     0x00003FFF /* C0 Completion Data Queue Depth */
+#define PCIE_VC0_CBD_CPL_DATA_QUEUE_ENTRIES_S   0
+#define PCIE_VC0_CBD_CPL_HDR_QUEUE_ENTRIES      0x03FF0000 /* VC0 Completion Header Queue Depth */
+#define PCIE_VC0_CBD_CPL_HDR_QUEUE_ENTRIES_S    16
+
+/* PHY Status Register, all zeros in VR9 */
+#define PCIE_PHYSR(X)                           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x810)
+
+/* PHY Control Register, all zeros in VR9 */
+#define PCIE_PHYCR(X)                           (volatile u32*)(PCIE_RC_PORT_TO_BASE(X) + 0x814)
+
+/* 
+ * PCIe PDI PHY register definition, suppose all the following 
+ * stuff is confidential. 
+ * XXX, detailed bit definition
+ */
+#define	PCIE_PHY_PLL_CTRL1(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x22 << 1))
+#define	PCIE_PHY_PLL_CTRL2(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x23 << 1))
+#define	PCIE_PHY_PLL_CTRL3(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x24 << 1))
+#define	PCIE_PHY_PLL_CTRL4(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x25 << 1))
+#define	PCIE_PHY_PLL_CTRL5(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x26 << 1))
+#define	PCIE_PHY_PLL_CTRL6(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x27 << 1))
+#define	PCIE_PHY_PLL_CTRL7(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x28 << 1))
+#define	PCIE_PHY_PLL_A_CTRL1(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x29 << 1))
+#define	PCIE_PHY_PLL_A_CTRL2(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x2A << 1))
+#define	PCIE_PHY_PLL_A_CTRL3(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x2B << 1))
+#define	PCIE_PHY_PLL_STATUS(X)      (PCIE_PHY_PORT_TO_BASE(X) + (0x2C << 1))
+ 
+#define PCIE_PHY_TX1_CTRL1(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x30 << 1))
+#define PCIE_PHY_TX1_CTRL2(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x31 << 1))
+#define PCIE_PHY_TX1_CTRL3(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x32 << 1))
+#define PCIE_PHY_TX1_A_CTRL1(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x33 << 1))
+#define PCIE_PHY_TX1_A_CTRL2(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x34 << 1))
+#define PCIE_PHY_TX1_MOD1(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x35 << 1))
+#define PCIE_PHY_TX1_MOD2(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x36 << 1))
+#define PCIE_PHY_TX1_MOD3(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x37 << 1))
+
+#define PCIE_PHY_TX2_CTRL1(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x38 << 1))
+#define PCIE_PHY_TX2_CTRL2(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x39 << 1))
+#define PCIE_PHY_TX2_A_CTRL1(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x3B << 1))
+#define PCIE_PHY_TX2_A_CTRL2(X)     (PCIE_PHY_PORT_TO_BASE(X) + (0x3C << 1))
+#define PCIE_PHY_TX2_MOD1(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x3D << 1))
+#define PCIE_PHY_TX2_MOD2(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x3E << 1))
+#define PCIE_PHY_TX2_MOD3(X)        (PCIE_PHY_PORT_TO_BASE(X) + (0x3F << 1))
+
+#define PCIE_PHY_RX1_CTRL1(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x50 << 1))
+#define PCIE_PHY_RX1_CTRL2(X)       (PCIE_PHY_PORT_TO_BASE(X) + (0x51 << 1))
+#define PCIE_PHY_RX1_CDR(X)         (PCIE_PHY_PORT_TO_BASE(X) + (0x52 << 1))
+#define PCIE_PHY_RX1_EI(X)          (PCIE_PHY_PORT_TO_BASE(X) + (0x53 << 1))
+#define PCIE_PHY_RX1_A_CTRL(X)      (PCIE_PHY_PORT_TO_BASE(X) + (0x55 << 1))
+
+/* Interrupt related stuff */
+#define PCIE_LEGACY_DISABLE 0
+#define PCIE_LEGACY_INTA  1
+#define PCIE_LEGACY_INTB  2
+#define PCIE_LEGACY_INTC  3
+#define PCIE_LEGACY_INTD  4
+#define PCIE_LEGACY_INT_MAX PCIE_LEGACY_INTD
+
+#define PCIE_IRQ_LOCK(lock) do {             \
+    unsigned long flags;                     \
+    spin_lock_irqsave(&(lock), flags);
+#define PCIE_IRQ_UNLOCK(lock)                \
+    spin_unlock_irqrestore(&(lock), flags);  \
+} while (0)
+
+#if LINUX_VERSION_CODE < KERNEL_VERSION(2,6,18)
+#define IRQF_SHARED SA_SHIRQ
+#endif
+
+#define PCIE_MSG_MSI        0x00000001
+#define PCIE_MSG_ISR        0x00000002
+#define PCIE_MSG_FIXUP      0x00000004
+#define PCIE_MSG_READ_CFG   0x00000008
+#define PCIE_MSG_WRITE_CFG  0x00000010
+#define PCIE_MSG_CFG        (PCIE_MSG_READ_CFG | PCIE_MSG_WRITE_CFG)
+#define PCIE_MSG_REG        0x00000020
+#define PCIE_MSG_INIT       0x00000040
+#define PCIE_MSG_ERR        0x00000080
+#define PCIE_MSG_PHY        0x00000100
+#define PCIE_MSG_ANY        0x000001ff
+
+#define IFX_PCIE_PORT0      0
+#define IFX_PCIE_PORT1      1
+
+#ifdef CONFIG_IFX_PCIE_2ND_CORE
+#define IFX_PCIE_CORE_NR    2
+#else
+#define IFX_PCIE_CORE_NR    1
+#endif
+
+//#define IFX_PCIE_ERROR_INT
+
+//#define IFX_PCIE_DBG
+
+#if defined(IFX_PCIE_DBG)
+#define IFX_PCIE_PRINT(_m, _fmt, args...) do {   \
+    if (g_pcie_debug_flag & (_m)) {              \
+        ifx_pcie_debug((_fmt), ##args);          \
+    }                                            \
+} while (0)
+
+#define INLINE 
+#else
+#define IFX_PCIE_PRINT(_m, _fmt, args...)   \
+    do {} while(0)
+#define INLINE inline
+#endif
+
+struct ifx_pci_controller {
+	struct pci_controller   pcic;
+    
+	/* RC specific, per host bus information */
+	u32   port;  /* Port index, 0 -- 1st core, 1 -- 2nd core */
+};
+
+typedef struct ifx_pcie_ir_irq {
+    const unsigned int irq;
+    const char name[16];
+}ifx_pcie_ir_irq_t;
+
+typedef struct ifx_pcie_legacy_irq{
+    const u32 irq_bit;
+    const int irq;
+}ifx_pcie_legacy_irq_t;
+
+typedef struct ifx_pcie_irq {
+    ifx_pcie_ir_irq_t ir_irq;
+    ifx_pcie_legacy_irq_t legacy_irq[PCIE_LEGACY_INT_MAX];
+}ifx_pcie_irq_t;
+
+extern u32 g_pcie_debug_flag;
+extern void ifx_pcie_debug(const char *fmt, ...);
+extern void pcie_phy_clock_mode_setup(int pcie_port);
+extern void pcie_msi_pic_init(int pcie_port);
+extern u32 ifx_pcie_bus_enum_read_hack(int where, u32 value);
+extern u32 ifx_pcie_bus_enum_write_hack(int where, u32 value);
+
+
+#include <linux/types.h>
+#include <linux/delay.h>
+#include <linux/gpio.h>
+#include <linux/clk.h>
+
+#include <lantiq_soc.h>
+
+#define IFX_PCIE_GPIO_RESET  38
+#define IFX_REG_R32	ltq_r32
+#define IFX_REG_W32	ltq_w32
+#define CONFIG_IFX_PCIE_HW_SWAP
+#define IFX_RCU_AHB_ENDIAN                      ((volatile u32*)(IFX_RCU + 0x004C))
+#define IFX_RCU_RST_REQ                         ((volatile u32*)(IFX_RCU + 0x0010))
+#define IFX_RCU_AHB_BE_PCIE_PDI                  0x00000080  /* Configure PCIE PDI module in big endian*/
+
+#define IFX_RCU                                 (KSEG1 | 0x1F203000)
+#define IFX_RCU_AHB_BE_PCIE_M                    0x00000001  /* Configure AHB master port that connects to PCIe RC in big endian */
+#define IFX_RCU_AHB_BE_PCIE_S                    0x00000010  /* Configure AHB slave port that connects to PCIe RC in little endian */
+#define IFX_RCU_AHB_BE_XBAR_M                    0x00000002  /* Configure AHB master port that connects to XBAR in big endian */
+#define CONFIG_IFX_PCIE_PHY_36MHZ_MODE
+
+#define IFX_PMU1_MODULE_PCIE_PHY   (0)
+#define IFX_PMU1_MODULE_PCIE_CTRL  (1)
+#define IFX_PMU1_MODULE_PDI        (4)
+#define IFX_PMU1_MODULE_MSI        (5)
+
+#define IFX_PMU_MODULE_PCIE_L0_CLK (31)
+
+
+static inline void pcie_ep_gpio_rst_init(int pcie_port)
+{
+}
+
+static inline void pcie_ahb_pmu_setup(void)
+{
+	struct clk *clk;
+	clk = clk_get_sys("ltq_pcie", "ahb");
+	clk_enable(clk);
+	//ltq_pmu_enable(PMU_AHBM | PMU_AHBS);
+}
+
+static inline void pcie_rcu_endian_setup(int pcie_port)
+{
+    u32 reg;
+
+    reg = IFX_REG_R32(IFX_RCU_AHB_ENDIAN);
+#ifdef CONFIG_IFX_PCIE_HW_SWAP
+    reg |= IFX_RCU_AHB_BE_PCIE_M;
+    reg |= IFX_RCU_AHB_BE_PCIE_S;
+    reg &= ~IFX_RCU_AHB_BE_XBAR_M;
+#else 
+    reg |= IFX_RCU_AHB_BE_PCIE_M;
+    reg &= ~IFX_RCU_AHB_BE_PCIE_S;
+    reg &= ~IFX_RCU_AHB_BE_XBAR_M;
+#endif /* CONFIG_IFX_PCIE_HW_SWAP */
+    IFX_REG_W32(reg, IFX_RCU_AHB_ENDIAN);
+    IFX_PCIE_PRINT(PCIE_MSG_REG, "%s IFX_RCU_AHB_ENDIAN: 0x%08x\n", __func__, IFX_REG_R32(IFX_RCU_AHB_ENDIAN));
+}
+
+static inline void pcie_phy_pmu_enable(int pcie_port)
+{
+	struct clk *clk;
+	clk = clk_get_sys("ltq_pcie", "phy");
+	clk_enable(clk);
+	//ltq_pmu1_enable(1<<IFX_PMU1_MODULE_PCIE_PHY);
+}
+
+static inline void pcie_phy_pmu_disable(int pcie_port)
+{
+	struct clk *clk;
+	clk = clk_get_sys("ltq_pcie", "phy");
+	clk_disable(clk);
+	//ltq_pmu1_disable(1<<IFX_PMU1_MODULE_PCIE_PHY);
+}
+
+static inline void pcie_pdi_big_endian(int pcie_port)
+{
+    u32 reg;
+
+    /* SRAM2PDI endianness control. */
+    reg = IFX_REG_R32(IFX_RCU_AHB_ENDIAN);
+    /* Config AHB->PCIe and PDI endianness */
+    reg |= IFX_RCU_AHB_BE_PCIE_PDI;
+    IFX_REG_W32(reg, IFX_RCU_AHB_ENDIAN);
+}
+
+static inline void pcie_pdi_pmu_enable(int pcie_port)
+{
+	struct clk *clk;
+	clk = clk_get_sys("ltq_pcie", "pdi");
+	clk_enable(clk);
+	//ltq_pmu1_enable(1<<IFX_PMU1_MODULE_PDI);
+}
+
+static inline void pcie_core_rst_assert(int pcie_port)
+{
+    u32 reg;
+
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+
+    /* Reset PCIe PHY & Core, bit 22, bit 26 may be affected if write it directly  */
+    reg |= 0x00400000;
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_core_rst_deassert(int pcie_port)
+{
+    u32 reg;
+
+    /* Make sure one micro-second delay */
+    udelay(1);
+
+    /* Reset PCIe PHY & Core, bit 22 */
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+    reg &= ~0x00400000;
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_phy_rst_assert(int pcie_port)
+{
+    u32 reg;
+
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+    reg |= 0x00001000; /* Bit 12 */
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_phy_rst_deassert(int pcie_port)
+{
+    u32 reg;
+
+    /* Make sure one micro-second delay */
+    udelay(1);
+
+    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
+    reg &= ~0x00001000; /* Bit 12 */
+    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
+}
+
+static inline void pcie_device_rst_assert(int pcie_port)
+{
+	gpio_set_value(IFX_PCIE_GPIO_RESET, 0);
+  //  ifx_gpio_output_clear(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
+}
+
+static inline void pcie_device_rst_deassert(int pcie_port)
+{
+    mdelay(100);
+	gpio_set_value(IFX_PCIE_GPIO_RESET, 1);
+//    ifx_gpio_output_set(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
+}
+
+static inline void pcie_core_pmu_setup(int pcie_port)
+{
+	struct clk *clk;
+	clk = clk_get_sys("ltq_pcie", "ctl");
+	clk_enable(clk);
+	clk = clk_get_sys("ltq_pcie", "bus");
+	clk_enable(clk);
+
+	//ltq_pmu1_enable(1 << IFX_PMU1_MODULE_PCIE_CTRL);
+	//ltq_pmu_enable(1 << IFX_PMU_MODULE_PCIE_L0_CLK);
+}
+
+static inline void pcie_msi_init(int pcie_port)
+{
+	struct clk *clk;
+    pcie_msi_pic_init(pcie_port);
+	clk = clk_get_sys("ltq_pcie", "msi");
+	clk_enable(clk);
+	//ltq_pmu1_enable(1 << IFX_PMU1_MODULE_MSI);
+}
+
+static inline u32
+ifx_pcie_bus_nr_deduct(u32 bus_number, int pcie_port)
+{
+    u32 tbus_number = bus_number;
+
+#ifdef CONFIG_IFX_PCI
+    if (pcibios_host_nr() > 1) {
+        tbus_number -= pcibios_1st_host_bus_nr();
+    }
+#endif /* CONFIG_IFX_PCI */
+    return tbus_number;
+}
+
+static inline u32
+ifx_pcie_bus_enum_hack(struct pci_bus *bus, u32 devfn, int where, u32 value, int pcie_port, int read)
+{
+    struct pci_dev *pdev;
+    u32 tvalue = value;
+
+    /* Sanity check */
+    pdev = pci_get_slot(bus, devfn);
+    if (pdev == NULL) {
+        return tvalue;
+    }
+
+    /* Only care about PCI bridge */
+    if (pdev->hdr_type != PCI_HEADER_TYPE_BRIDGE) {
+        return tvalue;
+    }
+
+    if (read) { /* Read hack */
+    #ifdef CONFIG_IFX_PCI
+        if (pcibios_host_nr() > 1) {
+            tvalue = ifx_pcie_bus_enum_read_hack(where, tvalue);
+        }
+    #endif /* CONFIG_IFX_PCI */  
+    }
+    else { /* Write hack */
+    #ifdef CONFIG_IFX_PCI    
+        if (pcibios_host_nr() > 1) {
+            tvalue = ifx_pcie_bus_enum_write_hack(where, tvalue);
+        }
+    #endif
+    }
+    return tvalue;
+}
+
+#endif /* IFXMIPS_PCIE_VR9_H */
+
--- a/drivers/pci/pcie/aer/Kconfig
+++ b/drivers/pci/pcie/aer/Kconfig
@@ -5,7 +5,7 @@
 config PCIEAER
 	boolean "Root Port Advanced Error Reporting support"
 	depends on PCIEPORTBUS
-	default y
+	default n
 	help
 	  This enables PCI Express Root Port Advanced Error Reporting
 	  (AER) driver support. Error reporting messages sent to Root
--- a/include/linux/pci.h
+++ b/include/linux/pci.h
@@ -1082,6 +1082,8 @@ void pci_walk_bus(struct pci_bus *top, i
 int pci_cfg_space_size_ext(struct pci_dev *dev);
 int pci_cfg_space_size(struct pci_dev *dev);
 unsigned char pci_bus_max_busnr(struct pci_bus *bus);
+int pcibios_host_nr(void);
+int pcibios_1st_host_bus_nr(void);
 void pci_setup_bridge(struct pci_bus *bus);
 resource_size_t pcibios_window_alignment(struct pci_bus *bus,
 					 unsigned long type);
--- a/include/linux/pci_ids.h
+++ b/include/linux/pci_ids.h
@@ -1044,6 +1044,12 @@
 #define PCI_DEVICE_ID_SGI_LITHIUM	0x1002
 #define PCI_DEVICE_ID_SGI_IOC4		0x100a
 
+#define PCI_VENDOR_ID_INFINEON		0x15D1
+#define PCI_DEVICE_ID_INFINEON_DANUBE	0x000F
+#define PCI_DEVICE_ID_INFINEON_PCIE	0x0011
+#define PCI_VENDOR_ID_LANTIQ		0x1BEF
+#define PCI_DEVICE_ID_LANTIQ_PCIE	0x00
+
 #define PCI_VENDOR_ID_WINBOND		0x10ad
 #define PCI_DEVICE_ID_WINBOND_82C105	0x0105
 #define PCI_DEVICE_ID_WINBOND_83C553	0x0565
