--- a/tn7sar.c
+++ b/tn7sar.c
@@ -103,10 +103,10 @@ enum
 
 #define RESERVED_OAM_CHANNEL              15
 
-#define AAL5_PARM "id=aal5, base = 0x03000000, offset = 0, int_line=15, ch0=[RxBufSize=1522; RxNumBuffers = 32; RxServiceMax = 50; TxServiceMax=50; TxNumBuffers=32; CpcsUU=0x5aa5; TxVc_CellRate=0x3000; TxVc_AtmHeader=0x00000640]"
-#define SAR_PARM "id=sar,base = 0x03000000, reset_bit = 9, offset = 0; UniNni = 0, PdspEnable = 1"
+#define CH0_PARM "RxBufSize=1522, RxNumBuffers=32, RxServiceMax=50, TxServiceMax=50, TxNumBuffers=32, CpcsUU=0x5aa5, TxVc_CellRate=0x3000, TxVc_AtmHeader=0x00000640"
+#define AAL5_PARM "id=aal5, base=0x03000000, offset=0, int_line=15, ch0=[" CH0_PARM "]"
+#define SAR_PARM "id=sar, base=0x03000000, reset_bit=9, offset=0; UniNni=0, PdspEnable=1, Debug=0xFFFFFFFF"
 #define RESET_PARM "id=ResetControl, base=0xA8611600"
-#define CH0_PARM "RxBufSize=1522, RxNumBuffers = 32, RxServiceMax = 50, TxServiceMax=50, TxNumBuffers=32, CpcsUU=0x5aa5, TxVc_CellRate=0x3000, TxVc_AtmHeader=0x00000640"
 
 #define MAX_PVC_TABLE_ENTRY 16
 
