From e2092cf1b164ede62b740c7c95905171fb6232ff Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Sat, 23 Mar 2013 12:32:56 +0100
Subject: [PATCH v2 1/3] MTD: bcm63xxpart: use size macro for CFE block size

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 drivers/mtd/bcm63xxpart.c |    3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/mtd/bcm63xxpart.c
+++ b/drivers/mtd/bcm63xxpart.c
@@ -27,6 +27,7 @@
 #include <linux/crc32.h>
 #include <linux/module.h>
 #include <linux/kernel.h>
+#include <linux/sizes.h>
 #include <linux/slab.h>
 #include <linux/vmalloc.h>
 #include <linux/mtd/mtd.h>
@@ -37,7 +38,7 @@
 
 #define BCM63XX_EXTENDED_SIZE	0xBFC00000	/* Extended flash address */
 
-#define BCM63XX_CFE_BLOCK_SIZE	0x10000		/* always at least 64KiB */
+#define BCM63XX_CFE_BLOCK_SIZE	SZ_64K		/* always at least 64KiB */
 
 #define BCM63XX_CFE_MAGIC_OFFSET 0x4e0
 
