From fa0e27879ec0fc9034eca320e4055539a1b97797 Mon Sep 17 00:00:00 2001
From: Grigori Goronzy <greg@blackbox>
Date: Mon, 11 Jun 2012 18:53:59 +0200
Subject: [PATCH 013/196] sdhci-bcm2708: add additional quirks

Some additional quirks are needed for correct operation.
There's no SDHCI capabilities register documented, and it always reads
zero, so add SDHCI_QUIRK_MISSING_CAPS. Apparently
SDHCI_QUIRK_NO_HISPD_BIT is needed for many cards to work correctly in
high-speed mode, so add it as well.
---
 drivers/mmc/host/sdhci-bcm2708.c | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

diff --git a/drivers/mmc/host/sdhci-bcm2708.c b/drivers/mmc/host/sdhci-bcm2708.c
index 0ed4d85..3001836 100644
--- a/drivers/mmc/host/sdhci-bcm2708.c
+++ b/drivers/mmc/host/sdhci-bcm2708.c
@@ -1189,7 +1189,9 @@ static int sdhci_bcm2708_probe(struct platform_device *pdev)
 	host->quirks = SDHCI_QUIRK_BROKEN_CARD_DETECTION |
 		       SDHCI_QUIRK_DATA_TIMEOUT_USES_SDCLK |
 		       SDHCI_QUIRK_BROKEN_TIMEOUT_VAL |
-		       SDHCI_QUIRK_NONSTANDARD_CLOCK;
+               SDHCI_QUIRK_MISSING_CAPS |
+               SDHCI_QUIRK_NO_HISPD_BIT;
+
 #ifdef CONFIG_MMC_SDHCI_BCM2708_DMA
 	host->flags = SDHCI_USE_PLATDMA;
 #endif
-- 
1.9.1

