--- /dev/null
+++ b/arch/arm/boot/dts/sun7i-a20-bananapi.dts
@@ -0,0 +1,160 @@
+/*
+ * Copyright 2014 Zoltan HERPAI
+ * Zoltan HERPAI <wigyori@uid0.hu>
+ *
+ * The code contained herein is licensed under the GNU General Public
+ * License. You may obtain a copy of the GNU General Public License
+ * Version 2 or later at the following locations:
+ *
+ * http://www.opensource.org/licenses/gpl-license.html
+ * http://www.gnu.org/copyleft/gpl.html
+ */
+
+/dts-v1/;
+/include/ "sun7i-a20.dtsi"
+/include/ "sunxi-ahci-reg.dtsi"
+/include/ "sun4i-a10-usb-vbus-reg.dtsi"
+#include <dt-bindings/input/input.h>
+
+/ {
+	model = "Lemaker bananaPi";
+	compatible = "lemaker,bananapi", "allwinner,sun7i-a20";
+
+	aliases {
+		spi0 = &spi1;
+		spi1 = &spi2;
+	};
+
+	soc@01c00000 {
+		spi1: spi@01c06000 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pins_a>;
+			status = "okay";
+		};
+
+		spi2: spi@01c17000 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi2_pins_a>;
+			status = "okay";
+		};
+
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_bananapi>;
+			cd-gpios = <&pio 7 10 0>; /* PH10 */
+			status = "okay";
+		};
+
+		usbphy: phy@01c13400 {
+			usb1_vbus-supply = <&reg_usb1_vbus>;
+			usb2_vbus-supply = <&reg_usb2_vbus>;
+			status = "okay";
+		};
+
+		ehci0: usb@01c14000 {
+			status = "okay";
+		};
+
+		ohci0: usb@01c14400 {
+			status = "okay";
+		};
+
+		ahci: sata@01c18000 {
+			target-supply = <&reg_ahci_5v>;
+			status = "okay";
+		};
+
+		ehci1: usb@01c1c000 {
+			status = "okay";
+		};
+
+		ohci1: usb@01c1c400 {
+			status = "okay";
+		};
+
+		pinctrl@01c20800 {
+			led_pins_bananapi: led_pins@0 {
+				allwinner,pins = "PH24";
+				allwinner,function = "gpio_out";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			mmc0_cd_pin_bananapi: mmc0_cd_pin@0 {
+				allwinner,pins = "PH10";
+				allwinner,function = "gpio_in";
+				allwinner,drive = <0>;
+				allwinner,pull = <1>;
+			};
+		};
+
+		lradc: lradc@01c22800 {
+			allwinner,chan0-step = <200>;
+			linux,chan0-keycodes = <KEY_VOLUMEUP KEY_VOLUMEDOWN
+						KEY_MENU KEY_SEARCH KEY_HOME
+						KEY_ESC KEY_ENTER>;
+			status = "okay";
+		};
+
+		uart0: serial@01c28000 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart0_pins_a>;
+			status = "okay";
+		};
+
+		uart6: serial@01c29800 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart6_pins_a>;
+			status = "okay";
+		};
+
+		uart7: serial@01c29c00 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart7_pins_a>;
+			status = "okay";
+		};
+
+		i2c0: i2c@01c2ac00 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c0_pins_a>;
+			status = "okay";
+		};
+
+		i2c1: i2c@01c2b000 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c1_pins_a>;
+			status = "okay";
+		};
+
+		i2c2: i2c@01c2b400 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c2_pins_a>;
+			status = "okay";
+		};
+
+		gmac: ethernet@01c50000 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&gmac_pins_mii_a>;
+			phy = <&phy1>;
+			phy-mode = "mii";
+			status = "okay";
+
+			phy1: ethernet-phy@1 {
+				reg = <1>;
+			};
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+		pinctrl-names = "default";
+		pinctrl-0 = <&led_pins_bananapi>;
+
+		green {
+			label = "bananapi:green:usr";
+			gpios = <&pio 7 24 0>;
+			linux,default-trigger = "heartbeat";
+		};
+	};
+};
