From 338560ad44f2e8b6f4eb095567830b6c78b35ba2 Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Wed, 5 Mar 2014 20:40:57 +0100
Subject: [PATCH] ARM: sun7i: dt: Add address- and size-cells info to i2c
 controller nodes

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -848,6 +848,8 @@
 			clocks = <&apb1_gates 0>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		i2c1: i2c@01c2b000 {
@@ -857,6 +859,8 @@
 			clocks = <&apb1_gates 1>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		i2c2: i2c@01c2b400 {
@@ -866,6 +870,8 @@
 			clocks = <&apb1_gates 2>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		i2c3: i2c@01c2b800 {
@@ -875,6 +881,8 @@
 			clocks = <&apb1_gates 3>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		i2c4: i2c@01c2bc00 {
@@ -884,6 +892,8 @@
 			clocks = <&apb1_gates 15>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		gmac: ethernet@01c50000 {
