--- a/drivers/mtd/nand/Kconfig
+++ b/drivers/mtd/nand/Kconfig
@@ -518,4 +518,12 @@ config MTD_NAND_RB750
 	tristate "NAND flash driver for the RouterBoard 750"
 	depends on MTD_NAND && ATH79_MACH_RB750
 
+config MTD_NAND_AR934X
+	tristate "NAND flash driver for the Qualcomm Atheros AR934x/QCA955x SoCs"
+	depends on (SOC_AR934X || SOC_QCA955X)
+
+config MTD_NAND_AR934X_HW_ECC
+	bool "Hardware ECC support for the AR934X NAND Controller (EXPERIMENTAL)"
+	depends on MTD_NAND_AR934X
+
 endif # MTD_NAND
--- a/drivers/mtd/nand/Makefile
+++ b/drivers/mtd/nand/Makefile
@@ -13,6 +13,7 @@ obj-$(CONFIG_MTD_NAND_AMS_DELTA)	+= ams-
 obj-$(CONFIG_MTD_NAND_DENALI)		+= denali.o
 obj-$(CONFIG_MTD_NAND_DENALI_PCI)	+= denali_pci.o
 obj-$(CONFIG_MTD_NAND_DENALI_DT)	+= denali_dt.o
+obj-$(CONFIG_MTD_NAND_AR934X)		+= ar934x_nfc.o
 obj-$(CONFIG_MTD_NAND_AU1550)		+= au1550nd.o
 obj-$(CONFIG_MTD_NAND_BF5XX)		+= bf5xx_nand.o
 obj-$(CONFIG_MTD_NAND_S3C2410)		+= s3c2410.o
