From 22b9ac16c600694b12479a75461bce031295e4b9 Mon Sep 17 00:00:00 2001
From: Chen-Yu Tsai <wens@csie.org>
Date: Mon, 10 Feb 2014 18:35:49 +0800
Subject: [PATCH] ARM: dts: sun7i: Add GMAC controller node to sun7i DTSI

Signed-off-by: Chen-Yu Tsai <wens@csie.org>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 15 +++++++++++++++
 1 file changed, 15 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -653,6 +653,21 @@
 			status = "disabled";
 		};
 
+		gmac: ethernet@01c50000 {
+			compatible = "allwinner,sun7i-a20-gmac";
+			reg = <0x01c50000 0x10000>;
+			interrupts = <0 85 4>;
+			interrupt-names = "macirq";
+			clocks = <&ahb_gates 49>, <&gmac_tx_clk>;
+			clock-names = "stmmaceth", "allwinner_gmac_tx";
+			snps,pbl = <2>;
+			snps,fixed-burst;
+			snps,force_sf_dma_mode;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
 		hstimer@01c60000 {
 			compatible = "allwinner,sun7i-a20-hstimer";
 			reg = <0x01c60000 0x1000>;
