From 98f63141190ac02c58b78d58f771bd263c61d756 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Sat, 7 Dec 2013 17:14:17 +0100
Subject: [PATCH 48/56] MIPS: BCM63XX: add support for BCM63268

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/bcm63xx/Kconfig                         |   5 +
 arch/mips/bcm63xx/boards/board_bcm963xx.c         |   2 +-
 arch/mips/bcm63xx/clk.c                           |  25 ++++-
 arch/mips/bcm63xx/cpu.c                           |  59 +++++++++-
 arch/mips/bcm63xx/dev-flash.c                     |   6 +
 arch/mips/bcm63xx/dev-spi.c                       |   4 +-
 arch/mips/bcm63xx/irq.c                           |  20 +++-
 arch/mips/bcm63xx/reset.c                         |  21 ++++
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h  | 130 ++++++++++++++++++++++
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_gpio.h |   2 +
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h |  79 +++++++++++++
 arch/mips/include/asm/mach-bcm63xx/ioremap.h      |   1 +
 12 files changed, 342 insertions(+), 12 deletions(-)

--- a/arch/mips/bcm63xx/Kconfig
+++ b/arch/mips/bcm63xx/Kconfig
@@ -60,6 +60,11 @@ config BCM63XX_CPU_6368
 	select HW_HAS_PCI
 	select BCM63XX_OHCI
 	select BCM63XX_EHCI
+
+config BCM63XX_CPU_63268
+	bool "support 63268 CPU"
+	select SYS_HAS_CPU_BMIPS4350
+	select HW_HAS_PCI
 endmenu
 
 source "arch/mips/bcm63xx/boards/Kconfig"
--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -737,7 +737,7 @@ void __init board_prom_init(void)
 	/* read base address of boot chip select (0)
 	 * 6328/6362 do not have MPI but boot from a fixed address
 	 */
-	if (BCMCPU_IS_6328() || BCMCPU_IS_6362()) {
+	if (BCMCPU_IS_6328() || BCMCPU_IS_6362() || BCMCPU_IS_63268()) {
 		val = 0x18000000;
 	} else {
 		val = bcm_mpi_readl(MPI_CSBASE_REG(0));
--- a/arch/mips/bcm63xx/clk.c
+++ b/arch/mips/bcm63xx/clk.c
@@ -133,6 +133,8 @@ static void enetsw_set(struct clk *clk,
 				CKCTL_6368_SWPKT_USB_EN |
 				CKCTL_6368_SWPKT_SAR_EN,
 				enable);
+	else if (BCMCPU_IS_63268())
+		bcm_hwclock_set(CKCTL_63268_ROBOSW_EN, enable);
 	else
 		return;
 
@@ -177,6 +179,8 @@ static void usbh_set(struct clk *clk, in
 		bcm_hwclock_set(CKCTL_6362_USBH_EN, enable);
 	else if (BCMCPU_IS_6368())
 		bcm_hwclock_set(CKCTL_6368_USBH_EN, enable);
+	else if (BCMCPU_IS_63268())
+		bcm_hwclock_set(CKCTL_63268_USBH_EN, enable);
 	else
 		return;
 
@@ -199,6 +203,8 @@ static void usbd_set(struct clk *clk, in
 		bcm_hwclock_set(CKCTL_6362_USBD_EN, enable);
 	else if (BCMCPU_IS_6368())
 		bcm_hwclock_set(CKCTL_6368_USBD_EN, enable);
+	else if (BCMCPU_IS_63268())
+		bcm_hwclock_set(CKCTL_63268_USBD_EN, enable);
 	else
 		return;
 
@@ -225,9 +231,13 @@ static void spi_set(struct clk *clk, int
 		mask = CKCTL_6358_SPI_EN;
 	else if (BCMCPU_IS_6362())
 		mask = CKCTL_6362_SPI_EN;
-	else
-		/* BCMCPU_IS_6368 */
+	else if (BCMCPU_IS_6368())
 		mask = CKCTL_6368_SPI_EN;
+	else if (BCMCPU_IS_63268())
+		mask = CKCTL_63268_SPI_EN;
+	else
+		return;
+
 	bcm_hwclock_set(mask, enable);
 }
 
@@ -246,6 +256,8 @@ static void hsspi_set(struct clk *clk, i
 		mask = CKCTL_6328_HSSPI_EN;
 	else if (BCMCPU_IS_6362())
 		mask = CKCTL_6362_HSSPI_EN;
+	else if (BCMCPU_IS_63268())
+		mask = CKCTL_63268_HSSPI_EN;
 	else
 		return;
 
@@ -307,6 +319,8 @@ static void pcie_set(struct clk *clk, in
 		bcm_hwclock_set(CKCTL_6328_PCIE_EN, enable);
 	else if (BCMCPU_IS_6362())
 		bcm_hwclock_set(CKCTL_6362_PCIE_EN, enable);
+	else if (BCMCPU_IS_63268())
+		bcm_hwclock_set(CKCTL_63268_PCIE_EN, enable);
 }
 
 static struct clk clk_pcie = {
@@ -386,9 +400,11 @@ struct clk *clk_get(struct device *dev,
 		return &clk_periph;
 	if ((BCMCPU_IS_3368() || BCMCPU_IS_6358()) && !strcmp(id, "pcm"))
 		return &clk_pcm;
-	if ((BCMCPU_IS_6362() || BCMCPU_IS_6368()) && !strcmp(id, "ipsec"))
+	if ((BCMCPU_IS_6362() || BCMCPU_IS_6368() || BCMCPU_IS_63268()) &&
+	    !strcmp(id, "ipsec"))
 		return &clk_ipsec;
-	if ((BCMCPU_IS_6328() || BCMCPU_IS_6362()) && !strcmp(id, "pcie"))
+	if ((BCMCPU_IS_6328() || BCMCPU_IS_6362() || BCMCPU_IS_63268()) &&
+	    !strcmp(id, "pcie"))
 		return &clk_pcie;
 	return ERR_PTR(-ENOENT);
 }
@@ -411,6 +427,7 @@ static int __init bcm63xx_clk_init(void)
 		clk_hsspi.rate = HSSPI_PLL_HZ_6328;
 		break;
 	case BCM6362_CPU_ID:
+	case BCM63268_CPU_ID:
 		clk_hsspi.rate = HSSPI_PLL_HZ_6362;
 		break;
 	}
--- a/arch/mips/bcm63xx/cpu.c
+++ b/arch/mips/bcm63xx/cpu.c
@@ -101,6 +101,15 @@ static const int bcm6368_irqs[] = {
 
 };
 
+static const unsigned long bcm63268_regs_base[] = {
+	__GEN_CPU_REGS_TABLE(63268)
+};
+
+static const int bcm63268_irqs[] = {
+	__GEN_CPU_IRQ_TABLE(63268)
+
+};
+
 u32 bcm63xx_get_cpu_variant(void)
 {
 	return bcm63xx_cpu_variant;
@@ -253,6 +262,27 @@ static unsigned int detect_cpu_clock(voi
 
 		return (((64 * 1000000) / p1) * p2 * ndiv) / m1;
 	}
+	case BCM63268_CPU_ID:
+	{
+		unsigned int tmp, mips_pll_fcvo;
+
+		tmp = bcm_misc_readl(MISC_STRAPBUS_63268_REG);
+		mips_pll_fcvo = (tmp & STRAPBUS_63268_FCVO_MASK) >>
+				STRAPBUS_63268_FCVO_SHIFT;
+		switch (mips_pll_fcvo) {
+		case 0x3:
+		case 0xe:
+			return 320000000;
+		case 0xa:
+			return 333000000;
+		case 0x2:
+		case 0xb:
+		case 0xf:
+			return 400000000;
+		default:
+			return 0;
+		}
+	}
 
 	default:
 		panic("Failed to detect clock for CPU with id=%04X\n", cpu_id);
@@ -267,7 +297,7 @@ static unsigned int detect_memory_size(v
 	unsigned int cols = 0, rows = 0, is_32bits = 0, banks = 0;
 	u32 val;
 
-	if (BCMCPU_IS_6328() || BCMCPU_IS_6362())
+	if (BCMCPU_IS_6328() || BCMCPU_IS_6362() || BCMCPU_IS_63268())
 		return bcm_ddr_readl(DDR_CSEND_REG) << 24;
 
 	if (BCMCPU_IS_6345()) {
@@ -306,6 +336,7 @@ void __init bcm63xx_cpu_init(void)
 	struct cpuinfo_mips *c = &current_cpu_data;
 	unsigned int cpu = smp_processor_id();
 	u32 chipid_reg;
+	bool long_chipid = false;
 	u8 __maybe_unused varid = 0;
 
 	/* soc registers location depends on cpu type */
@@ -327,6 +358,9 @@ void __init bcm63xx_cpu_init(void)
 		case 0x10:
 			chipid_reg = BCM_6345_PERF_BASE;
 			break;
+		case 0x80:
+			long_chipid = true;
+			/* fall-through */
 		default:
 			chipid_reg = BCM_6368_PERF_BASE;
 			break;
@@ -334,6 +368,7 @@ void __init bcm63xx_cpu_init(void)
 		break;
 	}
 
+
 	/*
 	 * really early to panic, but delaying panic would not help since we
 	 * will never get any working console
@@ -343,10 +378,17 @@ void __init bcm63xx_cpu_init(void)
 
 	/* read out CPU type */
 	tmp = bcm_readl(chipid_reg);
-	bcm63xx_cpu_id = (tmp & REV_CHIPID_MASK) >> REV_CHIPID_SHIFT;
-	bcm63xx_cpu_variant = bcm63xx_cpu_id;
+
+	if (long_chipid) {
+		bcm63xx_cpu_id = tmp & REV_LONG_CHIPID_MASK;
+		bcm63xx_cpu_id >>= REV_LONG_CHIPID_SHIFT;
+	} else {
+		bcm63xx_cpu_id = (tmp & REV_CHIPID_MASK) >> REV_CHIPID_SHIFT;
+		varid = (tmp & REV_VARID_MASK) >> REV_VARID_SHIFT;
+	}
+
 	bcm63xx_cpu_rev = (tmp & REV_REVID_MASK) >> REV_REVID_SHIFT;
-	varid = (tmp & REV_VARID_MASK) >> REV_VARID_SHIFT;
+	bcm63xx_cpu_variant = bcm63xx_cpu_id;
 
 	switch (bcm63xx_cpu_id) {
 	case BCM3368_CPU_ID:
@@ -401,6 +443,15 @@ void __init bcm63xx_cpu_init(void)
 		/* BCM6369 is a BCM6368 without xDSL, so treat it the same */
 		bcm63xx_cpu_id = BCM6368_CPU_ID;
 		break;
+	case BCM63168_CPU_ID:
+	case BCM63169_CPU_ID:
+	case BCM63268_CPU_ID:
+	case BCM63269_CPU_ID:
+		bcm63xx_regs_base = bcm63268_regs_base;
+		bcm63xx_irqs = bcm63268_irqs;
+
+		bcm63xx_cpu_id = BCM63268_CPU_ID;
+		break;
 	default:
 		panic("unsupported broadcom CPU %x", bcm63xx_cpu_id);
 		break;
--- a/arch/mips/bcm63xx/dev-flash.c
+++ b/arch/mips/bcm63xx/dev-flash.c
@@ -94,6 +94,12 @@ static int __init bcm63xx_detect_flash_t
 		case STRAPBUS_6368_BOOT_SEL_PARALLEL:
 			return BCM63XX_FLASH_TYPE_PARALLEL;
 		}
+	case BCM63268_CPU_ID:
+		val = bcm_misc_readl(MISC_STRAPBUS_63268_REG);
+		if (val & STRAPBUS_63268_BOOT_SEL_SERIAL)
+			return BCM63XX_FLASH_TYPE_SERIAL;
+		else
+			return BCM63XX_FLASH_TYPE_NAND;
 	default:
 		return -EINVAL;
 	}
--- a/arch/mips/bcm63xx/dev-spi.c
+++ b/arch/mips/bcm63xx/dev-spi.c
@@ -37,7 +37,7 @@ static __init void bcm63xx_spi_regs_init
 	if (BCMCPU_IS_6338() || BCMCPU_IS_6348())
 		bcm63xx_regs_spi = bcm6348_regs_spi;
 	if (BCMCPU_IS_3368() || BCMCPU_IS_6358() ||
-		BCMCPU_IS_6362() || BCMCPU_IS_6368())
+		BCMCPU_IS_6362() || BCMCPU_IS_6368() || BCMCPU_IS_63268())
 		bcm63xx_regs_spi = bcm6358_regs_spi;
 }
 
@@ -85,7 +85,7 @@ int __init bcm63xx_spi_register(void)
 	}
 
 	if (BCMCPU_IS_3368() || BCMCPU_IS_6358() || BCMCPU_IS_6362() ||
-		BCMCPU_IS_6368()) {
+		BCMCPU_IS_6368() || BCMCPU_IS_63268()) {
 		spi_resources[0].end += BCM_6358_RSET_SPI_SIZE - 1;
 		spi_pdata.fifo_size = SPI_6358_MSG_DATA_SIZE;
 		spi_pdata.msg_type_shift = SPI_6358_MSG_TYPE_SHIFT;
--- a/arch/mips/bcm63xx/irq.c
+++ b/arch/mips/bcm63xx/irq.c
@@ -150,6 +150,20 @@ static void bcm63xx_init_irq(void)
 		ext_irqs[5] = BCM_6368_EXT_IRQ5;
 		ext_shift = 4;
 		break;
+	case BCM63268_CPU_ID:
+		periph_bases[0] += PERF_IRQSTAT_63268_REG(0);
+		periph_bases[1] += PERF_IRQSTAT_63268_REG(1);
+		periph_irq_count = 2;
+		periph_width = 4;
+
+		ext_intc_bases[0] += PERF_EXTIRQ_CFG_REG_63268;
+		ext_irq_count = 4;
+		ext_irqs[0] = BCM_63268_EXT_IRQ0;
+		ext_irqs[1] = BCM_63268_EXT_IRQ1;
+		ext_irqs[2] = BCM_63268_EXT_IRQ2;
+		ext_irqs[3] = BCM_63268_EXT_IRQ3;
+		ext_shift = 4;
+		break;
 	default:
 		BUG();
 	}
--- a/arch/mips/bcm63xx/reset.c
+++ b/arch/mips/bcm63xx/reset.c
@@ -125,6 +125,20 @@
 #define BCM6368_RESET_PCIE	0
 #define BCM6368_RESET_PCIE_EXT	0
 
+#define BCM63268_RESET_SPI	SOFTRESET_63268_SPI_MASK
+#define BCM63268_RESET_ENET	0
+#define BCM63268_RESET_USBH	SOFTRESET_63268_USBH_MASK
+#define BCM63268_RESET_USBD	SOFTRESET_63268_USBS_MASK
+#define BCM63268_RESET_DSL	0
+#define BCM63268_RESET_SAR	SOFTRESET_63268_SAR_MASK
+#define BCM63268_RESET_EPHY	0
+#define BCM63268_RESET_ENETSW	SOFTRESET_63268_ENETSW_MASK
+#define BCM63268_RESET_PCM	SOFTRESET_63268_PCM_MASK
+#define BCM63268_RESET_MPI	0
+#define BCM63268_RESET_PCIE	(SOFTRESET_63268_PCIE_MASK | \
+				 SOFTRESET_63268_PCIE_CORE_MASK)
+#define BCM63268_RESET_PCIE_EXT	SOFTRESET_63268_PCIE_EXT_MASK
+
 /*
  * core reset bits
  */
@@ -156,6 +170,10 @@ static const u32 bcm6368_reset_bits[] =
 	__GEN_RESET_BITS_TABLE(6368)
 };
 
+static const u32 bcm63268_reset_bits[] = {
+	__GEN_RESET_BITS_TABLE(63268)
+};
+
 const u32 *bcm63xx_reset_bits;
 static int reset_reg;
 
@@ -182,6 +200,9 @@ static int __init bcm63xx_reset_bits_ini
 	} else if (BCMCPU_IS_6368()) {
 		reset_reg = PERF_SOFTRESET_6368_REG;
 		bcm63xx_reset_bits = bcm6368_reset_bits;
+	} else if (BCMCPU_IS_63268()) {
+		reset_reg = PERF_SOFTRESET_63268_REG;
+		bcm63xx_reset_bits = bcm63268_reset_bits;
 	}
 
 	return 0;
--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h
@@ -21,6 +21,10 @@
 #define BCM6362_CPU_ID		0x6362
 #define BCM6368_CPU_ID		0x6368
 #define BCM6369_CPU_ID		0x6369
+#define BCM63168_CPU_ID		0x63168
+#define BCM63169_CPU_ID		0x63169
+#define BCM63268_CPU_ID		0x63268
+#define BCM63269_CPU_ID		0x63269
 
 void __init bcm63xx_cpu_init(void);
 u32 bcm63xx_get_cpu_variant(void);
@@ -61,6 +65,10 @@ static inline u32 __pure __bcm63xx_get_c
 #ifdef CONFIG_BCM63XX_CPU_6368
 		case BCM6368_CPU_ID:
 #endif
+
+#ifdef CONFIG_BCM63XX_CPU_63268
+		case BCM63268_CPU_ID:
+#endif
 		break;
 	default:
 		unreachable();
@@ -86,6 +94,7 @@ static inline u32 __pure bcm63xx_get_cpu
 #define BCMCPU_IS_6358()	(bcm63xx_get_cpu_id() == BCM6358_CPU_ID)
 #define BCMCPU_IS_6362()	(bcm63xx_get_cpu_id() == BCM6362_CPU_ID)
 #define BCMCPU_IS_6368()	(bcm63xx_get_cpu_id() == BCM6368_CPU_ID)
+#define BCMCPU_IS_63268()	(bcm63xx_get_cpu_id() == BCM63268_CPU_ID)
 
 #define BCMCPU_VARIANT_IS_3368() \
 	(bcm63xx_get_cpu_variant() == BCM3368_CPU_ID)
@@ -109,6 +118,14 @@ static inline u32 __pure bcm63xx_get_cpu
 	(bcm63xx_get_cpu_variant() == BCM6368_CPU_ID)
 #define BCMCPU_VARIANT_IS_6369() \
 	(bcm63xx_get_cpu_variant() == BCM6369_CPU_ID)
+#define BCMCPU_VARIANT_IS_63168() \
+	(bcm63xx_get_cpu_variant() == BCM63168_CPU_ID)
+#define BCMCPU_VARIANT_IS_63169() \
+	(bcm63xx_get_cpu_variant() == BCM63169_CPU_ID)
+#define BCMCPU_VARIANT_IS_63268() \
+	(bcm63xx_get_cpu_variant() == BCM63268_CPU_ID)
+#define BCMCPU_VARIANT_IS_63269() \
+	(bcm63xx_get_cpu_variant() == BCM63269_CPU_ID)
 
 /*
  * While registers sets are (mostly) the same across 63xx CPU, base
@@ -573,6 +590,52 @@ enum bcm63xx_regs_set {
 #define BCM_6368_RNG_BASE		(0xb0004180)
 #define BCM_6368_MISC_BASE		(0xdeadbeef)
 
+/*
+ * 63268 register sets base address
+ */
+#define BCM_63268_DSL_LMEM_BASE		(0xdeadbeef)
+#define BCM_63268_PERF_BASE		(0xb0000000)
+#define BCM_63268_TIMER_BASE		(0xb0000080)
+#define BCM_63268_WDT_BASE		(0xb000009c)
+#define BCM_63268_UART0_BASE		(0xb0000180)
+#define BCM_63268_UART1_BASE		(0xb00001a0)
+#define BCM_63268_GPIO_BASE		(0xb00000c0)
+#define BCM_63268_SPI_BASE		(0xb0000800)
+#define BCM_63268_HSSPI_BASE		(0xb0001000)
+#define BCM_63268_UDC0_BASE		(0xdeadbeef)
+#define BCM_63268_USBDMA_BASE		(0xb000c800)
+#define BCM_63268_OHCI0_BASE		(0xb0002600)
+#define BCM_63268_OHCI_PRIV_BASE	(0xdeadbeef)
+#define BCM_63268_USBH_PRIV_BASE	(0xb0002700)
+#define BCM_63268_USBD_BASE		(0xb0002400)
+#define BCM_63268_MPI_BASE		(0xdeadbeef)
+#define BCM_63268_PCMCIA_BASE		(0xdeadbeef)
+#define BCM_63268_PCIE_BASE		(0xb06e0000)
+#define BCM_63268_SDRAM_REGS_BASE	(0xdeadbeef)
+#define BCM_63268_DSL_BASE		(0xdeadbeef)
+#define BCM_63268_UBUS_BASE		(0xdeadbeef)
+#define BCM_63268_ENET0_BASE		(0xdeadbeef)
+#define BCM_63268_ENET1_BASE		(0xdeadbeef)
+#define BCM_63268_ENETDMA_BASE		(0xb000d800)
+#define BCM_63268_ENETDMAC_BASE		(0xb000da00)
+#define BCM_63268_ENETDMAS_BASE		(0xb000dc00)
+#define BCM_63268_ENETSW_BASE		(0xb0700000)
+#define BCM_63268_EHCI0_BASE		(0xb0002500)
+#define BCM_63268_SDRAM_BASE		(0xdeadbeef)
+#define BCM_63268_MEMC_BASE		(0xdeadbeef)
+#define BCM_63268_DDR_BASE		(0xb0003000)
+#define BCM_63268_M2M_BASE		(0xdeadbeef)
+#define BCM_63268_ATM_BASE		(0xdeadbeef)
+#define BCM_63268_XTM_BASE		(0xb0007000)
+#define BCM_63268_XTMDMA_BASE		(0xb000b800)
+#define BCM_63268_XTMDMAC_BASE		(0xdeadbeef)
+#define BCM_63268_XTMDMAS_BASE		(0xdeadbeef)
+#define BCM_63268_PCM_BASE		(0xb000b000)
+#define BCM_63268_PCMDMA_BASE		(0xb000b800)
+#define BCM_63268_PCMDMAC_BASE		(0xdeadbeef)
+#define BCM_63268_PCMDMAS_BASE		(0xdeadbeef)
+#define BCM_63268_RNG_BASE		(0xdeadbeef)
+#define BCM_63268_MISC_BASE		(0xb0001800)
 
 extern const unsigned long *bcm63xx_regs_base;
 
@@ -1086,6 +1149,73 @@ enum bcm63xx_irq {
 #define BCM_6368_EXT_IRQ4		(IRQ_INTERNAL_BASE + 24)
 #define BCM_6368_EXT_IRQ5		(IRQ_INTERNAL_BASE + 25)
 
+/*
+ * 63268 irqs
+ */
+#define BCM_63268_HIGH_IRQ_BASE		(IRQ_INTERNAL_BASE + 32)
+#define BCM_63268_VERY_HIGH_IRQ_BASE	(BCM_63268_HIGH_IRQ_BASE + 32)
+
+#define BCM_63268_TIMER_IRQ		(IRQ_INTERNAL_BASE + 0)
+#define BCM_63268_SPI_IRQ		(BCM_63268_VERY_HIGH_IRQ_BASE + 16)
+#define BCM_63268_UART0_IRQ		(IRQ_INTERNAL_BASE + 5)
+#define BCM_63268_UART1_IRQ		(BCM_63268_HIGH_IRQ_BASE + 2)
+#define BCM_63268_DSL_IRQ		(IRQ_INTERNAL_BASE + 23)
+#define BCM_63268_UDC0_IRQ		0
+#define BCM_63268_ENET0_IRQ		0
+#define BCM_63268_ENET1_IRQ		0
+#define BCM_63268_ENET_PHY_IRQ		(IRQ_INTERNAL_BASE + 13)
+#define BCM_63268_HSSPI_IRQ		(IRQ_INTERNAL_BASE + 6)
+#define BCM_63268_OHCI0_IRQ		(IRQ_INTERNAL_BASE + 9)
+#define BCM_63268_EHCI0_IRQ		(IRQ_INTERNAL_BASE + 10)
+#define BCM_63268_USBD_IRQ		(IRQ_INTERNAL_BASE + 11)
+#define BCM_63268_USBD_RXDMA0_IRQ	(IRQ_INTERNAL_BASE + 19)
+#define BCM_63268_USBD_TXDMA0_IRQ	(BCM_63268_HIGH_IRQ_BASE + 4)
+#define BCM_63268_USBD_RXDMA1_IRQ	(IRQ_INTERNAL_BASE + 20)
+#define BCM_63268_USBD_TXDMA1_IRQ	(BCM_63268_HIGH_IRQ_BASE + 5)
+#define BCM_63268_USBD_RXDMA2_IRQ	(IRQ_INTERNAL_BASE + 21)
+#define BCM_63268_USBD_TXDMA2_IRQ	(BCM_63268_HIGH_IRQ_BASE + 6)
+#define BCM_63268_PCMCIA_IRQ		0
+#define BCM_63268_ENET0_RXDMA_IRQ	0
+#define BCM_63268_ENET0_TXDMA_IRQ	0
+#define BCM_63268_ENET1_RXDMA_IRQ	0
+#define BCM_63268_ENET1_TXDMA_IRQ	0
+#define BCM_63268_PCI_IRQ		(BCM_63268_HIGH_IRQ_BASE + 8)
+#define BCM_63268_ATM_IRQ		0
+#define BCM_63268_ENETSW_RXDMA0_IRQ	(IRQ_INTERNAL_BASE + 1)
+#define BCM_63268_ENETSW_RXDMA1_IRQ	(IRQ_INTERNAL_BASE + 2)
+#define BCM_63268_ENETSW_RXDMA2_IRQ	(IRQ_INTERNAL_BASE + 3)
+#define BCM_63268_ENETSW_RXDMA3_IRQ	(IRQ_INTERNAL_BASE + 4)
+#define BCM_63268_ENETSW_TXDMA0_IRQ	(BCM_63268_VERY_HIGH_IRQ_BASE + 0)
+#define BCM_63268_ENETSW_TXDMA1_IRQ	(BCM_63268_VERY_HIGH_IRQ_BASE + 1)
+#define BCM_63268_ENETSW_TXDMA2_IRQ	(BCM_63268_VERY_HIGH_IRQ_BASE + 2)
+#define BCM_63268_ENETSW_TXDMA3_IRQ	(BCM_63268_VERY_HIGH_IRQ_BASE + 3)
+#define BCM_63268_XTM_IRQ		(BCM_63268_HIGH_IRQ_BASE + 17)
+#define BCM_63268_XTM_DMA0_IRQ		(IRQ_INTERNAL_BASE + 26)
+
+#define BCM_63268_RING_OSC_IRQ		(BCM_63268_HIGH_IRQ_BASE + 20)
+#define BCM_63268_WLAN_GPIO_IRQ		(BCM_63268_HIGH_IRQ_BASE + 3)
+#define BCM_63268_WLAN_IRQ		(IRQ_INTERNAL_BASE + 7)
+#define BCM_63268_IPSEC_IRQ		(IRQ_INTERNAL_BASE + 8)
+#define BCM_63268_NAND_IRQ		(BCM_63268_HIGH_IRQ_BASE + 18)
+#define BCM_63268_PCM_IRQ		(IRQ_INTERNAL_BASE + 13)
+#define BCM_63268_DG_IRQ		(IRQ_INTERNAL_BASE + 15)
+#define BCM_63268_EPHY_ENERGY0_IRQ	(IRQ_INTERNAL_BASE + 16)
+#define BCM_63268_EPHY_ENERGY1_IRQ	(IRQ_INTERNAL_BASE + 17)
+#define BCM_63268_EPHY_ENERGY2_IRQ	(IRQ_INTERNAL_BASE + 18)
+#define BCM_63268_EPHY_ENERGY3_IRQ	(IRQ_INTERNAL_BASE + 19)
+#define BCM_63268_IPSEC_DMA0_IRQ	(IRQ_INTERNAL_BASE + 22)
+#define BCM_63268_IPSEC_DMA1_IRQ	(BCM_63268_HIGH_IRQ_BASE + 7)
+#define BCM_63268_FAP0_IRQ		(IRQ_INTERNAL_BASE + 24)
+#define BCM_63268_FAP1_IRQ		(IRQ_INTERNAL_BASE + 25)
+#define BCM_63268_PCM_DMA0_IRQ		(BCM_63268_HIGH_IRQ_BASE + 10)
+#define BCM_63268_PCM_DMA1_IRQ		(BCM_63268_HIGH_IRQ_BASE + 11)
+#define BCM_63268_DECT0_IRQ		(BCM_63268_HIGH_IRQ_BASE + 0)
+#define BCM_63268_DECT1_IRQ		(BCM_63268_HIGH_IRQ_BASE + 1)
+#define BCM_63268_EXT_IRQ0		(BCM_63268_HIGH_IRQ_BASE + 12)
+#define BCM_63268_EXT_IRQ1		(BCM_63268_HIGH_IRQ_BASE + 13)
+#define BCM_63268_EXT_IRQ2		(BCM_63268_HIGH_IRQ_BASE + 14)
+#define BCM_63268_EXT_IRQ3		(BCM_63268_HIGH_IRQ_BASE + 15)
+
 extern const int *bcm63xx_irqs;
 
 #define __GEN_CPU_IRQ_TABLE(__cpu)					\
--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_gpio.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_gpio.h
@@ -22,6 +22,8 @@ static inline unsigned long bcm63xx_gpio
 		return 48;
 	case BCM6368_CPU_ID:
 		return 38;
+	case BCM63268_CPU_ID:
+		return 52;
 	case BCM6348_CPU_ID:
 	default:
 		return 37;
--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h
@@ -9,6 +9,8 @@
 #define PERF_REV_REG			0x0
 #define REV_CHIPID_SHIFT		16
 #define REV_CHIPID_MASK			(0xffff << REV_CHIPID_SHIFT)
+#define REV_LONG_CHIPID_SHIFT		12
+#define REV_LONG_CHIPID_MASK		(0xfffff << REV_LONG_CHIPID_SHIFT)
 #define REV_VARID_SHIFT			12
 #define REV_VARID_MASK			(0xf << REV_VARID_SHIFT)
 #define REV_REVID_SHIFT			0
@@ -211,6 +213,52 @@
 					CKCTL_6368_NAND_EN |		\
 					CKCTL_6368_IPSEC_EN)
 
+#define CKCTL_63268_DISABLE_GLESS	(1 << 0)
+#define CKCTL_63268_VDSL_QPROC_EN	(1 << 1)
+#define CKCTL_63268_VDSL_AFE_EN		(1 << 2)
+#define CKCTL_63268_VDSL_EN		(1 << 3)
+#define CKCTL_63268_MIPS_EN		(1 << 4)
+#define CKCTL_63268_WLAN_OCP_EN		(1 << 5)
+#define CKCTL_63268_DECT_EN		(1 << 6)
+#define CKCTL_63268_FAP0_EN		(1 << 7)
+#define CKCTL_63268_FAP1_EN		(1 << 8)
+#define CKCTL_63268_SAR_EN		(1 << 9)
+#define CKCTL_63268_ROBOSW_EN		(1 << 10)
+#define CKCTL_63268_PCM_EN		(1 << 11)
+#define CKCTL_63268_USBD_EN		(1 << 12)
+#define CKCTL_63268_USBH_EN		(1 << 13)
+#define CKCTL_63268_IPSEC_EN		(1 << 14)
+#define CKCTL_63268_SPI_EN		(1 << 15)
+#define CKCTL_63268_HSSPI_EN		(1 << 16)
+#define CKCTL_63268_PCIE_EN		(1 << 17)
+#define CKCTL_63268_PHYMIPS_EN		(1 << 18)
+#define CKCTL_63268_GMAC_EN		(1 << 19)
+#define CKCTL_63268_NAND_EN		(1 << 20)
+#define CKCTL_63268_TBUS_EN		(1 << 27)
+#define CKCTL_63268_ROBOSW250_EN	(1 << 31)
+
+#define CKCTL_63268_ALL_SAFE_EN		(CKCTL_63268_VDSL_QPROC_EN |	\
+					CKCTL_63268_VDSL_AFE_EN |	\
+					CKCTL_63268_VDSL_EN |		\
+					CKCTL_63268_WLAN_OCP_EN |	\
+					CKCTL_63268_DECT_EN |		\
+					CKCTL_63268_FAP0_EN |		\
+					CKCTL_63268_FAP1_EN |		\
+					CKCTL_63268_SAR_EN |		\
+					CKCTL_63268_ROBOSW_EN |		\
+					CKCTL_63268_PCM_EN |		\
+					CKCTL_63268_USBD_EN |		\
+					CKCTL_63268_USBH_EN |		\
+					CKCTL_63268_IPSEC_EN |		\
+					CKCTL_63268_SPI_EN |		\
+					CKCTL_63268_HSSPI_EN |		\
+					CKCTL_63268_PCIE_EN |		\
+					CKCTL_63268_PHYMIPS_EN |	\
+					CKCTL_63268_GMAC_EN |		\
+					CKCTL_63268_NAND_EN |		\
+					CKCTL_63268_TBUS_EN |		\
+					CKCTL_63268_ROBOSW250_EN)
+
 /* System PLL Control register	*/
 #define PERF_SYS_PLL_CTL_REG		0x8
 #define SYS_PLL_SOFT_RESET		0x1
@@ -224,6 +272,7 @@
 #define PERF_IRQMASK_6358_REG(x)	(0xc + (x) * 0x2c)
 #define PERF_IRQMASK_6362_REG(x)	(0x20 + (x) * 0x10)
 #define PERF_IRQMASK_6368_REG(x)	(0x20 + (x) * 0x10)
+#define PERF_IRQMASK_63268_REG(x)	(0x20 + (x) * 0x20)
 
 /* Interrupt Status register */
 #define PERF_IRQSTAT_3368_REG		0x10
@@ -234,6 +283,7 @@
 #define PERF_IRQSTAT_6358_REG(x)	(0x10 + (x) * 0x2c)
 #define PERF_IRQSTAT_6362_REG(x)	(0x28 + (x) * 0x10)
 #define PERF_IRQSTAT_6368_REG(x)	(0x28 + (x) * 0x10)
+#define PERF_IRQSTAT_63268_REG(x)	(0x30 + (x) * 0x20)
 
 /* External Interrupt Configuration register */
 #define PERF_EXTIRQ_CFG_REG_3368	0x14
@@ -244,6 +294,7 @@
 #define PERF_EXTIRQ_CFG_REG_6358	0x14
 #define PERF_EXTIRQ_CFG_REG_6362	0x18
 #define PERF_EXTIRQ_CFG_REG_6368	0x18
+#define PERF_EXTIRQ_CFG_REG_63268	0x18
 
 #define PERF_EXTIRQ_CFG_REG2_6358	0x1c
 #define PERF_EXTIRQ_CFG_REG2_6368	0x1c
@@ -274,6 +325,7 @@
 #define PERF_SOFTRESET_6358_REG		0x34
 #define PERF_SOFTRESET_6362_REG		0x10
 #define PERF_SOFTRESET_6368_REG		0x10
+#define PERF_SOFTRESET_63268_REG	0x10
 
 #define SOFTRESET_3368_SPI_MASK		(1 << 0)
 #define SOFTRESET_3368_ENET_MASK	(1 << 2)
@@ -367,6 +419,26 @@
 #define SOFTRESET_6368_USBH_MASK	(1 << 12)
 #define SOFTRESET_6368_PCM_MASK		(1 << 13)
 
+#define SOFTRESET_63268_SPI_MASK	(1 << 0)
+#define SOFTRESET_63268_IPSEC_MASK	(1 << 1)
+#define SOFTRESET_63268_EPHY_MASK	(1 << 2)
+#define SOFTRESET_63268_SAR_MASK	(1 << 3)
+#define SOFTRESET_63268_ENETSW_MASK	(1 << 4)
+#define SOFTRESET_63268_USBS_MASK	(1 << 5)
+#define SOFTRESET_63268_USBH_MASK	(1 << 6)
+#define SOFTRESET_63268_PCM_MASK	(1 << 7)
+#define SOFTRESET_63268_PCIE_CORE_MASK	(1 << 8)
+#define SOFTRESET_63268_PCIE_MASK	(1 << 9)
+#define SOFTRESET_63268_PCIE_EXT_MASK	(1 << 10)
+#define SOFTRESET_63268_WLAN_SHIM_MASK	(1 << 11)
+#define SOFTRESET_63268_DDR_PHY_MASK	(1 << 12)
+#define SOFTRESET_63268_FAP0_MASK	(1 << 13)
+#define SOFTRESET_63268_WLAN_UBUS_MASK	(1 << 14)
+#define SOFTRESET_63268_DECT_MASK	(1 << 15)
+#define SOFTRESET_63268_FAP1_MASK	(1 << 16)
+#define SOFTRESET_63268_PCIE_HARD_MASK	(1 << 17)
+#define SOFTRESET_63268_GPHY_MASK	(1 << 18)
+
 /* MIPS PLL control register */
 #define PERF_MIPSPLLCTL_REG		0x34
 #define MIPSPLLCTL_N1_SHIFT		20
@@ -1380,6 +1452,13 @@
 #define STRAPBUS_6362_BOOT_SEL_SERIAL	(1 << 15)
 #define STRAPBUS_6362_BOOT_SEL_NAND	(0 << 15)
 
+#define MISC_STRAPBUS_63268_REG		0x14
+#define STRAPBUS_63268_HSSPI_CLK_FAST	(1 << 9)
+#define STRAPBUS_63268_BOOT_SEL_SERIAL	(1 << 11)
+#define STRAPBUS_63268_BOOT_SEL_NAND	(0 << 11)
+#define STRAPBUS_63268_FCVO_SHIFT	21
+#define STRAPBUS_63268_FCVO_MASK	(0xf << STRAPBUS_63268_FCVO_SHIFT)
+
 #define MISC_STRAPBUS_6328_REG		0x240
 #define STRAPBUS_6328_FCVO_SHIFT	7
 #define STRAPBUS_6328_FCVO_MASK		(0x1f << STRAPBUS_6328_FCVO_SHIFT)
--- a/arch/mips/include/asm/mach-bcm63xx/ioremap.h
+++ b/arch/mips/include/asm/mach-bcm63xx/ioremap.h
@@ -25,6 +25,7 @@ static inline int is_bcm63xx_internal_re
 	case BCM6328_CPU_ID:
 	case BCM6362_CPU_ID:
 	case BCM6368_CPU_ID:
+	case BCM63268_CPU_ID:
 		if (offset >= 0xb0000000 && offset < 0xb1000000)
 			return 1;
 		break;
--- a/arch/mips/bcm63xx/dev-hsspi.c
+++ b/arch/mips/bcm63xx/dev-hsspi.c
@@ -35,7 +35,7 @@ static struct platform_device bcm63xx_hs
 
 int __init bcm63xx_hsspi_register(void)
 {
-	if (!BCMCPU_IS_6328() && !BCMCPU_IS_6362())
+	if (!BCMCPU_IS_6328() && !BCMCPU_IS_6362() && !BCMCPU_IS_63268())
 		return -ENODEV;
 
 	spi_resources[0].start = bcm63xx_regset_address(RSET_HSSPI);
--- a/arch/mips/bcm63xx/dev-enet.c
+++ b/arch/mips/bcm63xx/dev-enet.c
@@ -176,7 +176,8 @@ static int __init register_shared(void)
 	else
 		shared_res[0].end += (RSET_ENETDMA_SIZE)  - 1;
 
-	if (BCMCPU_IS_6328() || BCMCPU_IS_6362() || BCMCPU_IS_6368())
+	if (BCMCPU_IS_6328() || BCMCPU_IS_6362() || BCMCPU_IS_6368() ||
+		BCMCPU_IS_63268())
 		chan_count = 32;
 	else if (BCMCPU_IS_6345())
 		chan_count = 8;
@@ -276,7 +277,8 @@ bcm63xx_enetsw_register(const struct bcm
 {
 	int ret;
 
-	if (!BCMCPU_IS_6328() && !BCMCPU_IS_6362() && !BCMCPU_IS_6368())
+	if (!BCMCPU_IS_6328() && !BCMCPU_IS_6362() && !BCMCPU_IS_6368() &&
+		!BCMCPU_IS_63268())
 		return -ENODEV;
 
 	ret = register_shared();
@@ -295,8 +297,11 @@ bcm63xx_enetsw_register(const struct bcm
 
 	if (BCMCPU_IS_6328())
 		enetsw_pd.num_ports = ENETSW_PORTS_6328;
-	else if (BCMCPU_IS_6362() || BCMCPU_IS_6368())
+	else if (BCMCPU_IS_6362() || BCMCPU_IS_6368() ||
+		 BCMCPU_VARIANT_IS_63168() || BCMCPU_VARIANT_IS_63169())
 		enetsw_pd.num_ports = ENETSW_PORTS_6368;
+	else if (BCMCPU_VARIANT_IS_63268() ||  BCMCPU_VARIANT_IS_63269())
+		enetsw_pd.num_ports = ENETSW_PORTS_63268;
 
 	enetsw_pd.dma_has_sram = true;
 	enetsw_pd.dma_chan_width = ENETDMA_CHAN_WIDTH;
--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_dev_enet.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_dev_enet.h
@@ -62,6 +62,7 @@ struct bcm63xx_enet_platform_data {
 #define ENETSW_MAX_PORT	8
 #define ENETSW_PORTS_6328 5 /* 4 FE PHY + 1 RGMII */
 #define ENETSW_PORTS_6368 6 /* 4 FE PHY + 2 RGMII */
+#define ENETSW_PORTS_63268 8 /* 3 FE PHY + 1 GE PHY + 4 RGMII */
 
 #define ENETSW_RGMII_PORT0	4
 
