From fbd3b188fbaa861165a074c454d8f8dcf15343a0 Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Mon, 8 Dec 2014 08:47:10 +0100
Subject: [PATCH 3/4] bgmac: activate irqs only if there is nothing to poll

IRQs should only get activated when there is nothing to poll in the
queue any more and to after every poll.

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
---
 drivers/net/ethernet/broadcom/bgmac.c | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/drivers/net/ethernet/broadcom/bgmac.c
+++ b/drivers/net/ethernet/broadcom/bgmac.c
@@ -1167,10 +1167,10 @@ static int bgmac_poll(struct napi_struct
 		bgmac->int_status = 0;
 	}
 
-	if (handled < weight)
+	if (handled < weight) {
 		napi_complete(napi);
-
-	bgmac_chip_intrs_on(bgmac);
+		bgmac_chip_intrs_on(bgmac);
+	}
 
 	return handled;
 }
