From cf454a47b64ef78ff85b097c8cb404120c14e6a5 Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Fri, 3 Jan 2014 10:27:51 +0100
Subject: [PATCH] ARM: sun7i: dt: Add ahci / sata support

This patch adds sunxi sata support to A20 boards that have such a connector.
Some boards also feature a regulator via a GPIO and support for this is also
added.

Signed-off-by: Olliver Schinagl <oliver@schinagl.nl>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20-cubieboard2.dts     | 10 ++++++++++
 arch/arm/boot/dts/sun7i-a20-cubietruck.dts      | 19 +++++++++++++++++++
 arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts | 10 ++++++++++
 arch/arm/boot/dts/sun7i-a20.dtsi                |  8 ++++++++
 4 files changed, 47 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
@@ -13,12 +13,18 @@
 
 /dts-v1/;
 /include/ "sun7i-a20.dtsi"
+/include/ "sunxi-common-regulators.dtsi"
 
 / {
 	model = "Cubietech Cubieboard2";
 	compatible = "cubietech,cubieboard2", "allwinner,sun7i-a20";
 
 	soc@01c00000 {
+		ahci: sata@01c18000 {
+			target-supply = <&reg_ahci_5v>;
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
 			led_pins_cubieboard2: led_pins@0 {
 				allwinner,pins = "PH20", "PH21";
@@ -74,4 +80,8 @@
 			gpios = <&pio 7 20 0>;
 		};
 	};
+
+	reg_ahci_5v: ahci-5v {
+		status = "okay";
+	};
 };
--- a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
@@ -13,13 +13,26 @@
 
 /dts-v1/;
 /include/ "sun7i-a20.dtsi"
+/include/ "sunxi-common-regulators.dtsi"
 
 / {
 	model = "Cubietech Cubietruck";
 	compatible = "cubietech,cubietruck", "allwinner,sun7i-a20";
 
 	soc@01c00000 {
+		ahci: sata@01c18000 {
+			target-supply = <&reg_ahci_5v>;
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
+			ahci_pwr_pin_cubietruck: ahci_pwr_pin@1 {
+				allwinner,pins = "PH12";
+				allwinner,function = "gpio_out";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
 			led_pins_cubietruck: led_pins@0 {
 				allwinner,pins = "PH7", "PH11", "PH20", "PH21";
 				allwinner,function = "gpio_out";
@@ -104,4 +117,10 @@
 			gpios = <&pio 7 7 0>;
 		};
 	};
+
+	reg_ahci_5v: ahci-5v {
+		pinctrl-0 = <&ahci_pwr_pin_cubietruck>;
+		gpio = <&pio 7 12 0>;
+		status = "okay";
+	};
 };
--- a/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
+++ b/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
@@ -13,6 +13,7 @@
 
 /dts-v1/;
 /include/ "sun7i-a20.dtsi"
+/include/ "sunxi-common-regulators.dtsi"
 
 / {
 	model = "Olimex A20-Olinuxino Micro";
@@ -36,6 +37,11 @@
 			status = "okay";
 		};
 
+		ahci: sata@01c18000 {
+			target-supply = <&reg_ahci_5v>;
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
 			led_pins_olinuxino: led_pins@0 {
 				allwinner,pins = "PH2";
@@ -105,4 +111,8 @@
 			default-state = "on";
 		};
 	};
+
+	reg_ahci_5v: ahci-5v {
+		status = "okay";
+	};
 };
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -450,6 +450,14 @@
 			#size-cells = <0>;
 		};
 
+		ahci: sata@01c18000 {
+			compatible = "allwinner,sun4i-a10-ahci";
+			reg = <0x01c18000 0x1000>;
+			interrupts = <0 56 4>;
+			clocks = <&pll6 0>, <&ahb_gates 25>;
+			status = "disabled";
+		};
+
 		spi3: spi@01c1f000 {
 			compatible = "allwinner,sun4i-a10-spi";
 			reg = <0x01c1f000 0x1000>;
