--- a/drivers/mtd/nand/Kconfig
+++ b/drivers/mtd/nand/Kconfig
@@ -510,4 +510,12 @@ config MTD_NAND_XWAY
 	  Enables support for NAND Flash chips on Lantiq XWAY SoCs. NAND is attached
 	  to the External Bus Unit (EBU).
 
+config MTD_NAND_OXNAS
+	tristate "Support for NAND on Plxtech NAS782X SoC"
+	depends on ARCH_OXNAS
+	select MTD_NAND_PLATFORM
+	help
+	  Enables support for NAND Flash chips on Plxtech NAS782X SoCs. NAND is attached
+	  to the STATIC Unit.
+
 endif # MTD_NAND
--- a/drivers/mtd/nand/Makefile
+++ b/drivers/mtd/nand/Makefile
@@ -49,5 +49,6 @@ obj-$(CONFIG_MTD_NAND_JZ4740)		+= jz4740
 obj-$(CONFIG_MTD_NAND_GPMI_NAND)	+= gpmi-nand/
 obj-$(CONFIG_MTD_NAND_XWAY)		+= xway_nand.o
 obj-$(CONFIG_MTD_NAND_BCM47XXNFLASH)	+= bcm47xxnflash/
+obj-$(CONFIG_MTD_NAND_OXNAS)		+= oxnas_nand.o
 
 nand-objs := nand_base.o nand_bbt.o
