From 7177efc5b030012c54c2e217c9d6decc0bcc1c53 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Tue, 28 Oct 2014 13:30:23 +0100
Subject: [PATCH 156/158] MIPS: BCM47XX: Make bcma init NVRAM instead of
 bcm47xx polling it
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This drops ssb/bcma dependency and will allow us to make it a standalone
driver.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Cc: linux-mips@linux-mips.org
Cc: Hauke Mehrtens <hauke@hauke-m.de>
Patchwork: https://patchwork.linux-mips.org/patch/8233/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/bcm47xx/nvram.c  | 42 ++----------------------------------------
 drivers/bcma/driver_mips.c | 13 +++++++++++--
 2 files changed, 13 insertions(+), 42 deletions(-)

diff --git a/arch/mips/bcm47xx/nvram.c b/arch/mips/bcm47xx/nvram.c
index fecc5ae..21712fb 100644
--- a/arch/mips/bcm47xx/nvram.c
+++ b/arch/mips/bcm47xx/nvram.c
@@ -121,48 +121,10 @@ int bcm47xx_nvram_init_from_mem(u32 base, u32 lim)
 	return err;
 }
 
-#ifdef CONFIG_BCM47XX_BCMA
-static int nvram_init_bcma(void)
-{
-	struct bcma_drv_cc *cc = &bcm47xx_bus.bcma.bus.drv_cc;
-	u32 base;
-	u32 lim;
-
-#ifdef CONFIG_BCMA_NFLASH
-	if (cc->nflash.boot) {
-		base = BCMA_SOC_FLASH1;
-		lim = BCMA_SOC_FLASH1_SZ;
-	} else
-#endif
-	if (cc->pflash.present) {
-		base = cc->pflash.window;
-		lim = cc->pflash.window_size;
-#ifdef CONFIG_BCMA_SFLASH
-	} else if (cc->sflash.present) {
-		base = cc->sflash.window;
-		lim = cc->sflash.size;
-#endif
-	} else {
-		pr_err("Couldn't find supported flash memory\n");
-		return -ENXIO;
-	}
-
-	return bcm47xx_nvram_init_from_mem(base, lim);
-}
-#endif
-
 static int nvram_init(void)
 {
-	switch (bcm47xx_bus_type) {
-#ifdef CONFIG_BCM47XX_SSB
-	case BCM47XX_BUS_TYPE_SSB:
-		break;
-#endif
-#ifdef CONFIG_BCM47XX_BCMA
-	case BCM47XX_BUS_TYPE_BCMA:
-		return nvram_init_bcma();
-#endif
-	}
+	/* TODO: Look for MTD "nvram" partition */
+
 	return -ENXIO;
 }
 
diff --git a/drivers/bcma/driver_mips.c b/drivers/bcma/driver_mips.c
index 004d6aa..8a653dc 100644
--- a/drivers/bcma/driver_mips.c
+++ b/drivers/bcma/driver_mips.c
@@ -20,6 +20,9 @@
 #include <linux/serial_core.h>
 #include <linux/serial_reg.h>
 #include <linux/time.h>
+#ifdef CONFIG_BCM47XX
+#include <bcm47xx_nvram.h>
+#endif
 
 enum bcma_boot_dev {
 	BCMA_BOOT_DEV_UNK = 0,
@@ -316,10 +319,16 @@ static void bcma_core_mips_flash_detect(struct bcma_drv_mips *mcore)
 	switch (boot_dev) {
 	case BCMA_BOOT_DEV_PARALLEL:
 	case BCMA_BOOT_DEV_SERIAL:
-		/* TODO: Init NVRAM using BCMA_SOC_FLASH2 window */
+#ifdef CONFIG_BCM47XX
+		bcm47xx_nvram_init_from_mem(BCMA_SOC_FLASH2,
+					    BCMA_SOC_FLASH2_SZ);
+#endif
 		break;
 	case BCMA_BOOT_DEV_NAND:
-		/* TODO: Init NVRAM using BCMA_SOC_FLASH1 window */
+#ifdef CONFIG_BCM47XX
+		bcm47xx_nvram_init_from_mem(BCMA_SOC_FLASH1,
+					    BCMA_SOC_FLASH1_SZ);
+#endif
 		break;
 	default:
 		break;
-- 
1.8.4.5

