Add properties to the gpio nodes to allow them to be also used
as pwm lines.

Signed-off-by: Andrew Lunn <andrew@lunn.ch>
---
 arch/arm/boot/dts/armada-370.dtsi        | 10 ++++++++--
 arch/arm/boot/dts/armada-xp-mv78230.dtsi | 10 ++++++++--
 arch/arm/boot/dts/armada-xp-mv78260.dtsi |  8 ++++++--
 arch/arm/boot/dts/armada-xp-mv78460.dtsi | 10 ++++++++--
 4 files changed, 30 insertions(+), 8 deletions(-)

--- a/arch/arm/boot/dts/armada-370.dtsi
+++ b/arch/arm/boot/dts/armada-370.dtsi
@@ -109,24 +109,30 @@
 
 			gpio0: gpio@18100 {
 				compatible = "marvell,orion-gpio";
-				reg = <0x18100 0x40>;
+				reg = <0x18100 0x40>, <0x181c0 0x08>;
+				reg-names = "gpio", "pwm";
 				ngpios = <32>;
 				gpio-controller;
 				#gpio-cells = <2>;
+				#pwm-cells = <2>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
 				interrupts = <82>, <83>, <84>, <85>;
+				clocks = <&coreclk 0>;
 			};
 
 			gpio1: gpio@18140 {
 				compatible = "marvell,orion-gpio";
-				reg = <0x18140 0x40>;
+				reg = <0x18140 0x40>, <0x181c8 0x08>;
+				reg-names = "gpio", "pwm";
 				ngpios = <32>;
 				gpio-controller;
 				#gpio-cells = <2>;
+				#pwm-cells = <2>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
 				interrupts = <87>, <88>, <89>, <90>;
+				clocks = <&coreclk 0>;
 			};
 
 			gpio2: gpio@18180 {
--- a/arch/arm/boot/dts/armada-xp-mv78230.dtsi
+++ b/arch/arm/boot/dts/armada-xp-mv78230.dtsi
@@ -169,24 +169,30 @@
 		internal-regs {
 			gpio0: gpio@18100 {
 				compatible = "marvell,orion-gpio";
-				reg = <0x18100 0x40>;
+				reg = <0x18100 0x40>, <0x181c0 0x08>;
+				reg-names = "gpio", "pwm";
 				ngpios = <32>;
 				gpio-controller;
 				#gpio-cells = <2>;
+				#pwm-cells = <2>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
 				interrupts = <82>, <83>, <84>, <85>;
+				clocks = <&coreclk 0>;
 			};
 
 			gpio1: gpio@18140 {
 				compatible = "marvell,orion-gpio";
-				reg = <0x18140 0x40>;
+				reg = <0x18140 0x40>, <0x181c8 0x08>;
+				reg-names = "gpio", "pwm";
 				ngpios = <17>;
 				gpio-controller;
 				#gpio-cells = <2>;
+				#pwm-cells = <2>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
 				interrupts = <87>, <88>, <89>;
+				clocks = <&coreclk 0>;
 			};
 		};
 	};
--- a/arch/arm/boot/dts/armada-xp-mv78260.dtsi
+++ b/arch/arm/boot/dts/armada-xp-mv78260.dtsi
@@ -253,24 +253,28 @@
 		internal-regs {
 			gpio0: gpio@18100 {
 				compatible = "marvell,orion-gpio";
-				reg = <0x18100 0x40>;
+				reg = <0x18100 0x40>, <0x181c0 0x08>;
+				reg-names = "gpio", "pwm";
 				ngpios = <32>;
 				gpio-controller;
 				#gpio-cells = <2>;
+				#pwm-cells = <2>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
 				interrupts = <82>, <83>, <84>, <85>;
+				clocks = <&coreclk 0>;
 			};
 
 			gpio1: gpio@18140 {
 				compatible = "marvell,orion-gpio";
-				reg = <0x18140 0x40>;
+				reg = <0x18140 0x40>, <0x181c8 0x08>;
 				ngpios = <32>;
 				gpio-controller;
 				#gpio-cells = <2>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
 				interrupts = <87>, <88>, <89>, <90>;
+				clocks = <&coreclk 0>;
 			};
 
 			gpio2: gpio@18180 {
--- a/arch/arm/boot/dts/armada-xp-mv78460.dtsi
+++ b/arch/arm/boot/dts/armada-xp-mv78460.dtsi
@@ -291,24 +291,30 @@
 		internal-regs {
 			gpio0: gpio@18100 {
 				compatible = "marvell,orion-gpio";
-				reg = <0x18100 0x40>;
+				reg = <0x18100 0x40>, <0x181c0 0x08>;
+				reg-names = "gpio", "pwm";
 				ngpios = <32>;
 				gpio-controller;
 				#gpio-cells = <2>;
+				#pwm-cells = <2>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
 				interrupts = <82>, <83>, <84>, <85>;
+				clocks = <&coreclk 0>;
 			};
 
 			gpio1: gpio@18140 {
 				compatible = "marvell,orion-gpio";
-				reg = <0x18140 0x40>;
+				reg = <0x18140 0x40>, <0x181c8 0x08>;
+				reg-names = "gpio", "pwm";
 				ngpios = <32>;
 				gpio-controller;
 				#gpio-cells = <2>;
+				#pwm-cells = <2>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
 				interrupts = <87>, <88>, <89>, <90>;
+				clocks = <&coreclk 0>;
 			};
 
 			gpio2: gpio@18180 {
