From eeacc2529942051504bc957726aa178671344421 Mon Sep 17 00:00:00 2001
From: Maxime Bizon <mbizon@freebox.fr>
Date: Wed, 20 Jan 2010 16:21:30 +0100
Subject: [PATCH 32/63] bcm63xx: add support for 96368MVWG board.

---
 arch/mips/bcm63xx/boards/board_bcm963xx.c          |   95 ++++++++++++++++++++
 .../mips/include/asm/mach-bcm63xx/board_bcm963xx.h |    2 +
 2 files changed, 97 insertions(+), 0 deletions(-)

--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -1920,6 +1920,85 @@ static struct board_info __initdata boar
 #endif /* CONFIG_BCM63XX_CPU_6358 */
 
 /*
+ * known 6368 boards
+ */
+#ifdef CONFIG_BCM63XX_CPU_6368
+static struct board_info __initdata board_96368mvwg = {
+	.name				= "96368MVWG",
+	.expected_cpu_id		= 0x6368,
+
+	.has_uart0			= 1,
+	.has_pci			= 1,
+
+	.has_usbd			= 1,
+
+	.usbd = {
+		.use_fullspeed		= 0,
+		.port_no		= 0,
+	},
+
+	.has_enetsw			= 1,
+
+	.enetsw = {
+		.used_ports = {
+			[1] = {
+				.used	= 1,
+				.phy_id	= 2,
+				.name	= "port1",
+			},
+
+			[2] = {
+				.used	= 1,
+				.phy_id	= 3,
+				.name	= "port2",
+			},
+
+			[4] = {
+				.used	= 1,
+				.phy_id	= 0x12,
+				.name	= "port0",
+			},
+
+			[5] = {
+				.used	= 1,
+				.phy_id	= 0x11,
+				.name	= "port3",
+			},
+		},
+	},
+
+	.leds = {
+		{
+			.name		= "96368MVWG:green:adsl",
+			.gpio		= 2,
+			.active_low	= 1,
+		},
+		{
+			.name		= "96368MVWG:green:ppp",
+			.gpio		= 5,
+		},
+		{
+			.name		= "96368MVWG:green:power",
+			.gpio		= 22,
+			.default_trigger = "default-on",
+		},
+		{
+			.name		= "96368MVWG:green:wps",
+			.gpio		= 23,
+			.active_low	= 1,
+		},
+		{
+			.name		= "96368MVWG:red:ppp-fail",
+			.gpio		= 31,
+		},
+	},
+
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+};
+#endif /* CONFIG_BCM63XX_CPU_6368 */
+
+/*
  * all boards
  */
 static const struct board_info __initconst *bcm963xx_boards[] = {
@@ -1971,6 +2050,10 @@ static const struct board_info __initcon
 	&board_HW553,
 	&board_spw303v,
 #endif
+
+#ifdef CONFIG_BCM63XX_CPU_6368
+	&board_96368mvwg,
+#endif
 };
 
 static struct of_device_id const bcm963xx_boards_dt[] = {
@@ -2025,6 +2108,7 @@ static struct of_device_id const bcm963x
 	{ .compatible = "telsey,cpva642", .data = &board_CPVA642, },
 #endif
 #ifdef CONFIG_BCM63XX_CPU_6368
+	{ .compatible = "brcm,bcm96368mvwg", .data = &board_96368mvwg, },
 #endif
 #ifdef CONFIG_BCM63XX_CPU_63268
 	{ .compatible = "brcm,bcm963268bu_p300", .data = &board_963268bu_p300, },
--- a/arch/mips/bcm63xx/boards/board_common.c
+++ b/arch/mips/bcm63xx/boards/board_common.c
@@ -88,12 +88,25 @@ void __init board_early_setup(const stru
 		bcm63xx_pci_enabled = 1;
 		if (BCMCPU_IS_6348())
 			val |= GPIO_MODE_6348_G2_PCI;
+
+		if (BCMCPU_IS_6368())
+			val |= GPIO_MODE_6368_PCI_REQ1 |
+				GPIO_MODE_6368_PCI_GNT1 |
+				GPIO_MODE_6368_PCI_INTB |
+				GPIO_MODE_6368_PCI_REQ0 |
+				GPIO_MODE_6368_PCI_GNT0;
 	}
 #endif
 
 	if (board.has_pccard) {
 		if (BCMCPU_IS_6348())
 			val |= GPIO_MODE_6348_G1_MII_PCCARD;
+
+		if (BCMCPU_IS_6368())
+			val |= GPIO_MODE_6368_PCMCIA_CD1 |
+				GPIO_MODE_6368_PCMCIA_CD2 |
+				GPIO_MODE_6368_PCMCIA_VS1 |
+				GPIO_MODE_6368_PCMCIA_VS2;
 	}
 
 	if (board.has_enet0 && !board.enet0.use_internal_phy) {
