From 3cdba35369b404875849008ea97cf1705e6060ed Mon Sep 17 00:00:00 2001
From: Kumar Gala <galak@codeaurora.org>
Date: Thu, 23 Jan 2014 14:09:54 -0600
Subject: [PATCH 001/182] ARM: dts: msm: split out msm8660 and msm8960 soc
 into dts include

Pull the SoC device tree bits into their own files so other boards based
on these SoCs can include them and reduce duplication across a number of
boards.

Signed-off-by: Kumar Gala <galak@codeaurora.org>
---
 arch/arm/boot/dts/qcom-msm8660-surf.dts |   59 +-------------------------
 arch/arm/boot/dts/qcom-msm8660.dtsi     |   63 ++++++++++++++++++++++++++++
 arch/arm/boot/dts/qcom-msm8960-cdp.dts  |   66 +----------------------------
 arch/arm/boot/dts/qcom-msm8960.dtsi     |   70 +++++++++++++++++++++++++++++++
 4 files changed, 135 insertions(+), 123 deletions(-)
 create mode 100644 arch/arm/boot/dts/qcom-msm8660.dtsi
 create mode 100644 arch/arm/boot/dts/qcom-msm8960.dtsi

--- a/arch/arm/boot/dts/qcom-msm8660-surf.dts
+++ b/arch/arm/boot/dts/qcom-msm8660-surf.dts
@@ -1,63 +1,6 @@
-/dts-v1/;
-
-/include/ "skeleton.dtsi"
-
-#include <dt-bindings/clock/qcom,gcc-msm8660.h>
+#include "qcom-msm8660.dtsi"
 
 / {
 	model = "Qualcomm MSM8660 SURF";
 	compatible = "qcom,msm8660-surf", "qcom,msm8660";
-	interrupt-parent = <&intc>;
-
-	intc: interrupt-controller@2080000 {
-		compatible = "qcom,msm-8660-qgic";
-		interrupt-controller;
-		#interrupt-cells = <3>;
-		reg = < 0x02080000 0x1000 >,
-		      < 0x02081000 0x1000 >;
-	};
-
-	timer@2000000 {
-		compatible = "qcom,scss-timer", "qcom,msm-timer";
-		interrupts = <1 0 0x301>,
-			     <1 1 0x301>,
-			     <1 2 0x301>;
-		reg = <0x02000000 0x100>;
-		clock-frequency = <27000000>,
-				  <32768>;
-		cpu-offset = <0x40000>;
-	};
-
-	msmgpio: gpio@800000 {
-		compatible = "qcom,msm-gpio";
-		reg = <0x00800000 0x4000>;
-		gpio-controller;
-		#gpio-cells = <2>;
-		ngpio = <173>;
-		interrupts = <0 16 0x4>;
-		interrupt-controller;
-		#interrupt-cells = <2>;
-	};
-
-	gcc: clock-controller@900000 {
-		compatible = "qcom,gcc-msm8660";
-		#clock-cells = <1>;
-		#reset-cells = <1>;
-		reg = <0x900000 0x4000>;
-	};
-
-	serial@19c40000 {
-		compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
-		reg = <0x19c40000 0x1000>,
-		      <0x19c00000 0x1000>;
-		interrupts = <0 195 0x0>;
-		clocks = <&gcc GSBI12_UART_CLK>, <&gcc GSBI12_H_CLK>;
-		clock-names = "core", "iface";
-	};
-
-	qcom,ssbi@500000 {
-		compatible = "qcom,ssbi";
-		reg = <0x500000 0x1000>;
-		qcom,controller-type = "pmic-arbiter";
-	};
 };
--- /dev/null
+++ b/arch/arm/boot/dts/qcom-msm8660.dtsi
@@ -0,0 +1,63 @@
+/dts-v1/;
+
+/include/ "skeleton.dtsi"
+
+#include <dt-bindings/clock/qcom,gcc-msm8660.h>
+
+/ {
+	model = "Qualcomm MSM8660";
+	compatible = "qcom,msm8660";
+	interrupt-parent = <&intc>;
+
+	intc: interrupt-controller@2080000 {
+		compatible = "qcom,msm-8660-qgic";
+		interrupt-controller;
+		#interrupt-cells = <3>;
+		reg = < 0x02080000 0x1000 >,
+		      < 0x02081000 0x1000 >;
+	};
+
+	timer@2000000 {
+		compatible = "qcom,scss-timer", "qcom,msm-timer";
+		interrupts = <1 0 0x301>,
+			     <1 1 0x301>,
+			     <1 2 0x301>;
+		reg = <0x02000000 0x100>;
+		clock-frequency = <27000000>,
+				  <32768>;
+		cpu-offset = <0x40000>;
+	};
+
+	msmgpio: gpio@800000 {
+		compatible = "qcom,msm-gpio";
+		reg = <0x00800000 0x4000>;
+		gpio-controller;
+		#gpio-cells = <2>;
+		ngpio = <173>;
+		interrupts = <0 16 0x4>;
+		interrupt-controller;
+		#interrupt-cells = <2>;
+	};
+
+	gcc: clock-controller@900000 {
+		compatible = "qcom,gcc-msm8660";
+		#clock-cells = <1>;
+		#reset-cells = <1>;
+		reg = <0x900000 0x4000>;
+	};
+
+	serial@19c40000 {
+		compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
+		reg = <0x19c40000 0x1000>,
+		      <0x19c00000 0x1000>;
+		interrupts = <0 195 0x0>;
+		clocks = <&gcc GSBI12_UART_CLK>, <&gcc GSBI12_H_CLK>;
+		clock-names = "core", "iface";
+	};
+
+	qcom,ssbi@500000 {
+		compatible = "qcom,ssbi";
+		reg = <0x500000 0x1000>;
+		qcom,controller-type = "pmic-arbiter";
+	};
+};
--- a/arch/arm/boot/dts/qcom-msm8960-cdp.dts
+++ b/arch/arm/boot/dts/qcom-msm8960-cdp.dts
@@ -1,70 +1,6 @@
-/dts-v1/;
-
-/include/ "skeleton.dtsi"
-
-#include <dt-bindings/clock/qcom,gcc-msm8960.h>
+#include "qcom-msm8960.dtsi"
 
 / {
 	model = "Qualcomm MSM8960 CDP";
 	compatible = "qcom,msm8960-cdp", "qcom,msm8960";
-	interrupt-parent = <&intc>;
-
-	intc: interrupt-controller@2000000 {
-		compatible = "qcom,msm-qgic2";
-		interrupt-controller;
-		#interrupt-cells = <3>;
-		reg = < 0x02000000 0x1000 >,
-		      < 0x02002000 0x1000 >;
-	};
-
-	timer@200a000 {
-		compatible = "qcom,kpss-timer", "qcom,msm-timer";
-		interrupts = <1 1 0x301>,
-			     <1 2 0x301>,
-			     <1 3 0x301>;
-		reg = <0x0200a000 0x100>;
-		clock-frequency = <27000000>,
-				  <32768>;
-		cpu-offset = <0x80000>;
-	};
-
-	msmgpio: gpio@800000 {
-		compatible = "qcom,msm-gpio";
-		gpio-controller;
-		#gpio-cells = <2>;
-		ngpio = <150>;
-		interrupts = <0 16 0x4>;
-		interrupt-controller;
-		#interrupt-cells = <2>;
-		reg = <0x800000 0x4000>;
-	};
-
-	gcc: clock-controller@900000 {
-		compatible = "qcom,gcc-msm8960";
-		#clock-cells = <1>;
-		#reset-cells = <1>;
-		reg = <0x900000 0x4000>;
-	};
-
-	clock-controller@4000000 {
-		compatible = "qcom,mmcc-msm8960";
-		reg = <0x4000000 0x1000>;
-		#clock-cells = <1>;
-		#reset-cells = <1>;
-	};
-
-	serial@16440000 {
-		compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
-		reg = <0x16440000 0x1000>,
-		      <0x16400000 0x1000>;
-		interrupts = <0 154 0x0>;
-		clocks = <&gcc GSBI5_UART_CLK>, <&gcc GSBI5_H_CLK>;
-		clock-names = "core", "iface";
-	};
-
-	qcom,ssbi@500000 {
-		compatible = "qcom,ssbi";
-		reg = <0x500000 0x1000>;
-		qcom,controller-type = "pmic-arbiter";
-	};
 };
--- /dev/null
+++ b/arch/arm/boot/dts/qcom-msm8960.dtsi
@@ -0,0 +1,70 @@
+/dts-v1/;
+
+/include/ "skeleton.dtsi"
+
+#include <dt-bindings/clock/qcom,gcc-msm8960.h>
+
+/ {
+	model = "Qualcomm MSM8960";
+	compatible = "qcom,msm8960";
+	interrupt-parent = <&intc>;
+
+	intc: interrupt-controller@2000000 {
+		compatible = "qcom,msm-qgic2";
+		interrupt-controller;
+		#interrupt-cells = <3>;
+		reg = < 0x02000000 0x1000 >,
+		      < 0x02002000 0x1000 >;
+	};
+
+	timer@200a000 {
+		compatible = "qcom,kpss-timer", "qcom,msm-timer";
+		interrupts = <1 1 0x301>,
+			     <1 2 0x301>,
+			     <1 3 0x301>;
+		reg = <0x0200a000 0x100>;
+		clock-frequency = <27000000>,
+				  <32768>;
+		cpu-offset = <0x80000>;
+	};
+
+	msmgpio: gpio@800000 {
+		compatible = "qcom,msm-gpio";
+		gpio-controller;
+		#gpio-cells = <2>;
+		ngpio = <150>;
+		interrupts = <0 16 0x4>;
+		interrupt-controller;
+		#interrupt-cells = <2>;
+		reg = <0x800000 0x4000>;
+	};
+
+	gcc: clock-controller@900000 {
+		compatible = "qcom,gcc-msm8960";
+		#clock-cells = <1>;
+		#reset-cells = <1>;
+		reg = <0x900000 0x4000>;
+	};
+
+	clock-controller@4000000 {
+		compatible = "qcom,mmcc-msm8960";
+		reg = <0x4000000 0x1000>;
+		#clock-cells = <1>;
+		#reset-cells = <1>;
+	};
+
+	serial@16440000 {
+		compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
+		reg = <0x16440000 0x1000>,
+		      <0x16400000 0x1000>;
+		interrupts = <0 154 0x0>;
+		clocks = <&gcc GSBI5_UART_CLK>, <&gcc GSBI5_H_CLK>;
+		clock-names = "core", "iface";
+	};
+
+	qcom,ssbi@500000 {
+		compatible = "qcom,ssbi";
+		reg = <0x500000 0x1000>;
+		qcom,controller-type = "pmic-arbiter";
+	};
+};
