#!/bin/sh
#
# Copyright (C) 2013 OpenWrt.org
#

[ -e /etc/config/network ] && exit 0

touch /etc/config/network

. /lib/functions/uci-defaults.sh
. /lib/imx6.sh

board=$(imx6_board_name)

ucidef_set_interface_loopback

case "$board" in
"gw51xx" |\
"gw52xx")
	ucidef_set_interface_lan 'eth0'
	;;
"gw53xx" |\
"gw54xx" |\
"gw552x")
	ucidef_set_interfaces_lan_wan 'eth0' 'eth1'
	;;
"wandboard")
	ucidef_set_interface_wan 'eth0'
	;;
esac

uci commit network

exit 0
