From 7720fe5faadae243806833c7a7ec5d15bae244c4 Mon Sep 17 00:00:00 2001
From: Alexander Bersenev <bay@hackerdom.ru>
Date: Mon, 9 Jun 2014 00:08:11 +0600
Subject: [PATCH] ARM: sunxi: Add pins for IR controller on A20 to dtsi

This patch adds pins for two IR controllers on A20

Signed-off-by: Alexander Bersenev <bay@hackerdom.ru>
Signed-off-by: Alexsey Shestacov <wingrime@linux-sunxi.org>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 14 ++++++++++++++
 1 file changed, 14 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -746,6 +746,20 @@
 				allwinner,drive = <2>;
 				allwinner,pull = <0>;
 			};
+
+			ir0_pins_a: ir0@0 {
+				    allwinner,pins = "PB3","PB4";
+				    allwinner,function = "ir0";
+				    allwinner,drive = <0>;
+				    allwinner,pull = <0>;
+			};
+
+			ir1_pins_a: ir1@0 {
+				    allwinner,pins = "PB22","PB23";
+				    allwinner,function = "ir1";
+				    allwinner,drive = <0>;
+				    allwinner,pull = <0>;
+			};
 		};
 
 		timer@01c20c00 {
