From 151c4e4a06b0b8d16c2fd392bb0e33868b12357f Mon Sep 17 00:00:00 2001
From: Felix Fietkau <nbd@openwrt.org>
Date: Mon, 12 Aug 2013 12:45:52 +0200
Subject: [PATCH] MIPS: remove unnecessary platform dma helper functions

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
---
 arch/mips/include/asm/mach-cavium-octeon/dma-coherence.h | 12 ------------
 arch/mips/include/asm/mach-generic/dma-coherence.h       | 10 ----------
 arch/mips/include/asm/mach-ip27/dma-coherence.h          | 10 ----------
 arch/mips/include/asm/mach-ip32/dma-coherence.h          | 11 -----------
 arch/mips/include/asm/mach-jazz/dma-coherence.h          | 10 ----------
 arch/mips/include/asm/mach-loongson/dma-coherence.h      | 10 ----------
 arch/mips/include/asm/mach-powertv/dma-coherence.h       | 10 ----------
 arch/mips/mm/dma-default.c                               |  4 +---
 8 files changed, 1 insertion(+), 76 deletions(-)

--- a/arch/mips/include/asm/mach-cavium-octeon/dma-coherence.h
+++ b/arch/mips/include/asm/mach-cavium-octeon/dma-coherence.h
@@ -46,22 +46,11 @@ static inline int plat_dma_supported(str
 	BUG();
 }
 
-static inline void plat_extra_sync_for_device(struct device *dev)
-{
-	BUG();
-}
-
 static inline int plat_device_is_coherent(struct device *dev)
 {
 	return 1;
 }
 
-static inline int plat_dma_mapping_error(struct device *dev,
-					 dma_addr_t dma_addr)
-{
-	BUG();
-}
-
 dma_addr_t phys_to_dma(struct device *dev, phys_addr_t paddr);
 phys_addr_t dma_to_phys(struct device *dev, dma_addr_t daddr);
 
--- a/arch/mips/include/asm/mach-generic/dma-coherence.h
+++ b/arch/mips/include/asm/mach-generic/dma-coherence.h
@@ -47,16 +47,6 @@ static inline int plat_dma_supported(str
 	return 1;
 }
 
-static inline void plat_extra_sync_for_device(struct device *dev)
-{
-}
-
-static inline int plat_dma_mapping_error(struct device *dev,
-					 dma_addr_t dma_addr)
-{
-	return 0;
-}
-
 static inline int plat_device_is_coherent(struct device *dev)
 {
 #ifdef CONFIG_DMA_COHERENT
--- a/arch/mips/include/asm/mach-ip27/dma-coherence.h
+++ b/arch/mips/include/asm/mach-ip27/dma-coherence.h
@@ -58,16 +58,6 @@ static inline int plat_dma_supported(str
 	return 1;
 }
 
-static inline void plat_extra_sync_for_device(struct device *dev)
-{
-}
-
-static inline int plat_dma_mapping_error(struct device *dev,
-					 dma_addr_t dma_addr)
-{
-	return 0;
-}
-
 static inline int plat_device_is_coherent(struct device *dev)
 {
 	return 1;		/* IP27 non-cohernet mode is unsupported */
--- a/arch/mips/include/asm/mach-ip32/dma-coherence.h
+++ b/arch/mips/include/asm/mach-ip32/dma-coherence.h
@@ -80,17 +80,6 @@ static inline int plat_dma_supported(str
 	return 1;
 }
 
-static inline void plat_extra_sync_for_device(struct device *dev)
-{
-	return;
-}
-
-static inline int plat_dma_mapping_error(struct device *dev,
-					 dma_addr_t dma_addr)
-{
-	return 0;
-}
-
 static inline int plat_device_is_coherent(struct device *dev)
 {
 	return 0;		/* IP32 is non-cohernet */
--- a/arch/mips/include/asm/mach-jazz/dma-coherence.h
+++ b/arch/mips/include/asm/mach-jazz/dma-coherence.h
@@ -48,16 +48,6 @@ static inline int plat_dma_supported(str
 	return 1;
 }
 
-static inline void plat_extra_sync_for_device(struct device *dev)
-{
-}
-
-static inline int plat_dma_mapping_error(struct device *dev,
-					 dma_addr_t dma_addr)
-{
-	return 0;
-}
-
 static inline int plat_device_is_coherent(struct device *dev)
 {
 	return 0;
--- a/arch/mips/include/asm/mach-loongson/dma-coherence.h
+++ b/arch/mips/include/asm/mach-loongson/dma-coherence.h
@@ -53,16 +53,6 @@ static inline int plat_dma_supported(str
 	return 1;
 }
 
-static inline void plat_extra_sync_for_device(struct device *dev)
-{
-}
-
-static inline int plat_dma_mapping_error(struct device *dev,
-					 dma_addr_t dma_addr)
-{
-	return 0;
-}
-
 static inline int plat_device_is_coherent(struct device *dev)
 {
 	return 0;
--- a/arch/mips/include/asm/mach-powertv/dma-coherence.h
+++ b/arch/mips/include/asm/mach-powertv/dma-coherence.h
@@ -99,16 +99,6 @@ static inline int plat_dma_supported(str
 	return 1;
 }
 
-static inline void plat_extra_sync_for_device(struct device *dev)
-{
-}
-
-static inline int plat_dma_mapping_error(struct device *dev,
-					 dma_addr_t dma_addr)
-{
-	return 0;
-}
-
 static inline int plat_device_is_coherent(struct device *dev)
 {
 	return 0;
--- a/arch/mips/mm/dma-default.c
+++ b/arch/mips/mm/dma-default.c
@@ -293,7 +293,6 @@ static void mips_dma_sync_single_for_cpu
 static void mips_dma_sync_single_for_device(struct device *dev,
 	dma_addr_t dma_handle, size_t size, enum dma_data_direction direction)
 {
-	plat_extra_sync_for_device(dev);
 	if (!plat_device_is_coherent(dev))
 		__dma_sync(dma_addr_to_page(dev, dma_handle),
 			   dma_handle & ~PAGE_MASK, size, direction);
@@ -327,7 +326,7 @@ static void mips_dma_sync_sg_for_device(
 
 int mips_dma_mapping_error(struct device *dev, dma_addr_t dma_addr)
 {
-	return plat_dma_mapping_error(dev, dma_addr);
+	return 0;
 }
 
 int mips_dma_supported(struct device *dev, u64 mask)
@@ -340,7 +339,6 @@ void dma_cache_sync(struct device *dev, 
 {
 	BUG_ON(direction == DMA_NONE);
 
-	plat_extra_sync_for_device(dev);
 	if (!plat_device_is_coherent(dev))
 		__dma_sync_virtual(vaddr, size, direction);
 }
