From f722ea226581a75107ef16b46db1b7b5b999c93a Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Sun, 2 Feb 2014 14:55:25 +0100
Subject: [PATCH] ARM: sunxi: dt: Update the watchdog compatibles

The watchdog compatibles were following a different pattern than the one found
in the other devices. Now that the driver supports the right pattern, switch to
it in the DT.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun4i-a10.dtsi  | 2 +-
 arch/arm/boot/dts/sun5i-a10s.dtsi | 2 +-
 arch/arm/boot/dts/sun5i-a13.dtsi  | 2 +-
 arch/arm/boot/dts/sun6i-a31.dtsi  | 2 +-
 arch/arm/boot/dts/sun7i-a20.dtsi  | 2 +-
 5 files changed, 5 insertions(+), 5 deletions(-)

--- a/arch/arm/boot/dts/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/sun4i-a10.dtsi
@@ -487,7 +487,7 @@
 		};
 
 		wdt: watchdog@01c20c90 {
-			compatible = "allwinner,sun4i-wdt";
+			compatible = "allwinner,sun4i-a10-wdt";
 			reg = <0x01c20c90 0x10>;
 		};
 
--- a/arch/arm/boot/dts/sun5i-a10s.dtsi
+++ b/arch/arm/boot/dts/sun5i-a10s.dtsi
@@ -392,7 +392,7 @@
 		};
 
 		wdt: watchdog@01c20c90 {
-			compatible = "allwinner,sun4i-wdt";
+			compatible = "allwinner,sun4i-a10-wdt";
 			reg = <0x01c20c90 0x10>;
 		};
 
--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -393,7 +393,7 @@
 		};
 
 		wdt: watchdog@01c20c90 {
-			compatible = "allwinner,sun4i-wdt";
+			compatible = "allwinner,sun4i-a10-wdt";
 			reg = <0x01c20c90 0x10>;
 		};
 
--- a/arch/arm/boot/dts/sun6i-a31.dtsi
+++ b/arch/arm/boot/dts/sun6i-a31.dtsi
@@ -289,7 +289,7 @@
 		};
 
 		wdt1: watchdog@01c20ca0 {
-			compatible = "allwinner,sun6i-wdt";
+			compatible = "allwinner,sun6i-a31-wdt";
 			reg = <0x01c20ca0 0x20>;
 		};
 
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -608,7 +608,7 @@
 		};
 
 		wdt: watchdog@01c20c90 {
-			compatible = "allwinner,sun4i-wdt";
+			compatible = "allwinner,sun4i-a10-wdt";
 			reg = <0x01c20c90 0x10>;
 		};
 
