From 0b24e0e6bf2d9a1ca5f95446bc025dafc226998c Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Fri, 15 Mar 2013 18:16:01 +0100
Subject: [PATCH 27/57] serial: ralink: adds mt7620 serial

Add the config symbol for Mediatek7620 SoC to SERIAL_8250_RT288X

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/tty/serial/8250/Kconfig |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/tty/serial/8250/Kconfig
+++ b/drivers/tty/serial/8250/Kconfig
@@ -301,7 +301,7 @@ config SERIAL_8250_EM
 
 config SERIAL_8250_RT288X
 	bool "Ralink RT288x/RT305x/RT3662/RT3883 serial port support"
-	depends on SERIAL_8250 && (SOC_RT288X || SOC_RT305X || SOC_RT3883)
+	depends on SERIAL_8250 && (SOC_RT288X || SOC_RT305X || SOC_RT3883 || SOC_MT7620)
 	help
 	  If you have a Ralink RT288x/RT305x SoC based board and want to use the
 	  serial port, say Y to this option. The driver can handle up to 2 serial
