--- a/drivers/ssb/Kconfig
+++ b/drivers/ssb/Kconfig
@@ -138,13 +138,13 @@ config SSB_DRIVER_MIPS
 
 config SSB_SFLASH
 	bool "SSB serial flash support"
-	depends on SSB_DRIVER_MIPS && BROKEN
+	depends on SSB_DRIVER_MIPS
 	default y
 
 # Assumption: We are on embedded, if we compile the MIPS core.
 config SSB_EMBEDDED
 	bool
-	depends on SSB_DRIVER_MIPS
+	depends on SSB_DRIVER_MIPS && SSB_PCICORE_HOSTMODE
 	default y
 
 config SSB_DRIVER_EXTIF
@@ -168,6 +168,7 @@ config SSB_DRIVER_GIGE
 config SSB_DRIVER_GPIO
 	bool "SSB GPIO driver"
 	depends on SSB && GPIOLIB
+	select IRQ_DOMAIN if SSB_EMBEDDED
 	help
 	  Driver to provide access to the GPIO pins on the bus.
 
--- a/drivers/ssb/b43_pci_bridge.c
+++ b/drivers/ssb/b43_pci_bridge.c
@@ -38,6 +38,7 @@ static const struct pci_device_id b43_pc
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x432b) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x432c) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4350) },
+	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4351) },
 	{ 0, },
 };
 MODULE_DEVICE_TABLE(pci, b43_pci_bridge_tbl);
--- a/drivers/ssb/driver_chipcommon_sflash.c
+++ b/drivers/ssb/driver_chipcommon_sflash.c
@@ -9,6 +9,19 @@
 
 #include "ssb_private.h"
 
+static struct resource ssb_sflash_resource = {
+	.name	= "ssb_sflash",
+	.start	= SSB_FLASH2,
+	.end	= 0,
+	.flags  = IORESOURCE_MEM | IORESOURCE_READONLY,
+};
+
+struct platform_device ssb_sflash_dev = {
+	.name		= "ssb_sflash",
+	.resource	= &ssb_sflash_resource,
+	.num_resources	= 1,
+};
+
 struct ssb_sflash_tbl_e {
 	char *name;
 	u32 id;
@@ -16,7 +29,7 @@ struct ssb_sflash_tbl_e {
 	u16 numblocks;
 };
 
-static struct ssb_sflash_tbl_e ssb_sflash_st_tbl[] = {
+static const struct ssb_sflash_tbl_e ssb_sflash_st_tbl[] = {
 	{ "M25P20", 0x11, 0x10000, 4, },
 	{ "M25P40", 0x12, 0x10000, 8, },
 
@@ -24,10 +37,10 @@ static struct ssb_sflash_tbl_e ssb_sflas
 	{ "M25P32", 0x15, 0x10000, 64, },
 	{ "M25P64", 0x16, 0x10000, 128, },
 	{ "M25FL128", 0x17, 0x10000, 256, },
-	{ 0 },
+	{ NULL },
 };
 
-static struct ssb_sflash_tbl_e ssb_sflash_sst_tbl[] = {
+static const struct ssb_sflash_tbl_e ssb_sflash_sst_tbl[] = {
 	{ "SST25WF512", 1, 0x1000, 16, },
 	{ "SST25VF512", 0x48, 0x1000, 16, },
 	{ "SST25WF010", 2, 0x1000, 32, },
@@ -42,10 +55,10 @@ static struct ssb_sflash_tbl_e ssb_sflas
 	{ "SST25VF016", 0x41, 0x1000, 512, },
 	{ "SST25VF032", 0x4a, 0x1000, 1024, },
 	{ "SST25VF064", 0x4b, 0x1000, 2048, },
-	{ 0 },
+	{ NULL },
 };
 
-static struct ssb_sflash_tbl_e ssb_sflash_at_tbl[] = {
+static const struct ssb_sflash_tbl_e ssb_sflash_at_tbl[] = {
 	{ "AT45DB011", 0xc, 256, 512, },
 	{ "AT45DB021", 0x14, 256, 1024, },
 	{ "AT45DB041", 0x1c, 256, 2048, },
@@ -53,7 +66,7 @@ static struct ssb_sflash_tbl_e ssb_sflas
 	{ "AT45DB161", 0x2c, 512, 4096, },
 	{ "AT45DB321", 0x34, 512, 8192, },
 	{ "AT45DB642", 0x3c, 1024, 8192, },
-	{ 0 },
+	{ NULL },
 };
 
 static void ssb_sflash_cmd(struct ssb_chipcommon *cc, u32 opcode)
@@ -73,7 +86,8 @@ static void ssb_sflash_cmd(struct ssb_ch
 /* Initialize serial flash access */
 int ssb_sflash_init(struct ssb_chipcommon *cc)
 {
-	struct ssb_sflash_tbl_e *e;
+	struct ssb_sflash *sflash = &cc->dev->bus->mipscore.sflash;
+	const struct ssb_sflash_tbl_e *e;
 	u32 id, id2;
 
 	switch (cc->capabilities & SSB_CHIPCO_CAP_FLASHT) {
@@ -131,10 +145,20 @@ int ssb_sflash_init(struct ssb_chipcommo
 		return -ENOTSUPP;
 	}
 
-	pr_info("Found %s serial flash (blocksize: 0x%X, blocks: %d)\n",
-		e->name, e->blocksize, e->numblocks);
-
-	pr_err("Serial flash support is not implemented yet!\n");
+	sflash->window = SSB_FLASH2;
+	sflash->blocksize = e->blocksize;
+	sflash->numblocks = e->numblocks;
+	sflash->size = sflash->blocksize * sflash->numblocks;
+	sflash->present = true;
+
+	pr_info("Found %s serial flash (size: %dKiB, blocksize: 0x%X, blocks: %d)\n",
+		e->name, sflash->size / 1024, e->blocksize, e->numblocks);
+
+	/* Prepare platform device, but don't register it yet. It's too early,
+	 * malloc (required by device_private_init) is not available yet. */
+	ssb_sflash_dev.resource[0].end = ssb_sflash_dev.resource[0].start +
+					 sflash->size;
+	ssb_sflash_dev.dev.platform_data = sflash;
 
-	return -ENOTSUPP;
+	return 0;
 }
--- a/drivers/ssb/driver_gpio.c
+++ b/drivers/ssb/driver_gpio.c
@@ -9,16 +9,40 @@
  */
 
 #include <linux/gpio.h>
+#include <linux/irq.h>
+#include <linux/interrupt.h>
+#include <linux/irqdomain.h>
 #include <linux/export.h>
 #include <linux/ssb/ssb.h>
 
 #include "ssb_private.h"
 
+
+/**************************************************
+ * Shared
+ **************************************************/
+
 static struct ssb_bus *ssb_gpio_get_bus(struct gpio_chip *chip)
 {
 	return container_of(chip, struct ssb_bus, gpio);
 }
 
+#if IS_ENABLED(CONFIG_SSB_EMBEDDED)
+static int ssb_gpio_to_irq(struct gpio_chip *chip, unsigned gpio)
+{
+	struct ssb_bus *bus = ssb_gpio_get_bus(chip);
+
+	if (bus->bustype == SSB_BUSTYPE_SSB)
+		return irq_find_mapping(bus->irq_domain, gpio);
+	else
+		return -EINVAL;
+}
+#endif
+
+/**************************************************
+ * ChipCommon
+ **************************************************/
+
 static int ssb_gpio_chipco_get_value(struct gpio_chip *chip, unsigned gpio)
 {
 	struct ssb_bus *bus = ssb_gpio_get_bus(chip);
@@ -74,19 +98,129 @@ static void ssb_gpio_chipco_free(struct
 	ssb_chipco_gpio_pullup(&bus->chipco, 1 << gpio, 0);
 }
 
-static int ssb_gpio_chipco_to_irq(struct gpio_chip *chip, unsigned gpio)
+#if IS_ENABLED(CONFIG_SSB_EMBEDDED)
+static void ssb_gpio_irq_chipco_mask(struct irq_data *d)
 {
-	struct ssb_bus *bus = ssb_gpio_get_bus(chip);
+	struct ssb_bus *bus = irq_data_get_irq_chip_data(d);
+	int gpio = irqd_to_hwirq(d);
 
-	if (bus->bustype == SSB_BUSTYPE_SSB)
-		return ssb_mips_irq(bus->chipco.dev) + 2;
-	else
-		return -EINVAL;
+	ssb_chipco_gpio_intmask(&bus->chipco, BIT(gpio), 0);
+}
+
+static void ssb_gpio_irq_chipco_unmask(struct irq_data *d)
+{
+	struct ssb_bus *bus = irq_data_get_irq_chip_data(d);
+	int gpio = irqd_to_hwirq(d);
+	u32 val = ssb_chipco_gpio_in(&bus->chipco, BIT(gpio));
+
+	ssb_chipco_gpio_polarity(&bus->chipco, BIT(gpio), val);
+	ssb_chipco_gpio_intmask(&bus->chipco, BIT(gpio), BIT(gpio));
+}
+
+static struct irq_chip ssb_gpio_irq_chipco_chip = {
+	.name		= "SSB-GPIO-CC",
+	.irq_mask	= ssb_gpio_irq_chipco_mask,
+	.irq_unmask	= ssb_gpio_irq_chipco_unmask,
+};
+
+static irqreturn_t ssb_gpio_irq_chipco_handler(int irq, void *dev_id)
+{
+	struct ssb_bus *bus = dev_id;
+	struct ssb_chipcommon *chipco = &bus->chipco;
+	u32 val = chipco_read32(chipco, SSB_CHIPCO_GPIOIN);
+	u32 mask = chipco_read32(chipco, SSB_CHIPCO_GPIOIRQ);
+	u32 pol = chipco_read32(chipco, SSB_CHIPCO_GPIOPOL);
+	unsigned long irqs = (val ^ pol) & mask;
+	int gpio;
+
+	if (!irqs)
+		return IRQ_NONE;
+
+	for_each_set_bit(gpio, &irqs, bus->gpio.ngpio)
+		generic_handle_irq(ssb_gpio_to_irq(&bus->gpio, gpio));
+	ssb_chipco_gpio_polarity(chipco, irqs, val & irqs);
+
+	return IRQ_HANDLED;
+}
+
+static int ssb_gpio_irq_chipco_domain_init(struct ssb_bus *bus)
+{
+	struct ssb_chipcommon *chipco = &bus->chipco;
+	struct gpio_chip *chip = &bus->gpio;
+	int gpio, hwirq, err;
+
+	if (bus->bustype != SSB_BUSTYPE_SSB)
+		return 0;
+
+	bus->irq_domain = irq_domain_add_linear(NULL, chip->ngpio,
+						&irq_domain_simple_ops, chipco);
+	if (!bus->irq_domain) {
+		err = -ENODEV;
+		goto err_irq_domain;
+	}
+	for (gpio = 0; gpio < chip->ngpio; gpio++) {
+		int irq = irq_create_mapping(bus->irq_domain, gpio);
+
+		irq_set_chip_data(irq, bus);
+		irq_set_chip_and_handler(irq, &ssb_gpio_irq_chipco_chip,
+					 handle_simple_irq);
+	}
+
+	hwirq = ssb_mips_irq(bus->chipco.dev) + 2;
+	err = request_irq(hwirq, ssb_gpio_irq_chipco_handler, IRQF_SHARED,
+			  "gpio", bus);
+	if (err)
+		goto err_req_irq;
+
+	ssb_chipco_gpio_intmask(&bus->chipco, ~0, 0);
+	chipco_set32(chipco, SSB_CHIPCO_IRQMASK, SSB_CHIPCO_IRQ_GPIO);
+
+	return 0;
+
+err_req_irq:
+	for (gpio = 0; gpio < chip->ngpio; gpio++) {
+		int irq = irq_find_mapping(bus->irq_domain, gpio);
+
+		irq_dispose_mapping(irq);
+	}
+	irq_domain_remove(bus->irq_domain);
+err_irq_domain:
+	return err;
+}
+
+static void ssb_gpio_irq_chipco_domain_exit(struct ssb_bus *bus)
+{
+	struct ssb_chipcommon *chipco = &bus->chipco;
+	struct gpio_chip *chip = &bus->gpio;
+	int gpio;
+
+	if (bus->bustype != SSB_BUSTYPE_SSB)
+		return;
+
+	chipco_mask32(chipco, SSB_CHIPCO_IRQMASK, ~SSB_CHIPCO_IRQ_GPIO);
+	free_irq(ssb_mips_irq(bus->chipco.dev) + 2, chipco);
+	for (gpio = 0; gpio < chip->ngpio; gpio++) {
+		int irq = irq_find_mapping(bus->irq_domain, gpio);
+
+		irq_dispose_mapping(irq);
+	}
+	irq_domain_remove(bus->irq_domain);
+}
+#else
+static int ssb_gpio_irq_chipco_domain_init(struct ssb_bus *bus)
+{
+	return 0;
+}
+
+static void ssb_gpio_irq_chipco_domain_exit(struct ssb_bus *bus)
+{
 }
+#endif
 
 static int ssb_gpio_chipco_init(struct ssb_bus *bus)
 {
 	struct gpio_chip *chip = &bus->gpio;
+	int err;
 
 	chip->label		= "ssb_chipco_gpio";
 	chip->owner		= THIS_MODULE;
@@ -96,7 +230,9 @@ static int ssb_gpio_chipco_init(struct s
 	chip->set		= ssb_gpio_chipco_set_value;
 	chip->direction_input	= ssb_gpio_chipco_direction_input;
 	chip->direction_output	= ssb_gpio_chipco_direction_output;
-	chip->to_irq		= ssb_gpio_chipco_to_irq;
+#if IS_ENABLED(CONFIG_SSB_EMBEDDED)
+	chip->to_irq		= ssb_gpio_to_irq;
+#endif
 	chip->ngpio		= 16;
 	/* There is just one SoC in one device and its GPIO addresses should be
 	 * deterministic to address them more easily. The other buses could get
@@ -106,9 +242,23 @@ static int ssb_gpio_chipco_init(struct s
 	else
 		chip->base		= -1;
 
-	return gpiochip_add(chip);
+	err = ssb_gpio_irq_chipco_domain_init(bus);
+	if (err)
+		return err;
+
+	err = gpiochip_add(chip);
+	if (err) {
+		ssb_gpio_irq_chipco_domain_exit(bus);
+		return err;
+	}
+
+	return 0;
 }
 
+/**************************************************
+ * EXTIF
+ **************************************************/
+
 #ifdef CONFIG_SSB_DRIVER_EXTIF
 
 static int ssb_gpio_extif_get_value(struct gpio_chip *chip, unsigned gpio)
@@ -145,19 +295,127 @@ static int ssb_gpio_extif_direction_outp
 	return 0;
 }
 
-static int ssb_gpio_extif_to_irq(struct gpio_chip *chip, unsigned gpio)
+#if IS_ENABLED(CONFIG_SSB_EMBEDDED)
+static void ssb_gpio_irq_extif_mask(struct irq_data *d)
 {
-	struct ssb_bus *bus = ssb_gpio_get_bus(chip);
+	struct ssb_bus *bus = irq_data_get_irq_chip_data(d);
+	int gpio = irqd_to_hwirq(d);
 
-	if (bus->bustype == SSB_BUSTYPE_SSB)
-		return ssb_mips_irq(bus->extif.dev) + 2;
-	else
-		return -EINVAL;
+	ssb_extif_gpio_intmask(&bus->extif, BIT(gpio), 0);
+}
+
+static void ssb_gpio_irq_extif_unmask(struct irq_data *d)
+{
+	struct ssb_bus *bus = irq_data_get_irq_chip_data(d);
+	int gpio = irqd_to_hwirq(d);
+	u32 val = ssb_extif_gpio_in(&bus->extif, BIT(gpio));
+
+	ssb_extif_gpio_polarity(&bus->extif, BIT(gpio), val);
+	ssb_extif_gpio_intmask(&bus->extif, BIT(gpio), BIT(gpio));
+}
+
+static struct irq_chip ssb_gpio_irq_extif_chip = {
+	.name		= "SSB-GPIO-EXTIF",
+	.irq_mask	= ssb_gpio_irq_extif_mask,
+	.irq_unmask	= ssb_gpio_irq_extif_unmask,
+};
+
+static irqreturn_t ssb_gpio_irq_extif_handler(int irq, void *dev_id)
+{
+	struct ssb_bus *bus = dev_id;
+	struct ssb_extif *extif = &bus->extif;
+	u32 val = ssb_read32(extif->dev, SSB_EXTIF_GPIO_IN);
+	u32 mask = ssb_read32(extif->dev, SSB_EXTIF_GPIO_INTMASK);
+	u32 pol = ssb_read32(extif->dev, SSB_EXTIF_GPIO_INTPOL);
+	unsigned long irqs = (val ^ pol) & mask;
+	int gpio;
+
+	if (!irqs)
+		return IRQ_NONE;
+
+	for_each_set_bit(gpio, &irqs, bus->gpio.ngpio)
+		generic_handle_irq(ssb_gpio_to_irq(&bus->gpio, gpio));
+	ssb_extif_gpio_polarity(extif, irqs, val & irqs);
+
+	return IRQ_HANDLED;
+}
+
+static int ssb_gpio_irq_extif_domain_init(struct ssb_bus *bus)
+{
+	struct ssb_extif *extif = &bus->extif;
+	struct gpio_chip *chip = &bus->gpio;
+	int gpio, hwirq, err;
+
+	if (bus->bustype != SSB_BUSTYPE_SSB)
+		return 0;
+
+	bus->irq_domain = irq_domain_add_linear(NULL, chip->ngpio,
+						&irq_domain_simple_ops, extif);
+	if (!bus->irq_domain) {
+		err = -ENODEV;
+		goto err_irq_domain;
+	}
+	for (gpio = 0; gpio < chip->ngpio; gpio++) {
+		int irq = irq_create_mapping(bus->irq_domain, gpio);
+
+		irq_set_chip_data(irq, bus);
+		irq_set_chip_and_handler(irq, &ssb_gpio_irq_extif_chip,
+					 handle_simple_irq);
+	}
+
+	hwirq = ssb_mips_irq(bus->extif.dev) + 2;
+	err = request_irq(hwirq, ssb_gpio_irq_extif_handler, IRQF_SHARED,
+			  "gpio", bus);
+	if (err)
+		goto err_req_irq;
+
+	ssb_extif_gpio_intmask(&bus->extif, ~0, 0);
+
+	return 0;
+
+err_req_irq:
+	for (gpio = 0; gpio < chip->ngpio; gpio++) {
+		int irq = irq_find_mapping(bus->irq_domain, gpio);
+
+		irq_dispose_mapping(irq);
+	}
+	irq_domain_remove(bus->irq_domain);
+err_irq_domain:
+	return err;
 }
 
+static void ssb_gpio_irq_extif_domain_exit(struct ssb_bus *bus)
+{
+	struct ssb_extif *extif = &bus->extif;
+	struct gpio_chip *chip = &bus->gpio;
+	int gpio;
+
+	if (bus->bustype != SSB_BUSTYPE_SSB)
+		return;
+
+	free_irq(ssb_mips_irq(bus->extif.dev) + 2, extif);
+	for (gpio = 0; gpio < chip->ngpio; gpio++) {
+		int irq = irq_find_mapping(bus->irq_domain, gpio);
+
+		irq_dispose_mapping(irq);
+	}
+	irq_domain_remove(bus->irq_domain);
+}
+#else
+static int ssb_gpio_irq_extif_domain_init(struct ssb_bus *bus)
+{
+	return 0;
+}
+
+static void ssb_gpio_irq_extif_domain_exit(struct ssb_bus *bus)
+{
+}
+#endif
+
 static int ssb_gpio_extif_init(struct ssb_bus *bus)
 {
 	struct gpio_chip *chip = &bus->gpio;
+	int err;
 
 	chip->label		= "ssb_extif_gpio";
 	chip->owner		= THIS_MODULE;
@@ -165,7 +423,9 @@ static int ssb_gpio_extif_init(struct ss
 	chip->set		= ssb_gpio_extif_set_value;
 	chip->direction_input	= ssb_gpio_extif_direction_input;
 	chip->direction_output	= ssb_gpio_extif_direction_output;
-	chip->to_irq		= ssb_gpio_extif_to_irq;
+#if IS_ENABLED(CONFIG_SSB_EMBEDDED)
+	chip->to_irq		= ssb_gpio_to_irq;
+#endif
 	chip->ngpio		= 5;
 	/* There is just one SoC in one device and its GPIO addresses should be
 	 * deterministic to address them more easily. The other buses could get
@@ -175,7 +435,17 @@ static int ssb_gpio_extif_init(struct ss
 	else
 		chip->base		= -1;
 
-	return gpiochip_add(chip);
+	err = ssb_gpio_irq_extif_domain_init(bus);
+	if (err)
+		return err;
+
+	err = gpiochip_add(chip);
+	if (err) {
+		ssb_gpio_irq_extif_domain_exit(bus);
+		return err;
+	}
+
+	return 0;
 }
 
 #else
@@ -185,6 +455,10 @@ static int ssb_gpio_extif_init(struct ss
 }
 #endif
 
+/**************************************************
+ * Init
+ **************************************************/
+
 int ssb_gpio_init(struct ssb_bus *bus)
 {
 	if (ssb_chipco_available(&bus->chipco))
@@ -201,7 +475,8 @@ int ssb_gpio_unregister(struct ssb_bus *
 {
 	if (ssb_chipco_available(&bus->chipco) ||
 	    ssb_extif_available(&bus->extif)) {
-		return gpiochip_remove(&bus->gpio);
+		gpiochip_remove(&bus->gpio);
+		return 0;
 	} else {
 		SSB_WARN_ON(1);
 	}
--- a/drivers/ssb/main.c
+++ b/drivers/ssb/main.c
@@ -553,6 +553,14 @@ static int ssb_devices_register(struct s
 	}
 #endif
 
+#ifdef CONFIG_SSB_SFLASH
+	if (bus->mipscore.sflash.present) {
+		err = platform_device_register(&ssb_sflash_dev);
+		if (err)
+			pr_err("Error registering serial flash\n");
+	}
+#endif
+
 	return 0;
 error:
 	/* Unwind the already registered devices. */
@@ -582,6 +590,13 @@ static int ssb_attach_queued_buses(void)
 		ssb_pcicore_init(&bus->pcicore);
 		if (bus->bustype == SSB_BUSTYPE_SSB)
 			ssb_watchdog_register(bus);
+
+		err = ssb_gpio_init(bus);
+		if (err == -ENOTSUPP)
+			ssb_dbg("GPIO driver not activated\n");
+		else if (err)
+			ssb_dbg("Error registering GPIO driver: %i\n", err);
+
 		ssb_bus_may_powerdown(bus);
 
 		err = ssb_devices_register(bus);
@@ -819,11 +834,6 @@ static int ssb_bus_register(struct ssb_b
 	ssb_chipcommon_init(&bus->chipco);
 	ssb_extif_init(&bus->extif);
 	ssb_mipscore_init(&bus->mipscore);
-	err = ssb_gpio_init(bus);
-	if (err == -ENOTSUPP)
-		ssb_dbg("GPIO driver not activated\n");
-	else if (err)
-		ssb_dbg("Error registering GPIO driver: %i\n", err);
 	err = ssb_fetch_invariants(bus, get_invariants);
 	if (err) {
 		ssb_bus_may_powerdown(bus);
--- a/drivers/ssb/pci.c
+++ b/drivers/ssb/pci.c
@@ -326,13 +326,13 @@ err_ctlreg:
 	return err;
 }
 
-static s8 r123_extract_antgain(u8 sprom_revision, const u16 *in,
-			       u16 mask, u16 shift)
+static s8 sprom_extract_antgain(u8 sprom_revision, const u16 *in, u16 offset,
+				u16 mask, u16 shift)
 {
 	u16 v;
 	u8 gain;
 
-	v = in[SPOFF(SSB_SPROM1_AGAIN)];
+	v = in[SPOFF(offset)];
 	gain = (v & mask) >> shift;
 	if (gain == 0xFF)
 		gain = 2; /* If unset use 2dBm */
@@ -416,12 +416,14 @@ static void sprom_extract_r123(struct ss
 	SPEX(alpha2[1], SSB_SPROM1_CCODE, 0x00ff, 0);
 
 	/* Extract the antenna gain values. */
-	out->antenna_gain.a0 = r123_extract_antgain(out->revision, in,
-						    SSB_SPROM1_AGAIN_BG,
-						    SSB_SPROM1_AGAIN_BG_SHIFT);
-	out->antenna_gain.a1 = r123_extract_antgain(out->revision, in,
-						    SSB_SPROM1_AGAIN_A,
-						    SSB_SPROM1_AGAIN_A_SHIFT);
+	out->antenna_gain.a0 = sprom_extract_antgain(out->revision, in,
+						     SSB_SPROM1_AGAIN,
+						     SSB_SPROM1_AGAIN_BG,
+						     SSB_SPROM1_AGAIN_BG_SHIFT);
+	out->antenna_gain.a1 = sprom_extract_antgain(out->revision, in,
+						     SSB_SPROM1_AGAIN,
+						     SSB_SPROM1_AGAIN_A,
+						     SSB_SPROM1_AGAIN_A_SHIFT);
 	if (out->revision >= 2)
 		sprom_extract_r23(out, in);
 }
@@ -468,7 +470,15 @@ static void sprom_extract_r458(struct ss
 
 static void sprom_extract_r45(struct ssb_sprom *out, const u16 *in)
 {
+	static const u16 pwr_info_offset[] = {
+		SSB_SPROM4_PWR_INFO_CORE0, SSB_SPROM4_PWR_INFO_CORE1,
+		SSB_SPROM4_PWR_INFO_CORE2, SSB_SPROM4_PWR_INFO_CORE3
+	};
 	u16 il0mac_offset;
+	int i;
+
+	BUILD_BUG_ON(ARRAY_SIZE(pwr_info_offset) !=
+		     ARRAY_SIZE(out->core_pwr_info));
 
 	if (out->revision == 4)
 		il0mac_offset = SSB_SPROM4_IL0MAC;
@@ -524,14 +534,59 @@ static void sprom_extract_r45(struct ssb
 	}
 
 	/* Extract the antenna gain values. */
-	SPEX(antenna_gain.a0, SSB_SPROM4_AGAIN01,
-	     SSB_SPROM4_AGAIN0, SSB_SPROM4_AGAIN0_SHIFT);
-	SPEX(antenna_gain.a1, SSB_SPROM4_AGAIN01,
-	     SSB_SPROM4_AGAIN1, SSB_SPROM4_AGAIN1_SHIFT);
-	SPEX(antenna_gain.a2, SSB_SPROM4_AGAIN23,
-	     SSB_SPROM4_AGAIN2, SSB_SPROM4_AGAIN2_SHIFT);
-	SPEX(antenna_gain.a3, SSB_SPROM4_AGAIN23,
-	     SSB_SPROM4_AGAIN3, SSB_SPROM4_AGAIN3_SHIFT);
+	out->antenna_gain.a0 = sprom_extract_antgain(out->revision, in,
+						     SSB_SPROM4_AGAIN01,
+						     SSB_SPROM4_AGAIN0,
+						     SSB_SPROM4_AGAIN0_SHIFT);
+	out->antenna_gain.a1 = sprom_extract_antgain(out->revision, in,
+						     SSB_SPROM4_AGAIN01,
+						     SSB_SPROM4_AGAIN1,
+						     SSB_SPROM4_AGAIN1_SHIFT);
+	out->antenna_gain.a2 = sprom_extract_antgain(out->revision, in,
+						     SSB_SPROM4_AGAIN23,
+						     SSB_SPROM4_AGAIN2,
+						     SSB_SPROM4_AGAIN2_SHIFT);
+	out->antenna_gain.a3 = sprom_extract_antgain(out->revision, in,
+						     SSB_SPROM4_AGAIN23,
+						     SSB_SPROM4_AGAIN3,
+						     SSB_SPROM4_AGAIN3_SHIFT);
+
+	/* Extract cores power info info */
+	for (i = 0; i < ARRAY_SIZE(pwr_info_offset); i++) {
+		u16 o = pwr_info_offset[i];
+
+		SPEX(core_pwr_info[i].itssi_2g, o + SSB_SPROM4_2G_MAXP_ITSSI,
+			SSB_SPROM4_2G_ITSSI, SSB_SPROM4_2G_ITSSI_SHIFT);
+		SPEX(core_pwr_info[i].maxpwr_2g, o + SSB_SPROM4_2G_MAXP_ITSSI,
+			SSB_SPROM4_2G_MAXP, 0);
+
+		SPEX(core_pwr_info[i].pa_2g[0], o + SSB_SPROM4_2G_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_2g[1], o + SSB_SPROM4_2G_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_2g[2], o + SSB_SPROM4_2G_PA_2, ~0, 0);
+		SPEX(core_pwr_info[i].pa_2g[3], o + SSB_SPROM4_2G_PA_3, ~0, 0);
+
+		SPEX(core_pwr_info[i].itssi_5g, o + SSB_SPROM4_5G_MAXP_ITSSI,
+			SSB_SPROM4_5G_ITSSI, SSB_SPROM4_5G_ITSSI_SHIFT);
+		SPEX(core_pwr_info[i].maxpwr_5g, o + SSB_SPROM4_5G_MAXP_ITSSI,
+			SSB_SPROM4_5G_MAXP, 0);
+		SPEX(core_pwr_info[i].maxpwr_5gh, o + SSB_SPROM4_5GHL_MAXP,
+			SSB_SPROM4_5GH_MAXP, 0);
+		SPEX(core_pwr_info[i].maxpwr_5gl, o + SSB_SPROM4_5GHL_MAXP,
+			SSB_SPROM4_5GL_MAXP, SSB_SPROM4_5GL_MAXP_SHIFT);
+
+		SPEX(core_pwr_info[i].pa_5gl[0], o + SSB_SPROM4_5GL_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gl[1], o + SSB_SPROM4_5GL_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gl[2], o + SSB_SPROM4_5GL_PA_2, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gl[3], o + SSB_SPROM4_5GL_PA_3, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[0], o + SSB_SPROM4_5G_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[1], o + SSB_SPROM4_5G_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[2], o + SSB_SPROM4_5G_PA_2, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[3], o + SSB_SPROM4_5G_PA_3, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[0], o + SSB_SPROM4_5GH_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[1], o + SSB_SPROM4_5GH_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[2], o + SSB_SPROM4_5GH_PA_2, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[3], o + SSB_SPROM4_5GH_PA_3, ~0, 0);
+	}
 
 	sprom_extract_r458(out, in);
 
@@ -621,14 +676,22 @@ static void sprom_extract_r8(struct ssb_
 	SPEX32(ofdm5ghpo, SSB_SPROM8_OFDM5GHPO, 0xFFFFFFFF, 0);
 
 	/* Extract the antenna gain values. */
-	SPEX(antenna_gain.a0, SSB_SPROM8_AGAIN01,
-	     SSB_SPROM8_AGAIN0, SSB_SPROM8_AGAIN0_SHIFT);
-	SPEX(antenna_gain.a1, SSB_SPROM8_AGAIN01,
-	     SSB_SPROM8_AGAIN1, SSB_SPROM8_AGAIN1_SHIFT);
-	SPEX(antenna_gain.a2, SSB_SPROM8_AGAIN23,
-	     SSB_SPROM8_AGAIN2, SSB_SPROM8_AGAIN2_SHIFT);
-	SPEX(antenna_gain.a3, SSB_SPROM8_AGAIN23,
-	     SSB_SPROM8_AGAIN3, SSB_SPROM8_AGAIN3_SHIFT);
+	out->antenna_gain.a0 = sprom_extract_antgain(out->revision, in,
+						     SSB_SPROM8_AGAIN01,
+						     SSB_SPROM8_AGAIN0,
+						     SSB_SPROM8_AGAIN0_SHIFT);
+	out->antenna_gain.a1 = sprom_extract_antgain(out->revision, in,
+						     SSB_SPROM8_AGAIN01,
+						     SSB_SPROM8_AGAIN1,
+						     SSB_SPROM8_AGAIN1_SHIFT);
+	out->antenna_gain.a2 = sprom_extract_antgain(out->revision, in,
+						     SSB_SPROM8_AGAIN23,
+						     SSB_SPROM8_AGAIN2,
+						     SSB_SPROM8_AGAIN2_SHIFT);
+	out->antenna_gain.a3 = sprom_extract_antgain(out->revision, in,
+						     SSB_SPROM8_AGAIN23,
+						     SSB_SPROM8_AGAIN3,
+						     SSB_SPROM8_AGAIN3_SHIFT);
 
 	/* Extract cores power info info */
 	for (i = 0; i < ARRAY_SIZE(pwr_info_offset); i++) {
--- a/drivers/ssb/pcihost_wrapper.c
+++ b/drivers/ssb/pcihost_wrapper.c
@@ -11,15 +11,17 @@
  * Licensed under the GNU/GPL. See COPYING for details.
  */
 
+#include <linux/pm.h>
 #include <linux/pci.h>
 #include <linux/export.h>
 #include <linux/slab.h>
 #include <linux/ssb/ssb.h>
 
 
-#ifdef CONFIG_PM
-static int ssb_pcihost_suspend(struct pci_dev *dev, pm_message_t state)
+#ifdef CONFIG_PM_SLEEP
+static int ssb_pcihost_suspend(struct device *d)
 {
+	struct pci_dev *dev = to_pci_dev(d);
 	struct ssb_bus *ssb = pci_get_drvdata(dev);
 	int err;
 
@@ -28,17 +30,23 @@ static int ssb_pcihost_suspend(struct pc
 		return err;
 	pci_save_state(dev);
 	pci_disable_device(dev);
-	pci_set_power_state(dev, pci_choose_state(dev, state));
+
+	/* if there is a wakeup enabled child device on ssb bus,
+	   enable pci wakeup posibility. */
+	device_set_wakeup_enable(d, d->power.wakeup_path);
+
+	pci_prepare_to_sleep(dev);
 
 	return 0;
 }
 
-static int ssb_pcihost_resume(struct pci_dev *dev)
+static int ssb_pcihost_resume(struct device *d)
 {
+	struct pci_dev *dev = to_pci_dev(d);
 	struct ssb_bus *ssb = pci_get_drvdata(dev);
 	int err;
 
-	pci_set_power_state(dev, 0);
+	pci_back_from_sleep(dev);
 	err = pci_enable_device(dev);
 	if (err)
 		return err;
@@ -49,10 +57,12 @@ static int ssb_pcihost_resume(struct pci
 
 	return 0;
 }
-#else /* CONFIG_PM */
-# define ssb_pcihost_suspend	NULL
-# define ssb_pcihost_resume	NULL
-#endif /* CONFIG_PM */
+
+static const struct dev_pm_ops ssb_pcihost_pm_ops = {
+	SET_SYSTEM_SLEEP_PM_OPS(ssb_pcihost_suspend, ssb_pcihost_resume)
+};
+
+#endif /* CONFIG_PM_SLEEP */
 
 static int ssb_pcihost_probe(struct pci_dev *dev,
 			     const struct pci_device_id *id)
@@ -115,8 +125,9 @@ int ssb_pcihost_register(struct pci_driv
 {
 	driver->probe = ssb_pcihost_probe;
 	driver->remove = ssb_pcihost_remove;
-	driver->suspend = ssb_pcihost_suspend;
-	driver->resume = ssb_pcihost_resume;
+#ifdef CONFIG_PM_SLEEP
+	driver->driver.pm = &ssb_pcihost_pm_ops;
+#endif
 
 	return pci_register_driver(driver);
 }
--- a/drivers/ssb/sprom.c
+++ b/drivers/ssb/sprom.c
@@ -54,7 +54,7 @@ static int hex2sprom(u16 *sprom, const c
 	while (cnt < sprom_size_words) {
 		memcpy(tmp, dump, 4);
 		dump += 4;
-		err = strict_strtoul(tmp, 16, &parsed);
+		err = kstrtoul(tmp, 16, &parsed);
 		if (err)
 			return err;
 		sprom[cnt++] = swab16((u16)parsed);
--- a/drivers/ssb/ssb_private.h
+++ b/drivers/ssb/ssb_private.h
@@ -243,6 +243,10 @@ static inline int ssb_sflash_init(struct
 extern struct platform_device ssb_pflash_dev;
 #endif
 
+#ifdef CONFIG_SSB_SFLASH
+extern struct platform_device ssb_sflash_dev;
+#endif
+
 #ifdef CONFIG_SSB_DRIVER_EXTIF
 extern u32 ssb_extif_watchdog_timer_set_wdt(struct bcm47xx_wdt *wdt, u32 ticks);
 extern u32 ssb_extif_watchdog_timer_set_ms(struct bcm47xx_wdt *wdt, u32 ms);
--- a/include/linux/ssb/ssb.h
+++ b/include/linux/ssb/ssb.h
@@ -33,6 +33,7 @@ struct ssb_sprom {
 	u8 et1phyaddr;		/* MII address for enet1 */
 	u8 et0mdcport;		/* MDIO for enet0 */
 	u8 et1mdcport;		/* MDIO for enet1 */
+	u16 dev_id;		/* Device ID overriding e.g. PCI ID */
 	u16 board_rev;		/* Board revision number from SPROM. */
 	u16 board_num;		/* Board number from SPROM. */
 	u16 board_type;		/* Board type from SPROM. */
@@ -486,6 +487,7 @@ struct ssb_bus {
 #endif /* EMBEDDED */
 #ifdef CONFIG_SSB_DRIVER_GPIO
 	struct gpio_chip gpio;
+	struct irq_domain *irq_domain;
 #endif /* DRIVER_GPIO */
 
 	/* Internal-only stuff follows. Do not touch. */
--- a/include/linux/ssb/ssb_driver_gige.h
+++ b/include/linux/ssb/ssb_driver_gige.h
@@ -108,6 +108,16 @@ static inline int ssb_gige_get_macaddr(s
 	return 0;
 }
 
+/* Get the device phy address */
+static inline int ssb_gige_get_phyaddr(struct pci_dev *pdev)
+{
+	struct ssb_gige *dev = pdev_to_ssb_gige(pdev);
+	if (!dev)
+		return -ENODEV;
+
+	return dev->dev->bus->sprom.et0phyaddr;
+}
+
 extern int ssb_gige_pcibios_plat_dev_init(struct ssb_device *sdev,
 					  struct pci_dev *pdev);
 extern int ssb_gige_map_irq(struct ssb_device *sdev,
@@ -174,6 +184,10 @@ static inline int ssb_gige_get_macaddr(s
 {
 	return -ENODEV;
 }
+static inline int ssb_gige_get_phyaddr(struct pci_dev *pdev)
+{
+	return -ENODEV;
+}
 
 #endif /* CONFIG_SSB_DRIVER_GIGE */
 #endif /* LINUX_SSB_DRIVER_GIGE_H_ */
--- a/include/linux/ssb/ssb_driver_mips.h
+++ b/include/linux/ssb/ssb_driver_mips.h
@@ -20,6 +20,18 @@ struct ssb_pflash {
 	u32 window_size;
 };
 
+#ifdef CONFIG_SSB_SFLASH
+struct ssb_sflash {
+	bool present;
+	u32 window;
+	u32 blocksize;
+	u16 numblocks;
+	u32 size;
+
+	void *priv;
+};
+#endif
+
 struct ssb_mipscore {
 	struct ssb_device *dev;
 
@@ -27,6 +39,9 @@ struct ssb_mipscore {
 	struct ssb_serial_port serial_ports[4];
 
 	struct ssb_pflash pflash;
+#ifdef CONFIG_SSB_SFLASH
+	struct ssb_sflash sflash;
+#endif
 };
 
 extern void ssb_mipscore_init(struct ssb_mipscore *mcore);
--- a/include/linux/ssb/ssb_regs.h
+++ b/include/linux/ssb/ssb_regs.h
@@ -172,6 +172,7 @@
 #define SSB_SPROMSIZE_WORDS_R4		220
 #define SSB_SPROMSIZE_BYTES_R123	(SSB_SPROMSIZE_WORDS_R123 * sizeof(u16))
 #define SSB_SPROMSIZE_BYTES_R4		(SSB_SPROMSIZE_WORDS_R4 * sizeof(u16))
+#define SSB_SPROMSIZE_WORDS_R10		230
 #define SSB_SPROM_BASE1			0x1000
 #define SSB_SPROM_BASE31		0x0800
 #define SSB_SPROM_REVISION		0x007E
@@ -344,6 +345,43 @@
 #define  SSB_SPROM4_TXPID5GH2_SHIFT	0
 #define  SSB_SPROM4_TXPID5GH3		0xFF00
 #define  SSB_SPROM4_TXPID5GH3_SHIFT	8
+
+/* There are 4 blocks with power info sharing the same layout */
+#define SSB_SPROM4_PWR_INFO_CORE0	0x0080
+#define SSB_SPROM4_PWR_INFO_CORE1	0x00AE
+#define SSB_SPROM4_PWR_INFO_CORE2	0x00DC
+#define SSB_SPROM4_PWR_INFO_CORE3	0x010A
+
+#define SSB_SPROM4_2G_MAXP_ITSSI	0x00	/* 2 GHz ITSSI and 2 GHz Max Power */
+#define  SSB_SPROM4_2G_MAXP		0x00FF
+#define  SSB_SPROM4_2G_ITSSI		0xFF00
+#define  SSB_SPROM4_2G_ITSSI_SHIFT	8
+#define SSB_SPROM4_2G_PA_0		0x02	/* 2 GHz power amp */
+#define SSB_SPROM4_2G_PA_1		0x04
+#define SSB_SPROM4_2G_PA_2		0x06
+#define SSB_SPROM4_2G_PA_3		0x08
+#define SSB_SPROM4_5G_MAXP_ITSSI	0x0A	/* 5 GHz ITSSI and 5.3 GHz Max Power */
+#define  SSB_SPROM4_5G_MAXP		0x00FF
+#define  SSB_SPROM4_5G_ITSSI		0xFF00
+#define  SSB_SPROM4_5G_ITSSI_SHIFT	8
+#define SSB_SPROM4_5GHL_MAXP		0x0C	/* 5.2 GHz and 5.8 GHz Max Power */
+#define  SSB_SPROM4_5GH_MAXP		0x00FF
+#define  SSB_SPROM4_5GL_MAXP		0xFF00
+#define  SSB_SPROM4_5GL_MAXP_SHIFT	8
+#define SSB_SPROM4_5G_PA_0		0x0E	/* 5.3 GHz power amp */
+#define SSB_SPROM4_5G_PA_1		0x10
+#define SSB_SPROM4_5G_PA_2		0x12
+#define SSB_SPROM4_5G_PA_3		0x14
+#define SSB_SPROM4_5GL_PA_0		0x16	/* 5.2 GHz power amp */
+#define SSB_SPROM4_5GL_PA_1		0x18
+#define SSB_SPROM4_5GL_PA_2		0x1A
+#define SSB_SPROM4_5GL_PA_3		0x1C
+#define SSB_SPROM4_5GH_PA_0		0x1E	/* 5.8 GHz power amp */
+#define SSB_SPROM4_5GH_PA_1		0x20
+#define SSB_SPROM4_5GH_PA_2		0x22
+#define SSB_SPROM4_5GH_PA_3		0x24
+
+/* TODO: Make it deprecated */
 #define SSB_SPROM4_MAXP_BG		0x0080  /* Max Power BG in path 1 */
 #define  SSB_SPROM4_MAXP_BG_MASK	0x00FF  /* Mask for Max Power BG */
 #define  SSB_SPROM4_ITSSI_BG		0xFF00	/* Mask for path 1 itssi_bg */
--- a/arch/mips/bcm47xx/sprom.c
+++ b/arch/mips/bcm47xx/sprom.c
@@ -168,6 +168,7 @@ static void nvram_read_alpha2(const char
 static void bcm47xx_fill_sprom_r1234589(struct ssb_sprom *sprom,
 					const char *prefix, bool fallback)
 {
+	nvram_read_u16(prefix, NULL, "devid", &sprom->dev_id, 0, fallback);
 	nvram_read_u8(prefix, NULL, "ledbh0", &sprom->gpio0, 0xff, fallback);
 	nvram_read_u8(prefix, NULL, "ledbh1", &sprom->gpio1, 0xff, fallback);
 	nvram_read_u8(prefix, NULL, "ledbh2", &sprom->gpio2, 0xff, fallback);
