From 49b47dfcef1353cd28eac8f64170e75d28ce4311 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Sun, 14 Jul 2013 23:18:57 +0200
Subject: [PATCH 29/57] serial: of: allow au1x00 and rt288x to load from OF

In order to make serial_8250 loadable via OF on Au1x00 and Ralink WiSoC we need
to default the iotype to UPIO_AU.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/tty/serial/of_serial.c |    5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

--- a/drivers/tty/serial/of_serial.c
+++ b/drivers/tty/serial/of_serial.c
@@ -102,7 +102,10 @@ static int of_platform_serial_setup(stru
 		port->fifosize = prop;
 
 	port->irq = irq_of_parse_and_map(np, 0);
-	port->iotype = UPIO_MEM;
+	if (of_device_is_compatible(np, "ralink,rt2880-uart"))
+		port->iotype = UPIO_AU;
+	else
+		port->iotype = UPIO_MEM;
 	if (of_property_read_u32(np, "reg-io-width", &prop) == 0) {
 		switch (prop) {
 		case 1:
