From c61dfeb17581d32360a817ba40636aaed85caade Mon Sep 17 00:00:00 2001
From: Roman Byshko <rbyshko@gmail.com>
Date: Fri, 7 Feb 2014 16:21:50 +0100
Subject: [PATCH] clk: sunxi: Add USB clock register defintions
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Add register definitions for the usb-clk register found on sun4i, sun5i and
sun7i SoCs.

Signed-off-by: Roman Byshko <rbyshko@gmail.com>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
Acked-by: Maxime Ripard <maxime.ripard@free-electrons.com>
Signed-off-by: Emilio López <emilio@elopez.com.ar>
---
 Documentation/devicetree/bindings/clock/sunxi.txt |  5 +++++
 drivers/clk/sunxi/clk-sunxi.c                     | 12 ++++++++++++
 2 files changed, 17 insertions(+)

--- a/Documentation/devicetree/bindings/clock/sunxi.txt
+++ b/Documentation/devicetree/bindings/clock/sunxi.txt
@@ -37,6 +37,8 @@ Required properties:
 	"allwinner,sun6i-a31-apb2-gates-clk" - for the APB2 gates on A31
 	"allwinner,sun4i-mod0-clk" - for the module 0 family of clocks
 	"allwinner,sun7i-a20-out-clk" - for the external output clocks
+	"allwinner,sun4i-a10-usb-clk" - for usb gates + resets on A10 / A20
+	"allwinner,sun5i-a13-usb-clk" - for usb gates + resets on A13
 
 Required properties for all clocks:
 - reg : shall be the control register address for the clock.
@@ -49,6 +51,9 @@ Required properties for all clocks:
 Additionally, "allwinner,*-gates-clk" clocks require:
 - clock-output-names : the corresponding gate names that the clock controls
 
+And "allwinner,*-usb-clk" clocks also require:
+- reset-cells : shall be set to 1
+
 Clock consumers should specify the desired clocks they use with a
 "clocks" phandle cell. Consumers that are using a gated clock should
 provide an additional ID in their clock property. This ID is the
--- a/drivers/clk/sunxi/clk-sunxi.c
+++ b/drivers/clk/sunxi/clk-sunxi.c
@@ -816,6 +816,16 @@ static const struct gates_data sun7i_a20
 	.mask = { 0xff80ff },
 };
 
+static const struct gates_data sun4i_a10_usb_gates_data __initconst = {
+	.mask = {0x1C0},
+	.reset_mask = 0x07,
+};
+
+static const struct gates_data sun5i_a13_usb_gates_data __initconst = {
+	.mask = {0x140},
+	.reset_mask = 0x03,
+};
+
 static void __init sunxi_gates_clk_setup(struct device_node *node,
 					 struct gates_data *data)
 {
@@ -1107,6 +1117,8 @@ static const struct of_device_id clk_gat
 	{.compatible = "allwinner,sun6i-a31-apb1-gates-clk", .data = &sun6i_a31_apb1_gates_data,},
 	{.compatible = "allwinner,sun7i-a20-apb1-gates-clk", .data = &sun7i_a20_apb1_gates_data,},
 	{.compatible = "allwinner,sun6i-a31-apb2-gates-clk", .data = &sun6i_a31_apb2_gates_data,},
+	{.compatible = "allwinner,sun4i-a10-usb-clk", .data = &sun4i_a10_usb_gates_data,},
+	{.compatible = "allwinner,sun5i-a13-usb-clk", .data = &sun5i_a13_usb_gates_data,},
 	{}
 };
 
