From c9bfaadf8973cb4d9074e80c4bf8708deca62712 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Sat, 22 Feb 2014 22:35:54 +0100
Subject: [PATCH] ARM: dt: sun7i: Add A20 SPI controller nodes

The A20 has 4 SPI controllers compatible with the one found in the A10. Add
them in the DT.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 44 ++++++++++++++++++++++++++++++++++++++++
 1 file changed, 44 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -401,6 +401,28 @@
 		#size-cells = <1>;
 		ranges;
 
+		spi0: spi@01c05000 {
+			compatible = "allwinner,sun4i-a10-spi";
+			reg = <0x01c05000 0x1000>;
+			interrupts = <0 10 4>;
+			clocks = <&ahb_gates 20>, <&spi0_clk>;
+			clock-names = "ahb", "mod";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		spi1: spi@01c06000 {
+			compatible = "allwinner,sun4i-a10-spi";
+			reg = <0x01c06000 0x1000>;
+			interrupts = <0 11 4>;
+			clocks = <&ahb_gates 21>, <&spi1_clk>;
+			clock-names = "ahb", "mod";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
 		emac: ethernet@01c0b000 {
 			compatible = "allwinner,sun4i-a10-emac";
 			reg = <0x01c0b000 0x1000>;
@@ -417,6 +439,28 @@
 			#size-cells = <0>;
 		};
 
+		spi2: spi@01c17000 {
+			compatible = "allwinner,sun4i-a10-spi";
+			reg = <0x01c17000 0x1000>;
+			interrupts = <0 12 4>;
+			clocks = <&ahb_gates 22>, <&spi2_clk>;
+			clock-names = "ahb", "mod";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		spi3: spi@01c1f000 {
+			compatible = "allwinner,sun4i-a10-spi";
+			reg = <0x01c1f000 0x1000>;
+			interrupts = <0 50 4>;
+			clocks = <&ahb_gates 23>, <&spi3_clk>;
+			clock-names = "ahb", "mod";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
 		pio: pinctrl@01c20800 {
 			compatible = "allwinner,sun7i-a20-pinctrl";
 			reg = <0x01c20800 0x400>;
