From ed6c71de07ad042691ec02e9eb97375ddc91ed01 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Tue, 3 Dec 2013 13:45:22 +0100
Subject: [PATCH 6/8] MIPS: BCM63XX: remove !RUNTIME_DETECT usage from enet
 code

---
 arch/mips/bcm63xx/dev-enet.c                       |  4 --
 .../include/asm/mach-bcm63xx/bcm63xx_dev_enet.h    | 46 ----------------------
 2 files changed, 50 deletions(-)

--- a/arch/mips/bcm63xx/dev-enet.c
+++ b/arch/mips/bcm63xx/dev-enet.c
@@ -14,7 +14,6 @@
 #include <bcm63xx_io.h>
 #include <bcm63xx_regs.h>
 
-#ifdef BCMCPU_RUNTIME_DETECT
 static const unsigned long bcm6348_regs_enetdmac[] = {
 	[ENETDMAC_CHANCFG]	= ENETDMAC_CHANCFG_REG,
 	[ENETDMAC_IR]		= ENETDMAC_IR_REG,
@@ -43,9 +42,6 @@ static __init void bcm63xx_enetdmac_regs
 	else
 		bcm63xx_regs_enetdmac = bcm6348_regs_enetdmac;
 }
-#else
-static __init void bcm63xx_enetdmac_regs_init(void) { }
-#endif
 
 static struct resource shared_res[] = {
 	{
--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_dev_enet.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_dev_enet.h
@@ -112,55 +112,9 @@ enum bcm63xx_regs_enetdmac {
 
 static inline unsigned long bcm63xx_enetdmacreg(enum bcm63xx_regs_enetdmac reg)
 {
-#ifdef BCMCPU_RUNTIME_DETECT
 	extern const unsigned long *bcm63xx_regs_enetdmac;
 
 	return bcm63xx_regs_enetdmac[reg];
-#else
-#ifdef CONFIG_BCM63XX_CPU_6345
-	switch (reg) {
-	case ENETDMAC_CHANCFG:
-		return ENETDMA_6345_CHANCFG_REG;
-	case ENETDMAC_IR:
-		return ENETDMA_6345_IR_REG;
-	case ENETDMAC_IRMASK:
-		return ENETDMA_6345_IRMASK_REG;
-	case ENETDMAC_MAXBURST:
-		return ENETDMA_6345_MAXBURST_REG;
-	case ENETDMAC_BUFALLOC:
-		return ENETDMA_6345_BUFALLOC_REG;
-	case ENETDMAC_RSTART:
-		return ENETDMA_6345_RSTART_REG;
-	case ENETDMAC_FC:
-		return ENETDMA_6345_FC_REG;
-	case ENETDMAC_LEN:
-		return ENETDMA_6345_LEN_REG;
-	}
-#endif
-#if defined(CONFIG_BCM63XX_CPU_6328) || \
-	defined(CONFIG_BCM63XX_CPU_6338) || \
-	defined(CONFIG_BCM63XX_CPU_6348) || \
-	defined(CONFIG_BCM63XX_CPU_6358) || \
-	defined(CONFIG_BCM63XX_CPU_6362) || \
-	defined(CONFIG_BCM63XX_CPU_6368)
-	switch (reg) {
-	case ENETDMAC_CHANCFG:
-		return ENETDMAC_CHANCFG_REG;
-	case ENETDMAC_IR:
-		return ENETDMAC_IR_REG;
-	case ENETDMAC_IRMASK:
-		return ENETDMAC_IRMASK_REG;
-	case ENETDMAC_MAXBURST:
-		return ENETDMAC_MAXBURST_REG;
-	case ENETDMAC_BUFALLOC:
-	case ENETDMAC_RSTART:
-	case ENETDMAC_FC:
-	case ENETDMAC_LEN:
-		return 0;
-	}
-#endif
-#endif
-	return 0;
 }
 
 
