--- a/net/bridge/br_multicast.c
+++ b/net/bridge/br_multicast.c
@@ -634,7 +634,8 @@ struct net_bridge_port_group *br_multica
 			struct net_bridge_port *port,
 			struct br_ip *group,
 			struct net_bridge_port_group __rcu *next,
-			unsigned char state)
+			unsigned char state,
+			const unsigned char *src)
 {
 	struct net_bridge_port_group *p;
 
@@ -649,12 +650,33 @@ struct net_bridge_port_group *br_multica
 	hlist_add_head(&p->mglist, &port->mglist);
 	setup_timer(&p->timer, br_multicast_port_group_expired,
 		    (unsigned long)p);
+	if ((port->flags & BR_MULTICAST_TO_UCAST) && src) {
+		memcpy(p->eth_addr, src, ETH_ALEN);
+		p->unicast = true;
+	}
 	return p;
 }
 
+static bool br_port_group_equal(struct net_bridge_port_group *p,
+				struct net_bridge_port *port,
+				const unsigned char *src)
+{
+	if (p->port != port)
+		return false;
+
+	if (!p->unicast)
+		return true;
+
+	if (!src)
+		return false;
+
+	return ether_addr_equal(src, p->eth_addr);
+}
+
 static int br_multicast_add_group(struct net_bridge *br,
 				  struct net_bridge_port *port,
-				  struct br_ip *group)
+				  struct br_ip *group,
+				  const unsigned char *src)
 {
 	struct net_bridge_mdb_entry *mp;
 	struct net_bridge_port_group *p;
@@ -681,13 +703,13 @@ static int br_multicast_add_group(struct
 	for (pp = &mp->ports;
 	     (p = mlock_dereference(*pp, br)) != NULL;
 	     pp = &p->next) {
-		if (p->port == port)
+		if (br_port_group_equal(p, port, src))
 			goto found;
 		if ((unsigned long)p->port < (unsigned long)port)
 			break;
 	}
 
-	p = br_multicast_new_port_group(port, group, *pp, MDB_TEMPORARY);
+	p = br_multicast_new_port_group(port, group, *pp, MDB_TEMPORARY, src);
 	if (unlikely(!p))
 		goto err;
 	rcu_assign_pointer(*pp, p);
@@ -706,7 +728,7 @@ err:
 static int br_ip4_multicast_add_group(struct net_bridge *br,
 				      struct net_bridge_port *port,
 				      __be32 group,
-				      __u16 vid)
+				      __u16 vid, const unsigned char *src)
 {
 	struct br_ip br_group;
 
@@ -717,14 +739,14 @@ static int br_ip4_multicast_add_group(st
 	br_group.proto = htons(ETH_P_IP);
 	br_group.vid = vid;
 
-	return br_multicast_add_group(br, port, &br_group);
+	return br_multicast_add_group(br, port, &br_group, src);
 }
 
 #if IS_ENABLED(CONFIG_IPV6)
 static int br_ip6_multicast_add_group(struct net_bridge *br,
 				      struct net_bridge_port *port,
 				      const struct in6_addr *group,
-				      __u16 vid)
+				      __u16 vid, const unsigned char *src)
 {
 	struct br_ip br_group;
 
@@ -735,7 +757,10 @@ static int br_ip6_multicast_add_group(st
 	br_group.proto = htons(ETH_P_IPV6);
 	br_group.vid = vid;
 
-	return br_multicast_add_group(br, port, &br_group);
+	if (ipv6_addr_is_solict_mult(group))
+		src = NULL;
+
+	return br_multicast_add_group(br, port, &br_group, src);
 }
 #endif
 
@@ -949,6 +974,7 @@ static int br_ip4_multicast_igmp3_report
 					 struct net_bridge_port *port,
 					 struct sk_buff *skb)
 {
+	const unsigned char *src = eth_hdr(skb)->h_source;
 	struct igmpv3_report *ih;
 	struct igmpv3_grec *grec;
 	int i;
@@ -994,7 +1020,7 @@ static int br_ip4_multicast_igmp3_report
 			continue;
 		}
 
-		err = br_ip4_multicast_add_group(br, port, group, vid);
+		err = br_ip4_multicast_add_group(br, port, group, vid, src);
 		if (err)
 			break;
 	}
@@ -1007,6 +1033,7 @@ static int br_ip6_multicast_mld2_report(
 					struct net_bridge_port *port,
 					struct sk_buff *skb)
 {
+	const unsigned char *src = eth_hdr(skb)->h_source;
 	struct icmp6hdr *icmp6h;
 	struct mld2_grec *grec;
 	int i;
@@ -1057,7 +1084,7 @@ static int br_ip6_multicast_mld2_report(
 		}
 
 		err = br_ip6_multicast_add_group(br, port, &grec->grec_mca,
-						 vid);
+						 vid, src);
 		if (!err)
 			break;
 	}
@@ -1302,7 +1329,8 @@ static void br_multicast_leave_group(str
 				     struct net_bridge_port *port,
 				     struct br_ip *group,
 				     struct bridge_mcast_querier *querier,
-				     struct bridge_mcast_query *query)
+				     struct bridge_mcast_query *query,
+				     const unsigned char *src)
 {
 	struct net_bridge_mdb_htable *mdb;
 	struct net_bridge_mdb_entry *mp;
@@ -1352,7 +1380,7 @@ static void br_multicast_leave_group(str
 		for (pp = &mp->ports;
 		     (p = mlock_dereference(*pp, br)) != NULL;
 		     pp = &p->next) {
-			if (p->port != port)
+			if (!br_port_group_equal(p, port, src))
 				continue;
 
 			rcu_assign_pointer(*pp, p->next);
@@ -1386,7 +1414,7 @@ static void br_multicast_leave_group(str
 	for (p = mlock_dereference(mp->ports, br);
 	     p != NULL;
 	     p = mlock_dereference(p->next, br)) {
-		if (p->port != port)
+		if (!br_port_group_equal(p, port, src))
 			continue;
 
 		if (!hlist_unhashed(&p->mglist) &&
@@ -1404,8 +1432,8 @@ out:
 
 static void br_ip4_multicast_leave_group(struct net_bridge *br,
 					 struct net_bridge_port *port,
-					 __be32 group,
-					 __u16 vid)
+					 __be32 group, __u16 vid,
+					 const unsigned char *src)
 {
 	struct br_ip br_group;
 	struct bridge_mcast_query *query = port ? &port->ip4_query :
@@ -1418,14 +1446,15 @@ static void br_ip4_multicast_leave_group
 	br_group.proto = htons(ETH_P_IP);
 	br_group.vid = vid;
 
-	br_multicast_leave_group(br, port, &br_group, &br->ip4_querier, query);
+	br_multicast_leave_group(br, port, &br_group, &br->ip4_querier, query,
+				 src);
 }
 
 #if IS_ENABLED(CONFIG_IPV6)
 static void br_ip6_multicast_leave_group(struct net_bridge *br,
 					 struct net_bridge_port *port,
 					 const struct in6_addr *group,
-					 __u16 vid)
+					 __u16 vid, const unsigned char *src)
 {
 	struct br_ip br_group;
 	struct bridge_mcast_query *query = port ? &port->ip6_query :
@@ -1439,7 +1468,8 @@ static void br_ip6_multicast_leave_group
 	br_group.proto = htons(ETH_P_IPV6);
 	br_group.vid = vid;
 
-	br_multicast_leave_group(br, port, &br_group, &br->ip6_querier, query);
+	br_multicast_leave_group(br, port, &br_group, &br->ip6_querier, query,
+				 src);
 }
 #endif
 
@@ -1447,6 +1477,7 @@ static int br_multicast_ipv4_rcv(struct 
 				 struct net_bridge_port *port,
 				 struct sk_buff *skb)
 {
+	const unsigned char *src = eth_hdr(skb)->h_source;
 	struct sk_buff *skb2 = skb;
 	const struct iphdr *iph;
 	struct igmphdr *ih;
@@ -1522,7 +1553,7 @@ static int br_multicast_ipv4_rcv(struct 
 	case IGMP_HOST_MEMBERSHIP_REPORT:
 	case IGMPV2_HOST_MEMBERSHIP_REPORT:
 		BR_INPUT_SKB_CB(skb)->mrouters_only = 1;
-		err = br_ip4_multicast_add_group(br, port, ih->group, vid);
+		err = br_ip4_multicast_add_group(br, port, ih->group, vid, src);
 		break;
 	case IGMPV3_HOST_MEMBERSHIP_REPORT:
 		err = br_ip4_multicast_igmp3_report(br, port, skb2);
@@ -1531,7 +1562,7 @@ static int br_multicast_ipv4_rcv(struct 
 		err = br_ip4_multicast_query(br, port, skb2);
 		break;
 	case IGMP_HOST_LEAVE_MESSAGE:
-		br_ip4_multicast_leave_group(br, port, ih->group, vid);
+		br_ip4_multicast_leave_group(br, port, ih->group, vid, src);
 		break;
 	}
 
@@ -1548,6 +1579,7 @@ static int br_multicast_ipv6_rcv(struct 
 				 struct net_bridge_port *port,
 				 struct sk_buff *skb)
 {
+	const unsigned char *src = eth_hdr(skb)->h_source;
 	struct sk_buff *skb2;
 	const struct ipv6hdr *ip6h;
 	u8 icmp6_type;
@@ -1659,7 +1691,8 @@ static int br_multicast_ipv6_rcv(struct 
 		}
 		mld = (struct mld_msg *)skb_transport_header(skb2);
 		BR_INPUT_SKB_CB(skb)->mrouters_only = 1;
-		err = br_ip6_multicast_add_group(br, port, &mld->mld_mca, vid);
+		err = br_ip6_multicast_add_group(br, port, &mld->mld_mca, vid,
+						 src);
 		break;
 	    }
 	case ICMPV6_MLD2_REPORT:
@@ -1676,7 +1709,7 @@ static int br_multicast_ipv6_rcv(struct 
 			goto out;
 		}
 		mld = (struct mld_msg *)skb_transport_header(skb2);
-		br_ip6_multicast_leave_group(br, port, &mld->mld_mca, vid);
+		br_ip6_multicast_leave_group(br, port, &mld->mld_mca, vid, src);
 	    }
 	}
 
--- a/net/bridge/br_private.h
+++ b/net/bridge/br_private.h
@@ -115,6 +115,9 @@ struct net_bridge_port_group {
 	struct timer_list		timer;
 	struct br_ip			addr;
 	unsigned char			state;
+
+	unsigned char			eth_addr[ETH_ALEN];
+	bool				unicast;
 };
 
 struct net_bridge_mdb_entry
@@ -172,6 +175,7 @@ struct net_bridge_port
 #define BR_MULTICAST_FAST_LEAVE	0x00000008
 #define BR_ADMIN_COST		0x00000010
 #define BR_ISOLATE_MODE		0x00000020
+#define BR_MULTICAST_TO_UCAST	0x00000040
 
 #ifdef CONFIG_BRIDGE_IGMP_SNOOPING
 	struct bridge_mcast_query	ip4_query;
@@ -489,7 +493,8 @@ extern struct net_bridge_port_group *br_
 				struct net_bridge_port *port,
 				struct br_ip *group,
 				struct net_bridge_port_group *next,
-				unsigned char state);
+				unsigned char state,
+				const unsigned char *src);
 extern void br_mdb_init(void);
 extern void br_mdb_uninit(void);
 extern void br_mdb_notify(struct net_device *dev, struct net_bridge_port *port,
--- a/net/bridge/br_mdb.c
+++ b/net/bridge/br_mdb.c
@@ -341,7 +341,7 @@ static int br_mdb_add_group(struct net_b
 			break;
 	}
 
-	p = br_multicast_new_port_group(port, group, *pp, state);
+	p = br_multicast_new_port_group(port, group, *pp, state, NULL);
 	if (unlikely(!p))
 		return -ENOMEM;
 	rcu_assign_pointer(*pp, p);
--- a/net/bridge/br_forward.c
+++ b/net/bridge/br_forward.c
@@ -170,6 +170,29 @@ out:
 	return p;
 }
 
+static struct net_bridge_port *maybe_deliver_addr(
+	struct net_bridge_port *prev, struct net_bridge_port *p,
+	struct sk_buff *skb, const unsigned char *addr,
+	void (*__packet_hook)(const struct net_bridge_port *p,
+			      struct sk_buff *skb))
+{
+	struct net_device *dev = BR_INPUT_SKB_CB(skb)->brdev;
+
+	if (!should_deliver(p, skb))
+		return prev;
+
+	skb = skb_copy(skb, GFP_ATOMIC);
+	if (!skb) {
+		dev->stats.tx_dropped++;
+		return prev;
+	}
+
+	memcpy(eth_hdr(skb)->h_dest, addr, ETH_ALEN);
+	__packet_hook(p, skb);
+
+	return prev;
+}
+
 /* called under bridge lock */
 static void br_flood(struct net_bridge *br, struct sk_buff *skb,
 		     struct sk_buff *skb0,
@@ -232,6 +255,7 @@ static void br_multicast_flood(struct ne
 	struct net_bridge_port *prev = NULL;
 	struct net_bridge_port_group *p;
 	struct hlist_node *rp;
+	const unsigned char *addr;
 
 	rp = rcu_dereference(hlist_first_rcu(&br->router_list));
 	p = mdst ? rcu_dereference(mdst->ports) : NULL;
@@ -242,10 +266,19 @@ static void br_multicast_flood(struct ne
 		rport = rp ? hlist_entry(rp, struct net_bridge_port, rlist) :
 			     NULL;
 
-		port = (unsigned long)lport > (unsigned long)rport ?
-		       lport : rport;
-
-		prev = maybe_deliver(prev, port, skb, __packet_hook);
+		if ((unsigned long)lport > (unsigned long)rport) {
+			port = lport;
+			addr = p->unicast ? p->eth_addr : NULL;
+		} else {
+			port = rport;
+			addr = NULL;
+		}
+
+		if (addr)
+			prev = maybe_deliver_addr(prev, port, skb, addr,
+						  __packet_hook);
+		else
+			prev = maybe_deliver(prev, port, skb, __packet_hook);
 		if (IS_ERR(prev))
 			goto out;
 
--- a/net/bridge/br_sysfs_if.c
+++ b/net/bridge/br_sysfs_if.c
@@ -190,6 +190,7 @@ static BRPORT_ATTR(multicast_router, S_I
 		   store_multicast_router);
 
 BRPORT_ATTR_FLAG(multicast_fast_leave, BR_MULTICAST_FAST_LEAVE);
+BRPORT_ATTR_FLAG(multicast_to_unicast, BR_MULTICAST_TO_UCAST);
 #endif
 
 static const struct brport_attribute *brport_attrs[] = {
@@ -214,6 +215,7 @@ static const struct brport_attribute *br
 #ifdef CONFIG_BRIDGE_IGMP_SNOOPING
 	&brport_attr_multicast_router,
 	&brport_attr_multicast_fast_leave,
+	&brport_attr_multicast_to_unicast,
 #endif
 	&brport_attr_isolate_mode,
 	NULL
