From 10f3c772363e549c3dbd3cc3755d270c5656d5b8 Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Sat, 22 Feb 2014 16:53:30 +0100
Subject: [PATCH 109/182] libahci: Allow drivers to override start_engine

Allwinner A10 and A20 ARM SoCs have an AHCI sata controller which needs a
special register to be poked before starting the DMA engine.

This register gets reset on an ahci_stop_engine call, so there is no other
place then ahci_start_engine where this poking can be done.

This commit allows drivers to override ahci_start_engine behavior for use by
the Allwinner AHCI driver (and potentially other drivers in the future).

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
Signed-off-by: Tejun Heo <tj@kernel.org>
---
 drivers/ata/ahci.c          |    6 ++++--
 drivers/ata/ahci.h          |    6 ++++++
 drivers/ata/libahci.c       |   26 +++++++++++++++++++-------
 drivers/ata/sata_highbank.c |    3 ++-
 4 files changed, 31 insertions(+), 10 deletions(-)

--- a/drivers/ata/ahci.c
+++ b/drivers/ata/ahci.c
@@ -606,6 +606,7 @@ static int ahci_vt8251_hardreset(struct
 				 unsigned long deadline)
 {
 	struct ata_port *ap = link->ap;
+	struct ahci_host_priv *hpriv = ap->host->private_data;
 	bool online;
 	int rc;
 
@@ -616,7 +617,7 @@ static int ahci_vt8251_hardreset(struct
 	rc = sata_link_hardreset(link, sata_ehc_deb_timing(&link->eh_context),
 				 deadline, &online, NULL);
 
-	ahci_start_engine(ap);
+	hpriv->start_engine(ap);
 
 	DPRINTK("EXIT, rc=%d, class=%u\n", rc, *class);
 
@@ -631,6 +632,7 @@ static int ahci_p5wdh_hardreset(struct a
 {
 	struct ata_port *ap = link->ap;
 	struct ahci_port_priv *pp = ap->private_data;
+	struct ahci_host_priv *hpriv = ap->host->private_data;
 	u8 *d2h_fis = pp->rx_fis + RX_FIS_D2H_REG;
 	struct ata_taskfile tf;
 	bool online;
@@ -646,7 +648,7 @@ static int ahci_p5wdh_hardreset(struct a
 	rc = sata_link_hardreset(link, sata_ehc_deb_timing(&link->eh_context),
 				 deadline, &online, NULL);
 
-	ahci_start_engine(ap);
+	hpriv->start_engine(ap);
 
 	/* The pseudo configuration device on SIMG4726 attached to
 	 * ASUS P5W-DH Deluxe doesn't send signature FIS after
--- a/drivers/ata/ahci.h
+++ b/drivers/ata/ahci.h
@@ -324,6 +324,12 @@ struct ahci_host_priv {
 	u32			em_msg_type;	/* EM message type */
 	struct clk		*clk;		/* Only for platforms supporting clk */
 	void			*plat_data;	/* Other platform data */
+	/*
+	 * Optional ahci_start_engine override, if not set this gets set to the
+	 * default ahci_start_engine during ahci_save_initial_config, this can
+	 * be overridden anytime before the host is activated.
+	 */
+	void			(*start_engine)(struct ata_port *ap);
 };
 
 extern int ahci_ignore_sss;
--- a/drivers/ata/libahci.c
+++ b/drivers/ata/libahci.c
@@ -394,6 +394,9 @@ static ssize_t ahci_show_em_supported(st
  *
  *	If inconsistent, config values are fixed up by this function.
  *
+ *	If it is not set already this function sets hpriv->start_engine to
+ *	ahci_start_engine.
+ *
  *	LOCKING:
  *	None.
  */
@@ -500,6 +503,9 @@ void ahci_save_initial_config(struct dev
 	hpriv->cap = cap;
 	hpriv->cap2 = cap2;
 	hpriv->port_map = port_map;
+
+	if (!hpriv->start_engine)
+		hpriv->start_engine = ahci_start_engine;
 }
 EXPORT_SYMBOL_GPL(ahci_save_initial_config);
 
@@ -766,7 +772,7 @@ static void ahci_start_port(struct ata_p
 
 	/* enable DMA */
 	if (!(hpriv->flags & AHCI_HFLAG_DELAY_ENGINE))
-		ahci_start_engine(ap);
+		hpriv->start_engine(ap);
 
 	/* turn on LEDs */
 	if (ap->flags & ATA_FLAG_EM) {
@@ -1234,7 +1240,7 @@ int ahci_kick_engine(struct ata_port *ap
 
 	/* restart engine */
  out_restart:
-	ahci_start_engine(ap);
+	hpriv->start_engine(ap);
 	return rc;
 }
 EXPORT_SYMBOL_GPL(ahci_kick_engine);
@@ -1426,6 +1432,7 @@ static int ahci_hardreset(struct ata_lin
 	const unsigned long *timing = sata_ehc_deb_timing(&link->eh_context);
 	struct ata_port *ap = link->ap;
 	struct ahci_port_priv *pp = ap->private_data;
+	struct ahci_host_priv *hpriv = ap->host->private_data;
 	u8 *d2h_fis = pp->rx_fis + RX_FIS_D2H_REG;
 	struct ata_taskfile tf;
 	bool online;
@@ -1443,7 +1450,7 @@ static int ahci_hardreset(struct ata_lin
 	rc = sata_link_hardreset(link, timing, deadline, &online,
 				 ahci_check_ready);
 
-	ahci_start_engine(ap);
+	hpriv->start_engine(ap);
 
 	if (online)
 		*class = ahci_dev_classify(ap);
@@ -2007,10 +2014,12 @@ static void ahci_thaw(struct ata_port *a
 
 void ahci_error_handler(struct ata_port *ap)
 {
+	struct ahci_host_priv *hpriv = ap->host->private_data;
+
 	if (!(ap->pflags & ATA_PFLAG_FROZEN)) {
 		/* restart engine */
 		ahci_stop_engine(ap);
-		ahci_start_engine(ap);
+		hpriv->start_engine(ap);
 	}
 
 	sata_pmp_error_handler(ap);
@@ -2031,6 +2040,7 @@ static void ahci_post_internal_cmd(struc
 
 static void ahci_set_aggressive_devslp(struct ata_port *ap, bool sleep)
 {
+	struct ahci_host_priv *hpriv = ap->host->private_data;
 	void __iomem *port_mmio = ahci_port_base(ap);
 	struct ata_device *dev = ap->link.device;
 	u32 devslp, dm, dito, mdat, deto;
@@ -2094,7 +2104,7 @@ static void ahci_set_aggressive_devslp(s
 		   PORT_DEVSLP_ADSE);
 	writel(devslp, port_mmio + PORT_DEVSLP);
 
-	ahci_start_engine(ap);
+	hpriv->start_engine(ap);
 
 	/* enable device sleep feature for the drive */
 	err_mask = ata_dev_set_feature(dev,
@@ -2106,6 +2116,7 @@ static void ahci_set_aggressive_devslp(s
 
 static void ahci_enable_fbs(struct ata_port *ap)
 {
+	struct ahci_host_priv *hpriv = ap->host->private_data;
 	struct ahci_port_priv *pp = ap->private_data;
 	void __iomem *port_mmio = ahci_port_base(ap);
 	u32 fbs;
@@ -2134,11 +2145,12 @@ static void ahci_enable_fbs(struct ata_p
 	} else
 		dev_err(ap->host->dev, "Failed to enable FBS\n");
 
-	ahci_start_engine(ap);
+	hpriv->start_engine(ap);
 }
 
 static void ahci_disable_fbs(struct ata_port *ap)
 {
+	struct ahci_host_priv *hpriv = ap->host->private_data;
 	struct ahci_port_priv *pp = ap->private_data;
 	void __iomem *port_mmio = ahci_port_base(ap);
 	u32 fbs;
@@ -2166,7 +2178,7 @@ static void ahci_disable_fbs(struct ata_
 		pp->fbs_enabled = false;
 	}
 
-	ahci_start_engine(ap);
+	hpriv->start_engine(ap);
 }
 
 static void ahci_pmp_attach(struct ata_port *ap)
--- a/drivers/ata/sata_highbank.c
+++ b/drivers/ata/sata_highbank.c
@@ -403,6 +403,7 @@ static int ahci_highbank_hardreset(struc
 	static const unsigned long timing[] = { 5, 100, 500};
 	struct ata_port *ap = link->ap;
 	struct ahci_port_priv *pp = ap->private_data;
+	struct ahci_host_priv *hpriv = ap->host->private_data;
 	u8 *d2h_fis = pp->rx_fis + RX_FIS_D2H_REG;
 	struct ata_taskfile tf;
 	bool online;
@@ -431,7 +432,7 @@ static int ahci_highbank_hardreset(struc
 			break;
 	} while (!online && retry--);
 
-	ahci_start_engine(ap);
+	hpriv->start_engine(ap);
 
 	if (online)
 		*class = ahci_dev_classify(ap);
