--- a/boards.cfg
+++ b/boards.cfg
@@ -198,6 +198,7 @@ Active  arm         arm926ejs      kirkw
 Active  arm         arm926ejs      kirkwood    Marvell         openrd              openrd_client                        openrd:BOARD_IS_OPENRD_CLIENT                                                                                                     -
 Active  arm         arm926ejs      kirkwood    Marvell         openrd              openrd_ultimate                      openrd:BOARD_IS_OPENRD_ULTIMATE                                                                                                   -
 Active  arm         arm926ejs      kirkwood    raidsonic       ib62x0              ib62x0                               -                                                                                                                                 Luka Perkov <luka@openwrt.org>
+Active  arm         arm926ejs      kirkwood    raidsonic       ib62x0              ib62x0_second_stage                  ib62x0:SECOND_STAGE                                                                                                               Luka Perkov <luka@openwrt.org>
 Active  arm         arm926ejs      kirkwood    Seagate         -                   dockstar                             -                                                                                                                                 Eric Cooper <ecc@cmu.edu>
 Active  arm         arm926ejs      kirkwood    Seagate         dockstar            dockstar_second_stage                dockstar:SECOND_STAGE                                                                                                             Luka Perkov <luka@openwrt.org>
 Active  arm         arm926ejs      kirkwood    Seagate         -                   goflexhome                           -                                                                                                                                 Suriyan Ramasami <suriyan.r@gmail.com>
--- a/include/configs/ib62x0.h
+++ b/include/configs/ib62x0.h
@@ -91,7 +91,8 @@
 	"mtdparts=orion_nand:"						\
 	"0xe0000@0x0(uboot),"						\
 	"0x20000@0xe0000(uboot_env),"					\
-	"-@0x100000(root)\0"
+	"0x100000@0x100000(second_stage_uboot),"			\
+	"-@0x200000(root)\0"
 
 #define CONFIG_EXTRA_ENV_SETTINGS \
 	"console=console=ttyS0,115200\0"				\
@@ -99,7 +100,7 @@
 	"mtdparts="CONFIG_MTDPARTS					\
 	"kernel=/boot/zImage\0"						\
 	"fdt=/boot/ib62x0.dtb\0"					\
-	"bootargs_root=ubi.mtd=2 root=ubi0:rootfs rootfstype=ubifs rw\0"
+	"bootargs_root=ubi.mtd=3 root=ubi0:rootfs rootfstype=ubifs rw\0"
 
 /*
  * Ethernet driver configuration
