From 33f352709fedc760be85adde5b834043a650f585 Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Fri, 20 Sep 2013 19:07:56 +0100
Subject: [PATCH 094/196] dwc_otg: Fix for occasional lockup on boot when doing
 a USB reset

---
 drivers/usb/host/dwc_otg/dwc_otg_hcd_intr.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/drivers/usb/host/dwc_otg/dwc_otg_hcd_intr.c b/drivers/usb/host/dwc_otg/dwc_otg_hcd_intr.c
index 509b629..57092d2 100644
--- a/drivers/usb/host/dwc_otg/dwc_otg_hcd_intr.c
+++ b/drivers/usb/host/dwc_otg/dwc_otg_hcd_intr.c
@@ -742,8 +742,8 @@ int32_t dwc_otg_hcd_handle_sof_intr(dwc_otg_hcd_t * hcd)
 	}
 
 	/* Clear interrupt */
-	//gintsts.b.sofintr = 1;
-	//DWC_WRITE_REG32(&hcd->core_if->core_global_regs->gintsts, gintsts.d32);
+	gintsts.b.sofintr = 1;
+	DWC_WRITE_REG32(&hcd->core_if->core_global_regs->gintsts, gintsts.d32);
 
 	return 1;
 }
-- 
1.9.1

