From 8605197c200786888415bf2e30d1fbde6ba8ba03 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Uwe=20Kleine-K=C3=B6nig?= <u.kleine-koenig@pengutronix.de>
Date: Tue, 1 Apr 2014 22:25:59 +0200
Subject: [PATCH 039/182] pinctrl: msm8x74: make Kconfig dependency more
 strict
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This driver is only useful on MSM8x74, so let the driver depend on
ARCH_QCOM but allow compile coverage testing.
The main benefit is that the driver isn't available to be selected for
machines that don't have the matching hardware.

Signed-off-by: Uwe Kleine-KÃ¶nig <u.kleine-koenig@pengutronix.de>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
---
 drivers/pinctrl/Kconfig |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/pinctrl/Kconfig
+++ b/drivers/pinctrl/Kconfig
@@ -232,7 +232,7 @@ config PINCTRL_APQ8064
 
 config PINCTRL_MSM8X74
 	tristate "Qualcomm 8x74 pin controller driver"
-	depends on GPIOLIB && OF
+	depends on GPIOLIB && OF && (ARCH_QCOM || COMPILE_TEST)
 	select PINCTRL_MSM
 	help
 	  This is the pinctrl, pinmux, pinconf and gpiolib driver for the
