From 36268d704307282109ec246f65cac2a42c825629 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Emilio=20L=C3=B3pez?= <emilio@elopez.com.ar>
Date: Fri, 20 Sep 2013 20:29:17 -0300
Subject: [PATCH] clk: sunxi: Implement MMC phase control
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

HdG: add header exporting clk_sunxi_mmc_phase_control

Signed-off-by: Emilio López <emilio@elopez.com.ar>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 drivers/clk/sunxi/clk-sunxi.c | 35 +++++++++++++++++++++++++++++++++++
 include/linux/clk/sunxi.h     | 22 ++++++++++++++++++++++
 2 files changed, 57 insertions(+)
 create mode 100644 include/linux/clk/sunxi.h

--- a/drivers/clk/sunxi/clk-sunxi.c
+++ b/drivers/clk/sunxi/clk-sunxi.c
@@ -507,6 +507,41 @@ CLK_OF_DECLARE(sun7i_a20_gmac, "allwinne
 
 
 /**
+ * clk_sunxi_mmc_phase_control() - configures MMC clock phase control
+ */
+
+void clk_sunxi_mmc_phase_control(struct clk_hw *hw, u8 sample, u8 output)
+{
+	#define to_clk_composite(_hw) container_of(_hw, struct clk_composite, hw)
+	#define to_clk_factors(_hw) container_of(_hw, struct clk_factors, hw)
+
+	struct clk_composite *composite = to_clk_composite(hw);
+	struct clk_hw *rate_hw = composite->rate_hw;
+	struct clk_factors *factors = to_clk_factors(rate_hw);
+	unsigned long flags = 0;
+	u32 reg;
+
+	if (factors->lock)
+		spin_lock_irqsave(factors->lock, flags);
+
+	reg = readl(factors->reg);
+
+	/* set sample clock phase control */
+	reg &= ~(0x7 << 20);
+	reg |= ((sample & 0x7) << 20);
+
+	/* set output clock phase control */
+	reg &= ~(0x7 << 8);
+	reg |= ((output & 0x7) << 8);
+
+	writel(reg, factors->reg);
+
+	if (factors->lock)
+		spin_unlock_irqrestore(factors->lock, flags);
+}
+
+
+/**
  * sunxi_factors_clk_setup() - Setup function for factor clocks
  */
 
--- /dev/null
+++ b/include/linux/clk/sunxi.h
@@ -0,0 +1,22 @@
+/*
+ * Copyright 2013 - Hans de Goede <hdegoede@redhat.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ */
+
+#ifndef __LINUX_CLK_SUNXI_H_
+#define __LINUX_CLK_SUNXI_H_
+
+#include <linux/clk.h>
+
+void clk_sunxi_mmc_phase_control(struct clk_hw *hw, u8 sample, u8 output);
+
+#endif
