From 082a49f0490008b999db80e3ccf1521c7dd21cec Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Mon, 2 Dec 2013 12:32:44 +0100
Subject: [PATCH 1/8] MIPS: BCM63XX: remove !RUNTIME_DETECT code from register
 sets

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h | 33 ------------------------
 1 file changed, 33 deletions(-)

--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h
@@ -598,10 +598,6 @@ enum bcm63xx_regs_set {
 
 extern const unsigned long *bcm63xx_regs_base;
 
-#define __GEN_RSET_BASE(__cpu, __rset)					\
-	case RSET_## __rset :						\
-		return BCM_## __cpu ##_## __rset ##_BASE;
-
 #define __GEN_RSET(__cpu)						\
 	switch (set) {							\
 	__GEN_RSET_BASE(__cpu, DSL_LMEM)				\
@@ -693,36 +689,7 @@ extern const unsigned long *bcm63xx_regs
 
 static inline unsigned long bcm63xx_regset_address(enum bcm63xx_regs_set set)
 {
-#ifdef BCMCPU_RUNTIME_DETECT
 	return bcm63xx_regs_base[set];
-#else
-#ifdef CONFIG_BCM63XX_CPU_3368
-	__GEN_RSET(3368)
-#endif
-#ifdef CONFIG_BCM63XX_CPU_6328
-	__GEN_RSET(6328)
-#endif
-#ifdef CONFIG_BCM63XX_CPU_6338
-	__GEN_RSET(6338)
-#endif
-#ifdef CONFIG_BCM63XX_CPU_6345
-	__GEN_RSET(6345)
-#endif
-#ifdef CONFIG_BCM63XX_CPU_6348
-	__GEN_RSET(6348)
-#endif
-#ifdef CONFIG_BCM63XX_CPU_6358
-	__GEN_RSET(6358)
-#endif
-#ifdef CONFIG_BCM63XX_CPU_6362
-	__GEN_RSET(6362)
-#endif
-#ifdef CONFIG_BCM63XX_CPU_6368
-	__GEN_RSET(6368)
-#endif
-#endif
-	/* unreached */
-	return 0;
 }
 
 /*
